Create Self-Signed Certificate

Overview
  This print server issues its own certificate and secret key.
  Using this certificate, you can easily use SSL/TLS communication without needing a CA (Certificate Authority).
Common Name
  Input common name for certificate(Required).
  The length of common name is less than 64 bytes.
  Enter an identifier such as an IP address, host name or domain name to use when accessing to this printer through SSL/TLS communication.
  The host name is displayed by default.
Valid Date
  Input the date of validity.
Public Key Algorithm
  Select Public key length.
  It is recommended that you select the default setting because it provides the strongest level of security. The other security settings are only recommended when the device does not support the strongest level of security.
  RSA(2048bit) : RSA 2048 bit key kength (default)
  RSA(1024bit) : RSA 1024 bit key length
Digest Algorithm
  Select Digest Algorithm for signature.
  It is recommended that you select the default setting because it provides the strongest level of security. The other security settings are only recommended when the device does not support the strongest level of security.
  SHA256 : SHA256 Digest Algorithm (default)
  SHA1 : SHA1 Digest Algorithm