Ethernet

Overview
  This page allows you to control the ethernet link mode. Auto allows the print server automatically to select the link mode. If the connection fails by Auto, please try a static configuration and select the static 100BaseTX or 10BaseT link mode.
  NOTE : if you set an incorrect static link mode, you might not be able to communicate with your print server.
Jumbo Frame (only for supported models)
  Jumbo Frame technology makes the communication speed faster by sending larger packets of data. Jumbo Frame technology can only be used in 1000BaseT mode.
  Jumbo Frame technology requires all peripherals such as PCs (LAN/Network adapters), hubs, switches and routers on your network support Jumbo Frame technology. If there are any devices on your LAN/Network that do not support Jumbo Frame technology then network communication may fail.