# SetTableData procedure

Retrieves scan results from the router processor.

## Syntax

Delphi
C++

    procedure SetTableData(
      Row: DWORD;
      Name,
      Value: PChar
    ); stdcall;

    VOID CALLBACK SetTableData(
      _In_  DWORD Row,
      _In_  LPCTSTR Name,
      _In_  LPCTSTR Value
    );

## Parameters

Row [in]

  Table row number, which was specified by PrepareRouter function.

Name [in]

  Table column internal name.

  Value | Meaning
  --- | ---
  stcStatus "Status" | Describes the current processing status.
  stcAuth "Auth" | Contains information about authorization on device.
  stcType "Type" | Contains information about device type.
  stcRadioOff "RadioOff" | Contains information about device wireless state. Possible values are: "[X]" - radio is turned off. "-" - device doesn't have wireless interface.
  stcHidden "Hidden" | Contains information about SSID broadcast state. Possible values are: "[X]" - SSID broadcast is disabled, Access Point is hidden. "-" - device doesn't have wireless interface.
  stcBSSID "BSSID" | Contains Access Point BSSID (MAC address). Also may contain string <no wireless>, which means that device doesn't have wireless interface.
  stcSSID "SSID" | Contains Access Point ESSID (network name).
  stcSec "Sec" | Contains Access Point security mode (encryption or authentication type).
  stcKey "Key" | Contains Access Point password key.
  stcPin "WPS" | Contains Access Point WPS pin code.
  stcLANIP "LANIP" | Contains Local Area Network IPv4 Address of a device. Also may contain string <bridge>, which means that LAN interface running in bridged mode or doesn't exist.
  stcLANMask "LANMask" | Contains Local Area Network IPv4 Subnet Mask of a device. Also may contain string <bridge>, which means that LAN interface running in bridged mode or doesn't exist.
  stcWANIP "WANIP" | Contains Wide Area Network IPv4 Address of a device.
  stcWANMask "WANMask" | Contains Wide Area Network IPv4 Subnet Mask of a device.
  stcWANGate "WANGate" | Contains Wide Area Network IPv4 Default Gateway of a device.
  stcDNS "DNS" | Contains IPv4 Domain Name Servers of a device, separated by space character.

Value [in]

  Table cell value set by router processor.