READ THIS FIRST!

IF YOU ARE UPGRADING CODE ON A B2360d, PLEASE READ AND FOLLOW THE INSTRUCTIONS BELOW:

For B2360d only:    
-  When updating from EC5 or older firmware to EC6 or newer firmware, use an intermediate release, LW50.PR.P593.pir2Lgr.FDN.PIR.E618.pirXXgre.fls, included in the zip package along with these release notes. 
-  If your device firmware is EC5 or older, update your device firmware first to LW50.PRL.P593. After your device reboots, you can proceed to update firmware to EC6.0 or newer firmware. 
-  This intermediate update is necessary due to increased code size of EC6.0 or newer and memory usage during code updates.  If you attempt to load EC6.0 or newer code over EC5 or older code other than LW50.PR.P593, it can take up to or more than 90 minutes to update or it may even fail completely due to an out of memory condition.  

For B2360d and B2360dn:
Downgrading to EC4.0 or EC4.05: 
-  Due to changes in EC4.0 and EC5, do NOT downgrade firmware from EC5 or newer directly to EC4.0 or EC4.05 based code.  EC4.0 and EC4.05 code levels have names like LW40.xx.P4xx.  This will cause a non-clearable 900 Service error. You will need to contact the TSC for instructions on how to clear this error. 
-  This warning includes installing a DLE with EC4.0 or EC4.05 code into a device that currently has EC5 or newer code. 
-  Code levels earlier than EC4.0 can be sent to EC5 level devices without causing a service error. 
-  To downgrade EC5 or newer code to an EC4.0 or EC4.05 level, you must first load an EC4.1 based code.  EC4.1 code levels have names like LW41.XX.P4xx. 
Once the device is at an EC4.1 level, EC4.0 code can be sent.  
-  We do not officially support downgrading firmware.  This is the reason we do not support it, even though we go to great efforts to prevent these kinds of events from happening, sometimes it is unavoidable.  We apologize for the inconvenience.



CUSTOMER RELEASE NOTES
Base firmware EC7.0, LW70.xx.P022, for the following devices (changes since EC6.3, LW63.xx.P638) 

B2360d (Bridge Upgrade Firmware):	LLW50.PR.P593.pir2Lgr.FDN.PIR.E618.pirXXgre.fls
B2360d, B2360dn:			LW70.PRL.P022.FDN.PIR.E704.fls


New features:
-  Added SMBv3 support.   
-  Enhanced TLS 1.2 support.  Can now disable TLS 1.0 and TLS1.1 
-  Added new "SSL Cipher List" setting 
-  Updated openSSL to version 1.0.2j 
-  Added support for PKCS #12 security certificates standard 


Security Issues Addressed:
-  Addressed KRACK which has the following CVEs associated with it: 
-  CVE-2017-13077 
-  CVE-2017-13078 
-  CVE-2017-13079 
-  CVE-2017-13080 
-  CVE-2017-13081 
-  CVE-2017-13082 
-  CVE-2017-13084 
-  CVE-2017-13086 
-  CVE-2017-13087 
-  CVE-2017-13088 


Field Issues Addressed and Other Improvements: 
-  Update jar signing algorithm for Remote Operator Panel and Scan Profile java applets 
-  Fix for an issue where pressing the sleep button does not always put the device to sleep even when the setting is configured to do so 
-  Fixes for several 900.xx crashes 
-  Multiple fixes for blank screen, white screen, and busy screen hangs 
-  Multiple translation changes 
-  Multiple card reader fixes 
-  Multiple fixes for PDF, PS, and PCL print job errors 

