Using Wired Connectivity
------------------------
1) Go to the EWS page of the printer.
2) Go to the Settings link.
3) In the Settings Link,Browse to the Engine.fls file & click on submit.
4) After printer is at the ready mode,Browse to the RIP.fls file & click on submit.

Wait for printer to get back to ready mode.
During flashing,do not power off,pull out power cord or restart the printer.


Using USB Connectivity
-----------------------

1) Launch the FDU Utility that comes with the package.Choose the right version depending on your
operating systems.

2) Follow the instructions on your screen.

3) Wait for printer to get back to ready mode.
During flashing,do not power off,pull out power cord or restart the printer.