Home > Specifications > General Specifications

### General Specifications

Printer Type | Laser
Print Method | Electrophotographic Laser Printer
Memory Capacity | Standard | (DocuPrint P225 db) 8 MB
(DocuPrint P225 d/DocuPrint P265 dw) 32 MB
LCD (liquid crystal display) | (DocuPrint P225 d/DocuPrint P265 dw) 16 characters × 1 line
Power Source | (For Taiwan) 110 - 120 V AC 50/60 Hz (Except Taiwan) 220 - 240 V AC 50/60 Hz
Power Consumption (Average) | Peak *1 | Approximately 1080 W
Printing *1 | (DocuPrint P225 db/DocuPrint P225 d) Approximately 455 W at 25 °C
(DocuPrint P265 dw) (Except Taiwan) Approximately 537 W at 25 °C (For Taiwan) Approximately 546 W at 25 °C
Ready *1 | Approximately 58 W at 25 °C
Sleep *1 | (Except Taiwan) Approximately 5.4 W (For Taiwan) Approximately 3.9 W
Deep Sleep *1 | (DocuPrint P225 db) Approximately 0.4 W
(DocuPrint P225 d/DocuPrint P265 dw) (Except Taiwan) Approximately 0.5 W (For Taiwan) Approximately 0.8 W
Power Off *1 *2 *3 | (Except Taiwan) Approximately 0.06 W (For Taiwan) Approximately 0.02 W
Dimensions |
Weights (with supplies) | 6.8 kg

Noise Level | Sound Pressure | Printing | (DocuPrint P225 db/DocuPrint P225 d) LpAm = 50 dB (A)
(DocuPrint P265 dw) LpAm = 51 dB (A)
Ready | LpAm = 30 dB (A)
Sound Power | Printing *4 | (DocuPrint P225 db/DocuPrint P225 d) LWAd = 6.40 B (A)
(DocuPrint P265 dw) LWAd = 6.60 B (A)
Ready *4 | LWAd = 4.60 B (A)
Temperature | Operating | 10 to 32 °C
Storage | 0 to 40 °C
Humidity | Operating | 20 to 80% (without condensation)
Storage | 35 to 85% (without condensation)

*1
Measured when the machine is connected to the USB interface.
*2
Measured according to IEC 62301 Edition 2.0.
*3
Power consumption varies slightly depending on the usage environment.
*4
Measured in accordance with the method described in RAL-UZ171.

Related Information
  - Specifications
  - Settings Table
  - WLAN Enable (Wireless Network Only)

Go to top of page