Home > Network > Additional Methods of Configuring Your Fuji Xerox Machine for a Wireless Network > Configure Your Machine for a Wireless Network Using the PIN Method of Wi-Fi Protected Setup™ (WPS) > Two Wireless Network Connection Types Using the PIN Method of Wi-Fi Protected Setup™ (WPS)

### Two Wireless Network Connection Types Using the PIN Method of Wi-Fi Protected Setup™ (WPS)

Related Models:DocuPrint P265 dw

Type A
  Connection when the wireless LAN access point/router (1) doubles as Registrar.

Type B
  Connection when another device (2), such as a computer, is used as Registrar.

Routers or access points that support WPS are marked with this symbol:

Related Information
  - Configure Your Machine for a Wireless Network Using the PIN Method of Wi-Fi Protected Setup™ (WPS)

Go to top of page