Home > Network > Additional Methods of Configuring Your Fuji Xerox Machine for a Wireless Network > Configure Your Machine for a Wireless Network Using the PIN Method of Wi-Fi Protected Setup™ (WPS)

### Configure Your Machine for a Wireless Network Using the PIN Method of Wi-Fi Protected Setup™ (WPS)

Related Models:DocuPrint P265 dw
If your wireless LAN access point/router supports WPS, you can use the Personal Identification Number (PIN) Method to configure your wireless network settings.

The PIN Method is one of the connection methods developed by the Wi-Fi Alliance®. By submitting a PIN created by an Enrollee (your machine) to the Registrar (a device that manages the wireless LAN), you can set up the wireless network and security settings. For more information on how to access WPS mode, see the instructions provided with your wireless access point/router.

Related Information
  - Additional Methods of Configuring Your Fuji Xerox Machine for a Wireless Network
  - Two Wireless Network Connection Types Using the PIN Method of Wi-Fi Protected Setup™ (WPS)
  - How to Configure Your Wireless Network Using the PIN Method of Wi-Fi Protected Setup™ (WPS)
  - Connected to a Computer with a Wireless LAN Access Point Router in the Network (Infrastructure Mode)
  - Install Drivers Used for Printing for Infrastructure Mode When Using Vertical Pairing (Windows® 7 and Windows® 8)

Go to top of page