Home > Network > Locate the Machine's Network Settings > Locate Network Settings When Using BRAdmin Light (Windows® and Macintosh)

### Locate Network Settings When Using BRAdmin Light (Windows® and Macintosh)

Related Models:DocuPrint P225 d / DocuPrint P265 dw

- Go to the download page for your model on the Fuji Xerox website at http://www.fujixeroxprinters.com to download the latest version of BRAdmin Light.
- If you are using Windows® Firewall, or the firewall function of an anti-spyware or antivirus application, temporarily disable them. When you are sure you can print, configure the software settings following the instructions.
- Node name: The node name appears in the current BRAdmin Light window. The default node name is "BRNxxxxxxxxxxxx" for a wired network or "BRWxxxxxxxxxxxx" for a wireless network (where "xxxxxxxxxxxx" is your machine's MAC Address / Ethernet address).
- No password is required by default. Type a password if you have set one.

1. Install BRAdmin Light.
2. Start BRAdmin Light.
   - (Windows Vista®, Windows® 7, Windows Server® 2003 and Windows Server® 2008)

     Click (Start)>All Programs>Fuji Xerox>BRAdmin Light>BRAdmin Light.

   - (Windows® 8, Windows Server® 2012 and Windows Server® 2012 R2)

     Click (BRAdmin Light).

   - (Macintosh)

     Go to the download page for your model on the Fuji Xerox website at http://www.fujixeroxprinters.com to download the latest version of BRAdmin Light.

     Select the folder you have downloaded, and then double-click the BRAdmin Light.jar icon.

   BRAdmin Light will search for devices automatically.
3. Double-click on the print server whose settings you want to change.
   - If the print server is set to its factory default settings (if you do not use a DHCP/BOOTP/RARP server), the device will appear as Unconfigured in BRAdmin Light. Double-click the unconfigured device.
   - You can find the Node Name and MAC Address (Ethernet Address) by printing the Network Configuration Report. You can also find the MAC Address using the Fuji Xerox machine's control panel.
4. Type a password if you have set one, and then click OK.

You can now change the network settings.

Related Information
  - Locate the Machine's Network Settings
  - Where Can I Find My Fuji Xerox Machine's Network Settings?
  - Install BRAdmin Light for Windows®
  - Print the Network Configuration Report
  - Reset the Network Settings to the Factory Settings

Go to top of page