Home > Network > Additional Methods of Configuring Your Fuji Xerox Machine for a Wireless Network > Configure Your Machine for a Wireless Network Using the One Push Method of Wi-Fi Protected Setup™ (WPS) or AOSS™ > How to Configure Your Wireless Network Using the One Push Method of WPS or AOSS™

### How to Configure Your Wireless Network Using the One Push Method of WPS or AOSS™

Related Models:DocuPrint P265 dw

1. Press or to select the Network option, and then press OK.
2. Press or to select the WLAN option, and then press OK.
3. Press or to select the WPS/AOSS option, and then press OK.
4. When WLAN Enable? appears, press to select On.
   This will start the wireless setup wizard. To cancel, press Back.
5. When the LCD displays Press Key on rtr, press the WPS or AOSS™ button on your wireless access point/router. Press on the machine's control panel and your machine will automatically detect which mode (WPS or AOSS™) your wireless access point/router uses and try to connect to your wireless network.

If your wireless device is connected successfully, the machine's LCD displays Connected. The machine will print your machine's wireless status report. If the connection fails, check the error code on the printed report.
If the connection fails, your machine reverts to a wired network interface.

For Windows®:

You have completed the wireless network setup. To install drivers and software necessary for operating your device, click Install Printer Driver on the Installer CD-ROM's Top Menu page.

For Macintosh:

You have completed the wireless network setup. Go to the download page for your model on the Fuji Xerox website at http://www.fujixeroxprinters.com to install drivers and software necessary for operating your device.

Related Information
  - Configure Your Machine for a Wireless Network Using the One Push Method of Wi-Fi Protected Setup™ (WPS) or AOSS™
  - Wireless LAN Report Error Codes

Go to top of page