Home > Network > Additional Methods of Configuring Your Fuji Xerox Machine for a Wireless Network > Use Wi-Fi Direct™ > Configure Your Wi-Fi Direct Network > Configure Your Wi-Fi Direct Network Using the PIN Method of Wi-Fi Protected Setup™ (WPS)

### Configure Your Wi-Fi Direct Network Using the PIN Method of Wi-Fi Protected Setup™ (WPS)

Related Models:DocuPrint P265 dw
If your mobile device supports the PIN Method of Wi-Fi Protected Setup™ (WPS), follow these steps to configure a Wi-Fi Direct network.

1. Press or to select the Network option, and then press OK.
2. Press or to select the Wi-Fi Direct option, and then press OK.
3. Press or to select the Group Owner option, and then press OK.
4. Press or to select the On option, and then press OK.
5. Press or to select the PIN Code option, and then press OK.
6. When Wi-Fi Direct On? appears, press to accept. To cancel, press .
7. Activate your mobile device's WPS PIN configuration method (see your mobile device's user's guide for instructions) when Activate Wi-Fi Direct on other device and press OK. appears on the machine's LCD. Press OK on your machine.
   This will start the Wi-Fi Direct setup. To cancel, press Back.
8. The machine will wait for a connection request from your mobile device. When Input PIN Code appears, enter the PIN displayed on your mobile device in the machine.
9. Press OK.
10. If your mobile device connects successfully, the machine's LCD displays Connected. You have completed the Wi-Fi Direct network setup.

Related Information
  - Configure Your Wi-Fi Direct Network
  - Step-by-step Guide for Wi-Fi Direct Network Configuration

Go to top of page