Home > Network > Additional Methods of Configuring Your Fuji Xerox Machine for a Wireless Network > Configure Your Machine for a Wireless Network in Ad-Hoc Mode (For IEEE 802.11b/g/n)

### Configure Your Machine for a Wireless Network in Ad-Hoc Mode (For IEEE 802.11b/g/n)

- Configure Your Machine for a Wireless Network in Ad-Hoc Mode Using a New SSID
  If you are using a new SSID, all other devices will connect using the SSID you assign to your Fuji Xerox machine in the following steps. You must connect to this SSID from your computer when it is configured for Ad-Hoc mode.
- Configure Your Machine for a Wireless Network in Ad-Hoc Mode Using an Existing SSID
  If you are trying to pair your Fuji Xerox machine to a computer that is already in Ad-Hoc mode and has a configured SSID, use these instructions.
- Connected to a Wireless Computer without a Wireless LAN Access Point Router in the Network (Ad-Hoc Mode)
  This type of network does not have a central wireless LAN access point/router. Each wireless client communicates directly with each other. When the Fuji Xerox wireless machine (your machine) is part of this network, it receives all print jobs directly from the computer sending print data.

Go to top of page