Home > Specifications > General Specifications

### General Specifications

Printer Type | Laser
Print Method | Electrophotographic Laser Printer
Memory Capacity | Standard | (DocuPrint P228 db/DocuPrint P268 b) 8 MB
(DocuPrint P268 d/DocuPrint P268 dw) 32 MB
LCD (liquid crystal display) | (DocuPrint P268 d/DocuPrint P268 dw) 16 characters × 1 line
Power Source | 220 - 240 V AC 50/60 Hz
Power Consumption (Average) | Peak *1 | Approximately 1080 W
Printing *1 | (DocuPrint P228 db) Approximately 455 W at 25 °C
(DocuPrint P268 b/DocuPrint P268 d/DocuPrint P268 dw) Approximately 537 W at 25 °C
Ready *1 | Approximately 58 W at 25 °C
Sleep *1 | Approximately 5.4 W
Deep Sleep *1
Approximately 0.5 W
Power Off *1 *2 *3 | Approximately 0.06 W
Dimensions |
Weights (with supplies) | DocuPrint P228 db/DocuPrint 268 d/DocuPrint 268 dw 6.8 kg DocuPrint P228 b 6.6 kg

Noise Level | Sound Pressure | Printing | (DocuPrint P228 db) LpAm = 50 dB (A)
(DocuPrint P268 b/DocuPrint P268 d/DocuPrint P268 dw) LpAm = 51 dB (A)
Ready | LpAm = 31dB (A)
Sound Power | Printing *4 | (DocuPrint P228 db) LWAd = 6.40 B (A) (DocuPrint P268 b/DocuPrint P268 d/DocuPrint P268 dw) LWAd = 6.60 B (A)
Ready *4 | LWAd = 4.60 B (A)
Temperature | Operating | 10 to 32.5 °C To ensure the high print quality, the maximum ambient temperature we recommend is 32.5 °C. The maximum ambient temperature to safely use this machine is 35 °C.
Storage | 0 to 40 °C
Humidity | Operating | 20 to 80% (without condensation)
Storage | 10 to 90% (without condensation)

*1
Measured when the machine is connected to the USB interface.
*2
Measured according to IEC 62301 Edition 2.0.
*3
Power consumption varies slightly depending on the usage environment.
*4
Measured in accordance with the method described in RAL-UZ171.

Related Information
  - Specifications
  - Settings Table
  - WLAN Enable (Wireless Network Only)

Go to top of page