Home > Network > Additional Methods of Configuring Your Fuji Xerox Machine for a Wireless Network > Use Wi-Fi Direct™ > Configure Your Wi-Fi Direct Network > Configure Your Wi-Fi Direct Network Manually

### Configure Your Wi-Fi Direct Network Manually

Related Models:DocuPrint P268 dw
If your mobile device does not support Wi-Fi Direct or WPS, you must configure a Wi-Fi Direct network manually.

1. Press or to select the Network option, and then press OK.
2. Press or to select the Wi-Fi Direct option, and then press OK.
3. Press or to select the Manual option, and then press OK.
4. When Wi-Fi Direct On? appears, press to accept. To cancel, press .
5. The machine will display the SSID name and Password for two minutes. Go to your mobile device's wireless network settings screen and enter the SSID name and password.
6. If your mobile device connects successfully, the machine's LCD displays Connected. You have completed the Wi-Fi Direct network setup.

Related Information
  - Configure Your Wi-Fi Direct Network
  - Step-by-step Guide for Wi-Fi Direct Network Configuration

Go to top of page