Home > Network > Select Your Network Connection Type > Wireless Network Connection Examples > Connected to a Computer with a Wireless LAN Access Point Router in the Network (Infrastructure Mode)

### Connected to a Computer with a Wireless LAN Access Point Router in the Network (Infrastructure Mode)

Related Models:DocuPrint P268 dw
This type of network has a wireless LAN central access point/router at the heart of the network. The access point can also act as a bridge or a gateway to a wired network. When the Fuji Xerox wireless machine (your machine) is part of this network, it receives all print jobs via an access point.

1. Wireless LAN Access Point/Router
2. Wireless Network Machine (your machine)
3. Wireless Computer Connected to the Wireless LAN Access Point/Router
4. Wired Computer Connected to the Wireless LAN Access Point/Router with a Network Cable

Configuration Method

Select one of these methods for configuring your Fuji Xerox machine in a wireless network environment.

- Wireless Configuration Using the Setup Wizard from the Computer (Recommended)
- Wireless Configuration Using the Setup Wizard from the Control Panel
- One-Push Wireless Configuration Using WPS or AOSS™
- PIN Method Wireless Configuration Using WPS

Related Information
  - Wireless Network Connection Examples
  - Configure Your Machine for a Wireless Network Using the PIN Method of Wi-Fi Protected Setup™ (WPS)
  - Configure Your Machine for a Wireless Network Using the One Push Method of Wi-Fi Protected Setup™ (WPS) or AOSS™
  - Configure Your Machine for a Wireless Network When the SSID Is Not Broadcast

Go to top of page