## Specifications

This chapter covers the machines primary specifications.

This chapter includes:

- Hardware specifications

- Environmental specifications

- Electrical specifications

- Print media specifications

The specification values are listed below: specifications are subject to change without notice: See www.lenovo.com.cn for possible changes in information.

## Hardware specifications

Item | Description
--- | ---
Dimension | Height | 234 mm (9.21 inches)
Depth | 299 mm (11.77 inches)
Width | 388 mm (15.28 inches)
Weight | Machine with consumables | 7.5 kg (16.53 lbs)
Package weight | Paper | 1.22 kg (2.69 lbs)
Plastic | 0.24 kg (0.52 lbs)

## Environmental specifications

Item | Description
--- | ---
Noise Level[a] | Ready mode | 26 dB(A)
Printing mode | 49 dB(A)
Copying mode | 49 dB(A)
Temperature | Operation | 10 to 32 °C (50 to 90 °F)
Storage (unpacked) | 0 to 40 °C (32 to 104 °F)
Humidity | Operation | 10 to 80% RH
Storage (unpacked) | 20 to 80% RH
[a] Sound Pressure Level, ISO 7779. Configuration tested: machine basic installation, A4 paper, simplex printing.

## Electrical specifications

Power requirements are based on the country/region where the device is sold. Do not convert operating voltages. Doing so might damage the device and void the product warranty.

Item | Description
--- | ---
Power rating [a] | 110 volt models | AC 110 - 127 V
220 volt models | AC 220 - 240 V
Power consumption | Average operating mode | Less than 270W
Ready mode | Less than 36W
Power save mode |

- SCX-3200 Series: 3.8W

- SCX-3205W(K): 5.6 W

Power off mode | Less than 0.45 W
[a] See the rating label on the machine for the correct voltage (V), frequency (hertz) and type of current (A) for your machine.

## Print media specifications

Type | Size | Dimensions | Print media weight[a]/Capacity[b]
--- | --- | --- | ---
Tray | Manual feeding in the tray
Plain paper | Letter | 216 x 279 mm (8.50 x 11.00 inches) | 60 to 120 g/m2 (16 to 32 lbs bond)

- 150 sheets of 80 g/m2 (20 lbs bond)

60 to 163 g/m2 (16 to 43 lbs bond)

- 1 sheet for manual feeding in the tray

Legal | 216 x 356 mm (8.50 x 14.00 inches)
US Folio | 216 x 330 mm (8.50 x 13.00 inches)
A4 | 210 x 297 mm (8.27 x 11.69 inches)
Oficio | 216 x 343 mm (8.50 x 13.50 inches)
JIS B5 | 182 x 257 mm (7.17 x 10.12 inches)
ISO B5 | 176 x 250 mm (6.93 x 9.84 inches)
Executive | 184 x 267 mm (7.25 x 0 inches)
A5 | 148 x 210 mm (5.83 x 8.27 inches)
Envelope | Envelope Monarch | 98 x 191 mm (3.87 x 7.50 inches) | 75 to 90 g/m2 (20 to 24 lbs bond)

- 1 sheet for manual feeding in the tray

Envelope No. 10 | 105 x 241 mm (4.12 x 9.50 inches)
Envelope DL | 110 x 220 mm (4.33 x 8.66 inches)
Envelope C5 | 162 x 229 mm (6.38 x 9.02 inches)
Thick paper | Refer to the Plain paper section | Refer to the Plain paper section | 90 g/m2 (24 lbs bond)

- 140 sheets

90 to 163 g/m2 (24 to 43 lbs bond)

- 1 sheet for manual feeding in the tray

Thin paper | Refer to the Plain paper section | Refer to the Plain paper section | 60 to 70 g/m2 (16 to 19 lbs bond)

- 1 sheet for manual feeding in the tray

Transparency | Letter, A4 | Refer to the Plain paper section | 138 to 146 g/m2 (37 to 39 lbs bond)

- 1 sheet for manual feeding in the tray

Labels[c] | Letter, Legal, US Folio, A4, JIS B5, ISO B5, Executive, A5 | Refer to the Plain paper section | 120 to 150 g/m2 (32 to 40 lbs bond)

- 1 sheet for manual feeding in the tray

Card stock | Letter, Legal, US Folio, A4, JIS B5, ISO B5, Executive, A5 | Refer to the Plain paper section | 105 to 163 g/m2 (28 to 43 lbs bond)

- 1 sheet for manual feeding in the tray

Minimum size (custom) | 76 x 196 mm (3.00 x 7.70 inches) | 60 to 163 g/m2 (16 to 43 lbs bond)
Maximum size (custom) | 216 x 356 mm (8.50 x 14.02 inches)
[a] If media weight is over 120 g/m2 (32 lbs), load a paper into the tray one by one. [b] Maximum capacity may differ depending on media weight, thickness and environmental conditions. [c] Smoothness: 100 to 250 (sheffield).