Lenovo Digital MFC


This product has the following restrictions and issues.  Please be sure to read this before using.

--------------------------------------------------------------------------------
Installation
--------------------------------------------------------------------------------

Issues
======

When a WIA driver is already installed, uninstall it manually and then install it again.
To uninstall the WIA driver manually, follow the procedure below:
(1) Open [Scanners and Cameras] in [Control Panel].
(2) Right-click the WIA driver you want to uninstall.
(3) Select [Delete].
(4) Restart the PC.
(5) Delete the C:\Windows\system32\LEewscan folder.
  (Note that the folder path may vary depending on the drive where the OS is installed.)

--------------------------------------------------------------------------------
M9530				Version 4.22.20.0
--------------------------------------------------------------------------------

To use M9530, perform the settings according to the procedure below.
(1) Open [Scanners and Cameras] in [Control Panel].
(2) Right-click the WIA driver you want to connect to the MFC.
(3) Select [Properties].
(4) Select [Device Setting] tab and click the [Discover] button.
(5) The local search function is available.  Make a local search.

This software supports the following models:
-M9530

Issues 
========

1. Notes on Using the WIA Driver
(1) Touch Panel during WIA Connection
- During WIA scan, the operation panel only displays special screens for RemoteScan.
- By pressing the [CANCEL] button on the operation panel, a WIA connection session can be forcibly terminated.
* Buttons other than [CANCEL] are disabled.
* Canceling from the client application or a Network Management Tool scan job is possible.
* WIA scan connection continues until image transfer to the client PC is finished.  Therefore, it may take several minutes before other operations become available after the scan is completed.
(2) Restrictions on the WIA Driver
- No notification report is transmitted whether WIA scan is completed normally or abnormally.

(3) When using Microsoft Office XP, SP2 or higher is required.

(4) When using Windows Server 2003, set the startup type for the Windows Image Acquisition (WIA) service to [Automatic] using the management tool beforehand.
 1. Right-click [My Computer].
 2. Select [Manage].
 3. Click [Services and Applications].
 4. Click [Services].
 5. Double-click [Windows Image Acquisition (WIA)].
 6. On the [General] tab, select [Automatic] in the [Startup Type] box.
 7. Click [Apply] and [OK].

(5) Only one driver can be installed.  Installation of several drivers is not supported.

(6) When you use Photoshop to scan a document, an error message may appear when scanning is completed.  However, it has no effect on scanning.

(7) When you use an imaging application to scan a document, configure the following settings before scanning:  When the settings have not been configured, scanned images become black.
 1. Select [Tools] -> [Options] -> [Scan] from the imaging application menu bar.
 2. Click the [Advanced] button.
 3. Check [Native].

(8) When you use Microsoft Scanner and Camera Wizard to scan a document, the resolution defined in the properties description for a saved file may be incorrect.
In such a case, use File Downloader or the TWAIN driver to save the document in a file.

(9) When you use Photoshop or other TWAIN-compliant imaging applications to scan a document, the ADF is not supported.
To use the ADF, use Microsoft Scanner and Camera Wizard or the TWAIN driver to scan a document.

(10) When you click the [Cancel] button to cancel scanning of a document using Photoshop or other TWAIN-compliant imaging applications, restart the application to scan the document.

(11) If you use the M9530 on which the user authentication is effective, perform the following procedure before scanning.
 When you use Microsoft Scanner and Camera Wizard:
 1. On the [Choose Scanning Preferences] window, click the [Custom Settings] button.
 2. When the Properties dialog box is displayed, click the [Device Setting] tab.
 3. Click the [User Authentication] button in the User Authentication box.
 4. When the User Authentication dialog box is displayed, input correct certification information in each field and click the [OK] button.

When the driver is used from another application, configure similar settings in the Properties dialog box.

Troubleshooting
======================
1. Cannot find the MFC.

[Problem Description] 
Even the Local Discovery function cannot find the MFC.

[Corrective Action] 
Please check the following:
- The MFC and PC are connected to the network via TCP/IP.
- The gateway setting is correct in the case that the device is in the different subnet area.


2. Cannot connect the MFC which was found by the Local Discovery function. 

[Problem Description]
The MFC was found by the Local Discovery function but cannot be connected after being selected.

[Corrective Action] 
(1) Check that the Microsoft Internet Explorer 5.5 SP2 or later is installed.
(2) Check that the proxy setting of the Microsoft Internet Explorer is correct so that the MFC can be connected.
(3) Check that the Microsoft Internet Explorer is online.  If it is offline, set it to online.

--------------------------------------------------------------------------------
Trademarks
--------------------------------------------------------------------------------

- The official name of Windows Server 2003 is Microsoft Windows Server 2003 Operating System.
- Microsoft, Windows and the brand names and product names of other Microsoft products are trademarks of Microsoft Corporation in the US and other countries.
- Other company names and product names in this manual are the trademarks of their respective companies.





			March 24, 2012