1.Before Using the Printer

1.1.Product series introduction

Product series parameters | P3010D series | P2800DW / P3010DW series | P3300 series | P3300DN series | P3300DW series
Interface type | USB | ● | ● | ● | ● | ●
NET |  | ● |  | ● | ●
Wi-Fi |  | ● |  |  | ●
Print Language | GDI | ● | ● |  |  |
PDL |  |  | ● | ● | ●
Control Panel | LED | ● |  |  |  |
LCD |  | ● | ● | ● | ●
Print Speed | A4 | 30ppm | ● | ● |  |  |
33ppm |  |  | ● | ● | ●
Letter | 32ppm | ● | ● |  |  |
35ppm |  |  | ● | ● | ●
Automatic Two-Sided Printing | ● | ● |  | ● | ●
NFC function |  | ● |  |  | ●
Mute printing | ● | ● | ● | ● | ●

(●: Support; Blank: Unsupport)

This product series is subject to additions or changes without prior notice.

1.2.Supplied Accessories

Name | Parts
Toner cartridge |
Drum component |
USB Interface Cable |
Power Cord |
CD |
Quick Setup Guide |
Pantum Warranty |

| Note： | • The Pantum Warranty may not be attached in some regions.

1.3.Product View

Side view

1 | Output Bin | For storing the printed paper.
2 | Control Panel | Indicate printer status to conduct set operation.
3 | Output Tray | To prevent the printed paper from falling.
4 | Front Cover | To open the front cover to take out the laser toner cartridge.
5 | Manual feed tray | For placing mediums that are printed in manual feed tray.
6 | Power switch | Turn the power on or off and press this button under Ready state to enter energy-saving mode. Press and hold this button for more than 2s to turn the printer power off.
7 | Automatic Feeder Tray | For placing mediums that are printed in auto feed tray.
8 | Paper deflector of manual feed tray | Slide paper deflector to adapt to paper width.
9 | NFC (Near Field Communication) label | Touch this label on mobile device to download or start Pantum printer App and connect Wi-Fi Directly.
10 | Paper width deflector of auto feed tray | Slide paper width deflector to adapt to paper width.
11 | Paper length deflector of auto feed tray | Slide paper length deflector to adapt to paper length.
12 | Clip of extended tray of auto feed tray | For adjustment of length extension of the tray .

Rear View

1 | USB Interface | For connecting product to computer with USB cable.
2 | Network Interface | For connecting product to network with network cable.
3 | Power Interface | For connecting product to power with power cord.
4 | Rear Cover | For paper release when it gets jammed.
5 | Duplex Printing Unit | For paper feed at duplex printing and paper release when paper gets jammed at duplex printing.

| Note： | Printer appearance may differ because of various models and functions, so the schematic diagram is only for your reference.

1.4.Laser Toner Cartridge

Laser toner cartridge is composed of drum component and toner cartridge.

Service life of drum component

Type | Average Print Volume
Longevity of drum component | About 12000 Pages(Based on ISO 19752 standard)

Service life of toner cartridge

Type | Average Print Volume
Standard-volume toner cartridge | About 1500 Pages(Based on ISO 19752 standard)
High-volume toner cartridge | About 3000 Pages(Based on ISO 19752 standard)

| Note： | • The model is subject to increase without notice. • Consumables capacity may vary with different using types. • The Company does not recommend using consumables other than the original consumables provided, as any damages caused by non-original consumables are not covered by the scope of warranty. • Toner cartridge appearance may differ because of multiple volume and models, so the schematic diagram is only for your reference.

1.5.Control Panel

1.5.1.Overview of control panel

The layout of the printer control panel is shown below:

LCD control panel

No. | Name | Functions
1 | LCD Display | Display operation interface and product information.
2 | Wi-Fi indicator/save toner indicator | Indicate Wi-Fi connection status (applicable to Wi-Fi model only). Indicate the on/off of save toner function (applicable to non-Wi-Fi model only). (Please refer to Chapter 1.5.2.1)
3 | Toner cartridge/status indicator | Indicate the status of toner cartridge and printer (please refer to Chapter 1.5.2.1)
4 | Menu | Open the main menu of control panel.
5 | OK | Confirm the selection on screen.
6 | UP | Scroll through the menus and options . For menu items need to input, change the numeric value by cycle accumulating.
7 | Down | Scroll through the menus and options . For menu item needs to be input, shift the entry positions from left to right, for example, IP address entry.
8 | Back | Return to the previous menu.
9 | Wi-Fi key/save toner key | Start Wi-Fi function (applicable to Wi-Fi model only). When Wi-Fi is connecting, press the button for 2s or longer to cancel Wi-Fi connection; when Wi-Fi is connected, press the button for 2s or longer, "Wi-Fi connection" interface will pop up, and select "Disc from RT" to disconnect Wi-Fi connection (only for Wi-Fi model). Open save toner function(applicable to non-Wi-Fi model only).
11 | Cancel | Execute cancel operation.

LED control panel

No. | Name | Functions
1 | Drum/paper status indicator | Indicate the status of paper and drum component (please refer to Chapter 1.5.2.2).
2 | Toner cartridge/status indicator | Indicate the status of toner cartridge and others other than paper (please refer to Chapter 1.5.2.2).
3 | Cancel/continously press key | Press this button for more than 2s to cancel current printing operation under normal printing condition. Press this button to continue the current printing operation, or press this key for more than 2s to cancel the current printing operation when paper feed fails or it is lack of paper. Press this button for more than 2s to print information page at idle state.

1.5.2.Indicator function of control panel

1.5.2.1.Indicator status display of LCD control panel

Display meanings of Wi-Fi / save toner indicator are as follows:

No. | Display of Wi-Fi/save toner indicator | Status | Status description (applicable to Wi-Fi model only) | Status description (applicable to non-Wi-Fi model only)
1 |  | Die out | Wi-Fi disconnected and sleep mode | Turn save toner state function and sleep mode
2 |  | Blue indicator blinks | Wi-Fi connecting | None
3 |  | Blue indicator normally on | Wi-Fi connected | Turn on save toner function

Display meanings of toner cartridge / status indicator are as follows:

No. | Display of toner cartridge/status indicator | Status | Status description
1 |  | Die out | Sleep mode
2 |  | Green indicator blinks | Warming up, printing, print cancelling
3 |  | Green indicator normally on | Printer is ready
4 |  | Orange indicator blinks | Low toner warning
5 |  | Orange indicator normally on | Toner cartridge error (uninstalled ink cartridge, unmatching ink cartridge, invalid toner cartridge)
6 |  | Red indicator normally on | Printer errors such as paper error (paper out, paper jam, paper feed failure), opened front cover

1.5.2.2.Indicator status display of LED control panel

Display meanings of drum component/paper status indicators are as follows:

No. | Display of drum component/paper status indicators | Status | Status description
1 |  | Die out | Sleep mode
2 |  | Green indicator normally on | Normal drum, paper out failure
3 |  | Red indicator normally on | Drum component error (uninstalled drum component, unmatching drum component, invalid drum component), paper error (paper out, paper jam, paper feed failure)
4 |  | Orange indicator normally on | Drum component is about to end its expected service life

Display meanings of toner cartridge/status indicator are as follows:

No. | Display of toner cartridge/status indicator | Status | Status description
1 |  | Die out | Sleep mode
2 |  | Green indicator normally on | Printer is ready
3 |  | Green indicator blinks | Warming up, printing, print cancelling
4 |  | Red indicator normally on | Printer errors such as opened front cover
5 |  | Orange indicator normally on | Toner cartridge error (uninstalled ink cartridge, unmatching ink cartridge, invalid toner cartridge)
6 |  | Orange indicator blinks | Low toner warning