OS_64.DCK
---------

LROS ROM extension cartridge which support 64-column writing on the screen.
Only two screen colors is supported with OS_64 because the attribute file
locations are not used. The colors can be changed using standard INK or PAPER
commands. Cartridge is auto-boot, so after Timex initialization you will
automatically enter 64-column mode.
