09:46:42|<info> Capture package is started!(localIP:10.11.9.220，port:5060, sockType:UdpServer)
09:46:42|<info> CATConnObj::start 
09:46:42|<info> Command Server is start!
09:46:42|<info> CATConnObjManager::start 
09:46:42|<info> CATRunEngine::start 
09:46:42|<info> Testcase is started! (testDevice IP:10.11.9.112)
09:47:23|<info> expectLuas REGISTER401, recvMsgID:Keepalive, state 0 
09:47:23|<info> ###respMsgSIP/2.0 200 OK
Via: SIP/2.0/UDP 10.11.9.112:5060;rport;branch=z9hG4bK584100212
To: <sip:34020000002000000001@10.11.9.220:5060>;tag=12341241234
From: <sip:34020000001180000001@10.11.9.112:5060>;tag=959229424
Call-ID: 716991739@10.11.9.112
CSeq: 20 MESSAGE
User-Agent: General
Content-Length: 0


09:48:23|<info> expectLuas REGISTER401, recvMsgID:Keepalive, state 0 
09:48:23|<info> ###respMsgSIP/2.0 200 OK
Via: SIP/2.0/UDP 10.11.9.112:5060;rport;branch=z9hG4bK1575133355
To: <sip:34020000002000000001@10.11.9.220:5060>;tag=12341241234
From: <sip:34020000001180000001@10.11.9.112:5060>;tag=1357898575
Call-ID: 1019749103@10.11.9.112
CSeq: 20 MESSAGE
User-Agent: General
Content-Length: 0


09:48:42|<info> CATRunEngine::notifyStepResult errSteps = 1
09:48:42|<info> caseName:1 注册, groupName:1.1 注册应答, stepName:1.1.1 等待无鉴权注册
recvMsg:
sendMsg:
09:48:49|<info> expectLuas REGISTER, recvMsgID:REGISTER401, state 0 
09:48:49|<info> recv a wait message REGISTER401, message id:0
09:48:49|<info> push  a wait message REGISTER401, message id:0, m_pos:0
09:48:49|<info> expectLuas REGISTER, recvMsgID:REGISTER, state 0 
09:48:49|<info> push  a wait message REGISTER, message id:1, m_pos:1
09:48:49|<info> caseName:1 注册, groupName:1.1 注册应答, stepName:1.1.2 等待有鉴权注册
recvMsg:
REGISTER sip:34020000002000000001@10.11.9.220:5060 SIP/2.0
Via: SIP/2.0/UDP 10.11.9.112:5060;rport;branch=z9hG4bK1243115335
Route: <sip:34020000001180000001@10.11.9.220:5060;lr>
From: <sip:34020000001180000001@10.11.9.112:5060>;tag=135343862
To: <sip:34020000001180000001@10.11.9.112:5060>
Call-ID: 932760449@10.11.9.112
CSeq: 4 REGISTER
Contact: <sip:34020000001180000001@10.11.9.112:5060>
Authorization: Digest username="34020000001180000001", realm="34020000", nonce="awer23sdfj123123", uri="sip:34020000002000000001@10.11.9.220:5060", response="95ee19d0c008be74995cdd6d048cfdc4", algorithm=MD5, opaque="c3a02f1ecb122d255c4ae2266129d044"
Max-Forwards: 70
User-Agent: Dahua SIP UAS V1.0
Expires: 3600
Content-Length: 0

sendMsg:
SIP/2.0 200 OK
Via: SIP/2.0/UDP 10.11.9.112:5060;rport;branch=z9hG4bK1243115335
From: <sip:34020000001180000001@10.11.9.112:5060>;tag=135343862
To: <sip:34020000001180000001@10.11.9.112:5060>;tag=31243r3412
Call-ID: 932760449@10.11.9.112
CSeq: 4 REGISTER
User-Agent: General
Date: 2017-03-30T09:48:49
Expires: 300
Content-Length: 0

09:48:50|<info> CATRunEngine::notifyStepResult errSteps = 1
09:48:50|<info> caseName:2 心跳, groupName:2.1 心跳, stepName:2.1.1 等待心跳
recvMsg:
sendMsg:
09:48:50|<info> CATRunEngine::notifyStepResult errSteps = 1
09:48:50|<info> caseName:3 设备信息查询, groupName:3.1 设备信息查询, stepName:3.1.1 发送设备查询信息
sendMsg:
recvMsg:
09:48:50|<info> CATRunEngine::notifyStepResult errSteps = 2
09:48:50|<info> caseName:3 设备信息查询, groupName:3.1 设备信息查询, stepName:3.1.2 等待设备查询信息
recvMsg:
sendMsg:
09:48:50|<info> CATRunEngine::notifyStepResult errSteps = 1
09:48:50|<info> caseName:4 设备目录查询, groupName:4.1 设备目录查询, stepName:4.1.1 发送设备目录查询命令
sendMsg:
recvMsg:
09:48:50|<info> CATRunEngine::notifyStepResult errSteps = 2
09:48:50|<info> caseName:4 设备目录查询, groupName:4.1 设备目录查询, stepName:4.1.2 等待设备目录信息
recvMsg:
sendMsg:
09:48:50|<info> CATRunEngine::notifyStepResult errSteps = 1
09:48:50|<info> caseName:5 设备状态查询, groupName:5.1 设备状态查询, stepName:5.1.1 发送状态查询
sendMsg:
recvMsg:
09:48:50|<info> CATRunEngine::notifyStepResult errSteps = 2
09:48:50|<info> caseName:5 设备状态查询, groupName:5.1 设备状态查询, stepName:5.1.2 等待状态消息
recvMsg:
sendMsg:
09:48:50|<info> expectLuas MESSAGE-200, recvMsgID:MESSAGE-200, state 0 
09:48:50|<info> caseName:6 配置查询, groupName:6.1 视频编码配置, stepName:6.1.1 视频配置查询
sendMsg:
MESSAGE sip:34020000001180000001@10.11.9.112:5060 SIP/2.0
From: <sip:34020000002000000001@3402000000>;tag=bccedfd000004
To: <sip:34020000001180000001@10.11.9.112:5060>
Content-Length: 183
CSeq: 5 MESSAGE
Route: <sip:34020000001180000001>
Call-ID: 12345678900004
Via: SIP/2.0/UDP 10.11.9.220:5060;wlsscid=377aa9afcf1b36f;branch=123133532300004
Content-Type: Application/MANSCDP+xml
Max-Forwards: 70


<?xml version="1.0"?>
<Query>
<CmdType>ConfigDownload</CmdType>
<SN>249</SN>
<DeviceID>34020000001310000001</DeviceID>
<ConfigType>VideoParamConfig</ConfigType>
</Query>


recvMsg:
SIP/2.0 200 OK
Via: SIP/2.0/UDP 10.11.9.220:5060;wlsscid=377aa9afcf1b36f;branch=123133532300004
From: <sip:34020000002000000001@3402000000>;tag=bccedfd000004
To: <sip:34020000001180000001@10.11.9.112:5060>;tag=1050068321
Call-ID: 12345678900004
CSeq: 5 MESSAGE
User-Agent: Dahua SIP UAS V1.0
Content-Length: 0

09:48:50|<info> expectLuas VideoParamConfig, recvMsgID:VideoParamConfig, state 0 
09:48:50|<info> push  a wait message VideoParamConfig, message id:0, m_pos:0
09:48:50|<info> caseName:6 配置查询, groupName:6.1 视频编码配置, stepName:6.1.2 等待视频编码
recvMsg:
MESSAGE sip:34020000002000000001@3402000000 SIP/2.0
Via: SIP/2.0/UDP 10.11.9.112:5060;rport;branch=z9hG4bK109742411
From: <sip:34020000001180000001@10.11.9.112:5060>;tag=1927854604
To: <sip:34020000002000000001@3402000000>
Call-ID: 2095346279@10.11.9.112
CSeq: 20 MESSAGE
Max-Forwards: 70
User-Agent: Dahua SIP UAS V1.0
Content-Type: Application/MANSCDP+xml
Content-Length:   521

<?xml version="1.0" encoding="GB2312" ?>
<Response>
    <CmdType>ConfigDownload</CmdType>
    <SN>249</SN>
    <DeviceID>34020000001310000001</DeviceID>
    <Result>OK</Result>
    <VideoParamConfig Num="1">
        <Item>
            <StreamName>Stream1</StreamName>
            <VideoFormat>2</VideoFormat>
            <Resolution>6</Resolution>
            <FrameRate>0</FrameRate>
            <BitRateType>2</BitRateType>
            <VideoBitRate>0</VideoBitRate>
        </Item>
    </VideoParamConfig>
</Response>
sendMsg:
SIP/2.0 200 OK
Via: SIP/2.0/UDP 10.11.9.112:5060;rport;branch=z9hG4bK109742411
To: <sip:34020000002000000001@3402000000>;tag=12341241234
From: <sip:34020000001180000001@10.11.9.112:5060>;tag=1927854604
Call-ID: 2095346279@10.11.9.112
CSeq: 20 MESSAGE
User-Agent: General
Content-Length: 0

09:48:50|<info> expectLuas MESSAGE-200, recvMsgID:MESSAGE-200, state 0 
09:48:50|<info> caseName:6 配置查询, groupName:6.2 音频编码配置, stepName:6.2.1 音频编码配置查询
sendMsg:
MESSAGE sip:34020000001180000001@10.11.9.112:5060 SIP/2.0
From: <sip:34020000002000000001@3402000000>;tag=bccedfd000005
To: <sip:34020000001180000001@10.11.9.112:5060>
Content-Length: 181
CSeq: 5 MESSAGE
Route: <sip:34020000001180000001>
Call-ID: 12345678900005
Via: SIP/2.0/UDP 10.11.9.220:5060;wlsscid=377aa9afcf1b36f;branch=123133532300005
Content-Type: Application/MANSCDP+xml
Max-Forwards: 70


<?xml version="1.0"?>
<Query>
<CmdType>ConfigDownload</CmdType>
<SN>249</SN>
<DeviceID>34020000001310000001</DeviceID>
<ConfigType>AudioParamConfig</ConfigType>
</Query>

recvMsg:
SIP/2.0 200 OK
Via: SIP/2.0/UDP 10.11.9.220:5060;wlsscid=377aa9afcf1b36f;branch=123133532300005
From: <sip:34020000002000000001@3402000000>;tag=bccedfd000005
To: <sip:34020000001180000001@10.11.9.112:5060>;tag=508193807
Call-ID: 12345678900005
CSeq: 5 MESSAGE
User-Agent: Dahua SIP UAS V1.0
Content-Length: 0

09:48:50|<info> expectLuas AudioParamConfig, recvMsgID:AudioParamConfig, state 0 
09:48:50|<info> push  a wait message AudioParamConfig, message id:0, m_pos:0
09:48:50|<info> caseName:6 配置查询, groupName:6.2 音频编码配置, stepName:6.2.2 等待音频编码
recvMsg:
MESSAGE sip:34020000002000000001@3402000000 SIP/2.0
Via: SIP/2.0/UDP 10.11.9.112:5060;rport;branch=z9hG4bK1735587929
From: <sip:34020000001180000001@10.11.9.112:5060>;tag=2099534560
To: <sip:34020000002000000001@3402000000>
Call-ID: 2057182779@10.11.9.112
CSeq: 20 MESSAGE
Max-Forwards: 70
User-Agent: Dahua SIP UAS V1.0
Content-Type: Application/MANSCDP+xml
Content-Length:   447

<?xml version="1.0" encoding="GB2312" ?>
<Response>
    <CmdType>ConfigDownload</CmdType>
    <SN>249</SN>
    <DeviceID>34020000001310000001</DeviceID>
    <Result>OK</Result>
    <AudioParamConfig Num="1">
        <Item>
            <StreamName>Stream1</StreamName>
            <AudioFormat>1</AudioFormat>
            <AudioBitRate>8</AudioBitRate>
            <SamplingRate>1</SamplingRate>
        </Item>
    </AudioParamConfig>
</Response>
sendMsg:
SIP/2.0 200 OK
Via: SIP/2.0/UDP 10.11.9.112:5060;rport;branch=z9hG4bK1735587929
To: <sip:34020000002000000001@3402000000>;tag=12341241234
From: <sip:34020000001180000001@10.11.9.112:5060>;tag=2099534560
Call-ID: 2057182779@10.11.9.112
CSeq: 20 MESSAGE
User-Agent: General
Content-Length: 0

09:48:50|<info> expectLuas MESSAGE-200, recvMsgID:MESSAGE-200, state 0 
09:48:50|<info> caseName:6 配置查询, groupName:6.3 国标配置查询, stepName:6.3.1 国标编码配置查询
sendMsg:
MESSAGE sip:34020000001180000001@10.11.9.112:5060 SIP/2.0
From: <sip:34020000002000000001@3402000000>;tag=bccedfd000006
To: <sip:34020000001180000001@10.11.9.112:5060>
Content-Length: 175
CSeq: 5 MESSAGE
Route: <sip:34020000001180000001>
Call-ID: 12345678900006
Via: SIP/2.0/UDP 10.11.9.220:5060;wlsscid=377aa9afcf1b36f;branch=123133532300006
Content-Type: Application/MANSCDP+xml
Max-Forwards: 70


<?xml version="1.0"?>
<Query>
<CmdType>ConfigDownload</CmdType>
<SN>249</SN>
<DeviceID>34020000001310000001</DeviceID>
<ConfigType>BasicParam</ConfigType>
</Query>

recvMsg:
SIP/2.0 200 OK
Via: SIP/2.0/UDP 10.11.9.220:5060;wlsscid=377aa9afcf1b36f;branch=123133532300006
From: <sip:34020000002000000001@3402000000>;tag=bccedfd000006
To: <sip:34020000001180000001@10.11.9.112:5060>;tag=1926780054
Call-ID: 12345678900006
CSeq: 5 MESSAGE
User-Agent: Dahua SIP UAS V1.0
Content-Length: 0

09:48:50|<info> expectLuas BasicParam, recvMsgID:BasicParam, state 0 
09:48:50|<info> push  a wait message BasicParam, message id:0, m_pos:0
09:48:50|<info> caseName:6 配置查询, groupName:6.3 国标配置查询, stepName:6.3.2 等待国标配置
recvMsg:
MESSAGE sip:34020000002000000001@3402000000 SIP/2.0
Via: SIP/2.0/UDP 10.11.9.112:5060;rport;branch=z9hG4bK1481942178
From: <sip:34020000001180000001@10.11.9.112:5060>;tag=1681582188
To: <sip:34020000002000000001@3402000000>
Call-ID: 2003613146@10.11.9.112
CSeq: 20 MESSAGE
Max-Forwards: 70
User-Agent: Dahua SIP UAS V1.0
Content-Type: Application/MANSCDP+xml
Content-Length:   666

<?xml version="1.0" encoding="GB2312" ?>
<Response>
    <CmdType>ConfigDownload</CmdType>
    <SN>249</SN>
    <DeviceID>34020000001310000001</DeviceID>
    <Result>OK</Result>
    <BasicParam>
        <Name>DH-NVR7808</Name>
        <DeviceID>34020000001180000001</DeviceID>
        <SIPServerID>34020000002000000001</SIPServerID>
        <SIPServerIP>10.11.9.220</SIPServerIP>
        <SIPServerPort>5060</SIPServerPort>
        <DomainName>3402000000</DomainName>
        <Expiration>3600</Expiration>
        <Password>12345678</Password>
        <HeartBeatInterval>60</HeartBeatInterval>
        <HeartBeatCount>3</HeartBeatCount>
    </BasicParam>
</Response>
sendMsg:
SIP/2.0 200 OK
Via: SIP/2.0/UDP 10.11.9.112:5060;rport;branch=z9hG4bK1481942178
To: <sip:34020000002000000001@3402000000>;tag=12341241234
From: <sip:34020000001180000001@10.11.9.112:5060>;tag=1681582188
Call-ID: 2003613146@10.11.9.112
CSeq: 20 MESSAGE
User-Agent: General
Content-Length: 0

09:48:50|<info> CATRunEngine::notifyStepResult errSteps = 1
09:48:50|<info> caseName:7 手动录像, groupName:7.1 开启手动录像, stepName:7.1.1 开始手动录像
sendMsg:
recvMsg:
09:48:50|<info> CATRunEngine::notifyStepResult errSteps = 2
09:48:50|<info> caseName:7 手动录像, groupName:7.1 开启手动录像, stepName:7.1.2 等待开启成功
recvMsg:
sendMsg:
09:48:51|<info> CATRunEngine::notifyStepResult errSteps = 3
09:48:51|<info> caseName:7 手动录像, groupName:7.2 等待录像, stepName:7.2.1 录像ing
sendMsg:
recvMsg:
09:48:51|<info> CATRunEngine::notifyStepResult errSteps = 4
09:48:51|<info> caseName:7 手动录像, groupName:7.3 停止手动录像, stepName:7.3.1 停止手动录像
sendMsg:
recvMsg:
09:48:51|<info> CATRunEngine::notifyStepResult errSteps = 5
09:48:51|<info> caseName:7 手动录像, groupName:7.3 停止手动录像, stepName:7.3.2 等待停止成功
recvMsg:
sendMsg:
09:48:51|<info> CATRunEngine::notifyStepResult errSteps = 1
09:48:51|<info> caseName:8 视频通道布撤防与报警, groupName:8.1 远程撤防, stepName:8.1.1 全部撤防
sendMsg:
recvMsg:
09:48:51|<info> CATRunEngine::notifyStepResult errSteps = 2
09:48:51|<info> caseName:8 视频通道布撤防与报警, groupName:8.1 远程撤防, stepName:8.1.2 等待控制结果
recvMsg:
sendMsg:
09:48:51|<info> CATRunEngine::notifyStepResult errSteps = 3
09:48:51|<info> caseName:8 视频通道布撤防与报警, groupName:8.1 远程撤防, stepName:8.1.3 普通等待
sendMsg:
recvMsg:
09:48:51|<info> CATRunEngine::notifyStepResult errSteps = 4
09:48:51|<info> caseName:8 视频通道布撤防与报警, groupName:8.2 布防与报警上报, stepName:8.2.1 布防通道
sendMsg:
recvMsg:
09:48:51|<info> CATRunEngine::notifyStepResult errSteps = 5
09:48:51|<info> caseName:8 视频通道布撤防与报警, groupName:8.2 布防与报警上报, stepName:8.2.2 等待布防成功
recvMsg:
sendMsg:
09:48:51|<info> CATRunEngine::notifyStepResult errSteps = 6
09:48:51|<info> caseName:8 视频通道布撤防与报警, groupName:8.2 布防与报警上报, stepName:8.2.3 等待初次遮挡报警
recvMsg:
sendMsg:
09:48:52|<info> CATRunEngine::notifyStepResult errSteps = 7
09:48:52|<info> caseName:8 视频通道布撤防与报警, groupName:8.2 布防与报警上报, stepName:8.2.4 回复初次报警信息
sendMsg:
recvMsg:
09:48:52|<info> CATRunEngine::notifyStepResult errSteps = 8
09:48:52|<info> caseName:8 视频通道布撤防与报警, groupName:8.2 布防与报警上报, stepName:8.2.5 普通等待
sendMsg:
recvMsg:
09:48:52|<info> CATRunEngine::notifyStepResult errSteps = 9
09:48:52|<info> caseName:8 视频通道布撤防与报警, groupName:8.3 复位与报警上报, stepName:8.3.1 发送复位命令
sendMsg:
recvMsg:
09:48:52|<info> CATRunEngine::notifyStepResult errSteps = 10
09:48:52|<info> caseName:8 视频通道布撤防与报警, groupName:8.3 复位与报警上报, stepName:8.3.2 等待复位成功
recvMsg:
sendMsg:
09:48:55|<info> CATRunEngine::notifyStepResult errSteps = 11
09:48:55|<info> caseName:8 视频通道布撤防与报警, groupName:8.3 复位与报警上报, stepName:8.3.3 等待复位后遮挡报警
recvMsg:
sendMsg:
09:48:55|<info> CATRunEngine::notifyStepResult errSteps = 12
09:48:55|<info> caseName:8 视频通道布撤防与报警, groupName:8.3 复位与报警上报, stepName:8.3.4 回复复位后报警信息
sendMsg:
recvMsg:
09:48:55|<info> CATRunEngine::notifyStepResult errSteps = 13
09:48:55|<info> caseName:8 视频通道布撤防与报警, groupName:8.4 撤防, stepName:8.4.1 撤防通道
sendMsg:
recvMsg:
09:48:55|<info> CATRunEngine::notifyStepResult errSteps = 14
09:48:55|<info> caseName:8 视频通道布撤防与报警, groupName:8.4 撤防, stepName:8.4.2 等待撤防成功
recvMsg:
sendMsg:
09:48:55|<info> CATRunEngine::notifyStepResult errSteps = 15
09:48:55|<info> caseName:8 视频通道布撤防与报警, groupName:8.4 撤防, stepName:8.4.3 普通等待
sendMsg:
recvMsg:
09:48:55|<info> CATRunEngine::notifyStepResult errSteps = 1
09:48:55|<info> caseName:9 报警通道布撤防与报警, groupName:9.1 远程撤防, stepName:9.1.1 全部撤防
sendMsg:
recvMsg:
09:48:55|<info> CATRunEngine::notifyStepResult errSteps = 2
09:48:55|<info> caseName:9 报警通道布撤防与报警, groupName:9.1 远程撤防, stepName:9.1.2 等待控制结果
recvMsg:
sendMsg:
09:48:55|<info> CATRunEngine::notifyStepResult errSteps = 3
09:48:55|<info> caseName:9 报警通道布撤防与报警, groupName:9.1 远程撤防, stepName:9.1.3 普通等待
sendMsg:
recvMsg:
09:48:55|<info> CATRunEngine::notifyStepResult errSteps = 4
09:48:55|<info> caseName:9 报警通道布撤防与报警, groupName:9.2 布防与报警上报, stepName:9.2.1 布防通道
sendMsg:
recvMsg:
09:48:55|<info> CATRunEngine::notifyStepResult errSteps = 5
09:48:55|<info> caseName:9 报警通道布撤防与报警, groupName:9.2 布防与报警上报, stepName:9.2.2 等待布防成功
recvMsg:
sendMsg:
09:48:58|<info> CATRunEngine::notifyStepResult errSteps = 6
09:48:58|<info> caseName:9 报警通道布撤防与报警, groupName:9.2 布防与报警上报, stepName:9.2.3 等待初次IO报警
recvMsg:
sendMsg:
09:48:58|<info> CATRunEngine::notifyStepResult errSteps = 7
09:48:58|<info> caseName:9 报警通道布撤防与报警, groupName:9.2 布防与报警上报, stepName:9.2.4 回复初次报警信息
sendMsg:
recvMsg:
09:48:59|<info> CATRunEngine::notifyStepResult errSteps = 8
09:48:59|<info> caseName:9 报警通道布撤防与报警, groupName:9.2 布防与报警上报, stepName:9.2.5 普通等待
sendMsg:
recvMsg:
09:48:59|<info> CATRunEngine::notifyStepResult errSteps = 9
09:48:59|<info> caseName:9 报警通道布撤防与报警, groupName:9.3 复位与报警上报, stepName:9.3.1 发送复位命令
sendMsg:
recvMsg:
09:48:59|<info> CATRunEngine::notifyStepResult errSteps = 10
09:48:59|<info> caseName:9 报警通道布撤防与报警, groupName:9.3 复位与报警上报, stepName:9.3.2 等待复位成功
recvMsg:
sendMsg:
09:49:00|<info> CATRunEngine::notifyStepResult errSteps = 11
09:49:00|<info> caseName:9 报警通道布撤防与报警, groupName:9.3 复位与报警上报, stepName:9.3.3 等待复位后IO报警
recvMsg:
sendMsg:
09:49:00|<info> CATRunEngine::notifyStepResult errSteps = 12
09:49:00|<info> caseName:9 报警通道布撤防与报警, groupName:9.3 复位与报警上报, stepName:9.3.4 回复复位后报警信息
sendMsg:
recvMsg:
09:49:01|<info> CATRunEngine::notifyStepResult errSteps = 13
09:49:01|<info> caseName:9 报警通道布撤防与报警, groupName:9.4 撤防, stepName:9.4.1 撤防通道
sendMsg:
recvMsg:
09:49:01|<info> CATRunEngine::notifyStepResult errSteps = 14
09:49:01|<info> caseName:9 报警通道布撤防与报警, groupName:9.4 撤防, stepName:9.4.2 等待撤防成功
recvMsg:
sendMsg:
09:49:01|<info> CATRunEngine::notifyStepResult errSteps = 15
09:49:01|<info> caseName:9 报警通道布撤防与报警, groupName:9.4 撤防, stepName:9.4.3 普通等待
sendMsg:
recvMsg:
09:49:01|<info> CATRunEngine::notifyStepResult errSteps = 1
09:49:01|<info> caseName:10 实时视频, groupName:10.1 实时视频建立_UDP, stepName:10.1.1 打开视频端口
sendMsg:
recvMsg:
09:49:01|<info> CATRunEngine::notifyStepResult errSteps = 2
09:49:01|<info> caseName:10 实时视频, groupName:10.1 实时视频建立_UDP, stepName:10.1.2 发送实时视频请求
sendMsg:
recvMsg:
09:49:01|<info> CATRunEngine::notifyStepResult errSteps = 3
09:49:01|<info> caseName:10 实时视频, groupName:10.1 实时视频建立_UDP, stepName:10.1.3 等待设备回复200OK
recvMsg:
sendMsg:
09:49:01|<info> CATRunEngine::notifyStepResult errSteps = 4
09:49:01|<info> caseName:10 实时视频, groupName:10.1 实时视频建立_UDP, stepName:10.1.4 发送ACK
sendMsg:
recvMsg:
09:49:01|<info> CATRunEngine::notifyStepResult errSteps = 5
09:49:01|<info> caseName:10 实时视频, groupName:10.1 实时视频建立_UDP, stepName:10.1.5 播放码流
sendMsg:
recvMsg:
09:49:01|<info> CATRunEngine::notifyStepResult errSteps = 6
09:49:01|<info> caseName:10 实时视频, groupName:10.1 实时视频建立_UDP, stepName:10.1.6 停止视频请求
sendMsg:
recvMsg:
09:49:01|<info> CATRunEngine::notifyStepResult errSteps = 7
09:49:01|<info> caseName:10 实时视频, groupName:10.1 实时视频建立_UDP, stepName:10.1.7 关闭视频端口
sendMsg:
recvMsg:
09:49:01|<info> CATRunEngine::notifyStepResult errSteps = 8
09:49:01|<info> caseName:10 实时视频, groupName:10.1 实时视频建立_UDP, stepName:10.1.8 普通等待
sendMsg:
recvMsg:
09:49:02|<info> CATRunEngine::notifyStepResult errSteps = 9
09:49:02|<info> caseName:10 实时视频, groupName:10.2 实时视频建立_TCP, stepName:10.2.1 打开视频端口
sendMsg:
recvMsg:
09:49:02|<info> CATRunEngine::notifyStepResult errSteps = 10
09:49:02|<info> caseName:10 实时视频, groupName:10.2 实时视频建立_TCP, stepName:10.2.2 发送实时视频请求
sendMsg:
recvMsg:
09:49:02|<info> CATRunEngine::notifyStepResult errSteps = 11
09:49:02|<info> caseName:10 实时视频, groupName:10.2 实时视频建立_TCP, stepName:10.2.3 等待设备回复200OK
recvMsg:
sendMsg:
09:49:02|<info> CATRunEngine::notifyStepResult errSteps = 12
09:49:02|<info> caseName:10 实时视频, groupName:10.2 实时视频建立_TCP, stepName:10.2.4 发送ACK
sendMsg:
recvMsg:
09:49:02|<info> CATRunEngine::notifyStepResult errSteps = 13
09:49:02|<info> caseName:10 实时视频, groupName:10.2 实时视频建立_TCP, stepName:10.2.5 播放码流
sendMsg:
recvMsg:
09:49:02|<info> CATRunEngine::notifyStepResult errSteps = 14
09:49:02|<info> caseName:10 实时视频, groupName:10.2 实时视频建立_TCP, stepName:10.2.6 停止视频请求
sendMsg:
recvMsg:
09:49:02|<info> CATRunEngine::notifyStepResult errSteps = 15
09:49:02|<info> caseName:10 实时视频, groupName:10.2 实时视频建立_TCP, stepName:10.2.7 关闭视频端口
sendMsg:
recvMsg:
09:49:02|<info> CATRunEngine::notifyStepResult errSteps = 16
09:49:02|<info> caseName:10 实时视频, groupName:10.2 实时视频建立_TCP, stepName:10.2.8 普通等待
sendMsg:
recvMsg:
09:49:02|<info> CATRunEngine::notifyStepResult errSteps = 1
09:49:02|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.1 打开视频端口
sendMsg:
recvMsg:
09:49:02|<info> CATRunEngine::notifyStepResult errSteps = 2
09:49:02|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.2 发送实时视频请求
sendMsg:
recvMsg:
09:49:02|<info> CATRunEngine::notifyStepResult errSteps = 3
09:49:02|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.3 等待设备回复200OK
recvMsg:
sendMsg:
09:49:03|<info> CATRunEngine::notifyStepResult errSteps = 4
09:49:03|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.4 发送ACK
sendMsg:
recvMsg:
09:49:03|<info> CATRunEngine::notifyStepResult errSteps = 5
09:49:03|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.5 播放码流
sendMsg:
recvMsg:
09:49:03|<info> CATRunEngine::notifyStepResult errSteps = 6
09:49:03|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.6 向左转
sendMsg:
recvMsg:
09:49:03|<info> CATRunEngine::notifyStepResult errSteps = 7
09:49:03|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.7 停止向左转
sendMsg:
recvMsg:
09:49:03|<info> CATRunEngine::notifyStepResult errSteps = 8
09:49:03|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.8 等待1
sendMsg:
recvMsg:
09:49:03|<info> CATRunEngine::notifyStepResult errSteps = 9
09:49:03|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.9 向右转
sendMsg:
recvMsg:
09:49:03|<info> CATRunEngine::notifyStepResult errSteps = 10
09:49:03|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.10 停止向右转
sendMsg:
recvMsg:
09:49:03|<info> CATRunEngine::notifyStepResult errSteps = 11
09:49:03|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.11 等待2
sendMsg:
recvMsg:
09:49:03|<info> CATRunEngine::notifyStepResult errSteps = 12
09:49:03|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.12 向上转
sendMsg:
recvMsg:
09:49:03|<info> CATRunEngine::notifyStepResult errSteps = 13
09:49:03|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.13 停止向上转
sendMsg:
recvMsg:
09:49:03|<info> CATRunEngine::notifyStepResult errSteps = 14
09:49:03|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.14 等待3
sendMsg:
recvMsg:
09:49:03|<info> CATRunEngine::notifyStepResult errSteps = 15
09:49:03|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.15 向下转
sendMsg:
recvMsg:
09:49:03|<info> CATRunEngine::notifyStepResult errSteps = 16
09:49:03|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.16 停止向下转
sendMsg:
recvMsg:
09:49:03|<info> CATRunEngine::notifyStepResult errSteps = 17
09:49:03|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.17 等待4
sendMsg:
recvMsg:
09:49:03|<info> CATRunEngine::notifyStepResult errSteps = 18
09:49:03|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.18 焦距放大
sendMsg:
recvMsg:
09:49:03|<info> CATRunEngine::notifyStepResult errSteps = 19
09:49:03|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.19 停止放大
sendMsg:
recvMsg:
09:49:03|<info> CATRunEngine::notifyStepResult errSteps = 20
09:49:03|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.20 等待5
sendMsg:
recvMsg:
09:49:03|<info> CATRunEngine::notifyStepResult errSteps = 21
09:49:03|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.21 焦距缩小
sendMsg:
recvMsg:
09:49:04|<info> CATRunEngine::notifyStepResult errSteps = 22
09:49:04|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.22 停止缩小
sendMsg:
recvMsg:
09:49:04|<info> CATRunEngine::notifyStepResult errSteps = 23
09:49:04|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.23 停止视频请求
sendMsg:
recvMsg:
09:49:04|<info> CATRunEngine::notifyStepResult errSteps = 24
09:49:04|<info> caseName:11 云台控制, groupName:11.1 云台控制, stepName:11.1.24 关闭视频端口
sendMsg:
recvMsg:
09:49:04|<info> CATRunEngine::notifyStepResult errSteps = 1
09:49:04|<info> caseName:12 录像查询全部, groupName:12.1 录像查询_ALL, stepName:12.1.1 查询录像(all)
sendMsg:
recvMsg:
09:49:04|<info> CATRunEngine::notifyStepResult errSteps = 2
09:49:04|<info> caseName:12 录像查询全部, groupName:12.1 录像查询_ALL, stepName:12.1.2 等待录像(all)
recvMsg:
sendMsg:
09:49:04|<info> CATRunEngine::notifyStepResult errSteps = 1
09:49:04|<info> caseName:13 录像回放, groupName:13.1 录像回放_UDP, stepName:13.1.1 获取录像播放时间
sendMsg:
recvMsg:
09:49:04|<info> CATRunEngine::notifyStepResult errSteps = 2
09:49:04|<info> caseName:13 录像回放, groupName:13.1 录像回放_UDP, stepName:13.1.2 等待录像(all)
recvMsg:
sendMsg:
09:49:04|<info> CATRunEngine::notifyStepResult errSteps = 3
09:49:04|<info> caseName:13 录像回放, groupName:13.1 录像回放_UDP, stepName:13.1.3 打开媒体端口
sendMsg:
recvMsg:
09:49:04|<info> CATRunEngine::notifyStepResult errSteps = 4
09:49:04|<info> caseName:13 录像回放, groupName:13.1 录像回放_UDP, stepName:13.1.4 发送录像播放请求
sendMsg:
recvMsg:
09:49:04|<info> CATRunEngine::notifyStepResult errSteps = 5
09:49:04|<info> caseName:13 录像回放, groupName:13.1 录像回放_UDP, stepName:13.1.5 等待设备回复200OK
recvMsg:
sendMsg:
09:49:04|<info> CATRunEngine::notifyStepResult errSteps = 6
09:49:04|<info> caseName:13 录像回放, groupName:13.1 录像回放_UDP, stepName:13.1.6 发送ACK
sendMsg:
recvMsg:
09:49:04|<info> CATRunEngine::notifyStepResult errSteps = 7
09:49:04|<info> caseName:13 录像回放, groupName:13.1 录像回放_UDP, stepName:13.1.7 录像回放
sendMsg:
recvMsg:
09:49:04|<info> CATRunEngine::notifyStepResult errSteps = 8
09:49:04|<info> caseName:13 录像回放, groupName:13.1 录像回放_UDP, stepName:13.1.8 等待录像结束消息
recvMsg:
sendMsg:
09:49:04|<info> CATRunEngine::notifyStepResult errSteps = 9
09:49:04|<info> caseName:13 录像回放, groupName:13.1 录像回放_UDP, stepName:13.1.9 发送录像停止请求
sendMsg:
recvMsg:
09:49:04|<info> CATRunEngine::notifyStepResult errSteps = 10
09:49:04|<info> caseName:13 录像回放, groupName:13.1 录像回放_UDP, stepName:13.1.10 关闭媒体端口
sendMsg:
recvMsg:
09:49:04|<info> CATRunEngine::notifyStepResult errSteps = 11
09:49:04|<info> caseName:13 录像回放, groupName:13.2 录像回放_TCP, stepName:13.2.1 获取录像播放时间
sendMsg:
recvMsg:
09:49:04|<info> CATRunEngine::notifyStepResult errSteps = 12
09:49:04|<info> caseName:13 录像回放, groupName:13.2 录像回放_TCP, stepName:13.2.2 等待录像(all)
recvMsg:
sendMsg:
09:49:05|<info> CATRunEngine::notifyStepResult errSteps = 13
09:49:05|<info> caseName:13 录像回放, groupName:13.2 录像回放_TCP, stepName:13.2.3 打开媒体端口
sendMsg:
recvMsg:
09:49:05|<info> CATRunEngine::notifyStepResult errSteps = 14
09:49:05|<info> caseName:13 录像回放, groupName:13.2 录像回放_TCP, stepName:13.2.4 发送录像播放请求
sendMsg:
recvMsg:
09:49:05|<info> CATRunEngine::notifyStepResult errSteps = 15
09:49:05|<info> caseName:13 录像回放, groupName:13.2 录像回放_TCP, stepName:13.2.5 等待设备回复200OK
recvMsg:
sendMsg:
09:49:05|<info> CATRunEngine::notifyStepResult errSteps = 16
09:49:05|<info> caseName:13 录像回放, groupName:13.2 录像回放_TCP, stepName:13.2.6 发送ACK
sendMsg:
recvMsg:
09:49:05|<info> CATRunEngine::notifyStepResult errSteps = 17
09:49:05|<info> caseName:13 录像回放, groupName:13.2 录像回放_TCP, stepName:13.2.7 录像回放
sendMsg:
recvMsg:
09:49:05|<info> CATRunEngine::notifyStepResult errSteps = 18
09:49:05|<info> caseName:13 录像回放, groupName:13.2 录像回放_TCP, stepName:13.2.8 等待录像结束消息
recvMsg:
sendMsg:
09:49:05|<info> CATRunEngine::notifyStepResult errSteps = 19
09:49:05|<info> caseName:13 录像回放, groupName:13.2 录像回放_TCP, stepName:13.2.9 发送录像停止请求
sendMsg:
recvMsg:
09:49:05|<info> CATRunEngine::notifyStepResult errSteps = 20
09:49:05|<info> caseName:13 录像回放, groupName:13.2 录像回放_TCP, stepName:13.2.10 关闭媒体端口
sendMsg:
recvMsg:
09:49:05|<info> CATRunEngine::notifyStepResult errSteps = 21
09:49:05|<info> caseName:13 录像回放, groupName:13.3 录像慢放, stepName:13.3.1 获取录像播放时间
sendMsg:
recvMsg:
09:49:05|<info> CATRunEngine::notifyStepResult errSteps = 22
09:49:05|<info> caseName:13 录像回放, groupName:13.3 录像慢放, stepName:13.3.2 等待录像(all)
recvMsg:
sendMsg:
09:49:05|<info> CATRunEngine::notifyStepResult errSteps = 23
09:49:05|<info> caseName:13 录像回放, groupName:13.3 录像慢放, stepName:13.3.3 打开媒体端口
sendMsg:
recvMsg:
09:49:05|<info> CATRunEngine::notifyStepResult errSteps = 24
09:49:05|<info> caseName:13 录像回放, groupName:13.3 录像慢放, stepName:13.3.4 发送录像播放请求
sendMsg:
recvMsg:
09:49:05|<info> CATRunEngine::notifyStepResult errSteps = 25
09:49:05|<info> caseName:13 录像回放, groupName:13.3 录像慢放, stepName:13.3.5 等待设备回复200OK
recvMsg:
sendMsg:
09:49:05|<info> CATRunEngine::notifyStepResult errSteps = 26
09:49:05|<info> caseName:13 录像回放, groupName:13.3 录像慢放, stepName:13.3.6 发送ACK
sendMsg:
recvMsg:
09:49:05|<info> CATRunEngine::notifyStepResult errSteps = 27
09:49:05|<info> caseName:13 录像回放, groupName:13.3 录像慢放, stepName:13.3.7 录像回放
sendMsg:
recvMsg:
09:49:05|<info> CATRunEngine::notifyStepResult errSteps = 28
09:49:05|<info> caseName:13 录像回放, groupName:13.3 录像慢放, stepName:13.3.8 1/4速度播放
sendMsg:
recvMsg:
09:49:05|<info> CATRunEngine::notifyStepResult errSteps = 29
09:49:05|<info> caseName:13 录像回放, groupName:13.3 录像慢放, stepName:13.3.9 恢复正常播放
sendMsg:
recvMsg:
09:49:05|<info> CATRunEngine::notifyStepResult errSteps = 30
09:49:05|<info> caseName:13 录像回放, groupName:13.3 录像慢放, stepName:13.3.10 发送录像停止请求
sendMsg:
recvMsg:
09:49:05|<info> CATRunEngine::notifyStepResult errSteps = 31
09:49:05|<info> caseName:13 录像回放, groupName:13.3 录像慢放, stepName:13.3.11 关闭媒体端口
sendMsg:
recvMsg:
09:49:05|<info> CATRunEngine::notifyStepResult errSteps = 32
09:49:05|<info> caseName:13 录像回放, groupName:13.4 录像快放, stepName:13.4.1 获取录像播放时间
sendMsg:
recvMsg:
09:49:05|<info> CATRunEngine::notifyStepResult errSteps = 33
09:49:05|<info> caseName:13 录像回放, groupName:13.4 录像快放, stepName:13.4.2 等待录像(all)
recvMsg:
sendMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 34
09:49:06|<info> caseName:13 录像回放, groupName:13.4 录像快放, stepName:13.4.3 打开媒体端口
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 35
09:49:06|<info> caseName:13 录像回放, groupName:13.4 录像快放, stepName:13.4.4 发送录像播放请求
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 36
09:49:06|<info> caseName:13 录像回放, groupName:13.4 录像快放, stepName:13.4.5 等待设备回复200OK
recvMsg:
sendMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 37
09:49:06|<info> caseName:13 录像回放, groupName:13.4 录像快放, stepName:13.4.6 发送ACK
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 38
09:49:06|<info> caseName:13 录像回放, groupName:13.4 录像快放, stepName:13.4.7 录像回放
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 39
09:49:06|<info> caseName:13 录像回放, groupName:13.4 录像快放, stepName:13.4.8 4倍速播放
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 40
09:49:06|<info> caseName:13 录像回放, groupName:13.4 录像快放, stepName:13.4.9 恢复正常播放
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 41
09:49:06|<info> caseName:13 录像回放, groupName:13.4 录像快放, stepName:13.4.10 发送录像停止请求
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 42
09:49:06|<info> caseName:13 录像回放, groupName:13.4 录像快放, stepName:13.4.11 关闭媒体端口
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 43
09:49:06|<info> caseName:13 录像回放, groupName:13.5 录像暂停, stepName:13.5.1 获取录像播放时间
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 44
09:49:06|<info> caseName:13 录像回放, groupName:13.5 录像暂停, stepName:13.5.2 等待录像(all)
recvMsg:
sendMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 45
09:49:06|<info> caseName:13 录像回放, groupName:13.5 录像暂停, stepName:13.5.3 打开媒体端口
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 46
09:49:06|<info> caseName:13 录像回放, groupName:13.5 录像暂停, stepName:13.5.4 发送录像播放请求
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 47
09:49:06|<info> caseName:13 录像回放, groupName:13.5 录像暂停, stepName:13.5.5 等待设备回复200OK
recvMsg:
sendMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 48
09:49:06|<info> caseName:13 录像回放, groupName:13.5 录像暂停, stepName:13.5.6 发送ACK
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 49
09:49:06|<info> caseName:13 录像回放, groupName:13.5 录像暂停, stepName:13.5.7 录像回放
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 50
09:49:06|<info> caseName:13 录像回放, groupName:13.5 录像暂停, stepName:13.5.8 录像暂停
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 51
09:49:06|<info> caseName:13 录像回放, groupName:13.5 录像暂停, stepName:13.5.9 恢复正常播放
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 52
09:49:06|<info> caseName:13 录像回放, groupName:13.5 录像暂停, stepName:13.5.10 发送录像停止请求
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 53
09:49:06|<info> caseName:13 录像回放, groupName:13.5 录像暂停, stepName:13.5.11 关闭媒体端口
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 54
09:49:06|<info> caseName:13 录像回放, groupName:13.6 录像拖放, stepName:13.6.1 获取录像播放时间
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 55
09:49:06|<info> caseName:13 录像回放, groupName:13.6 录像拖放, stepName:13.6.2 等待录像(all)
recvMsg:
sendMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 56
09:49:06|<info> caseName:13 录像回放, groupName:13.6 录像拖放, stepName:13.6.3 打开媒体端口
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 57
09:49:06|<info> caseName:13 录像回放, groupName:13.6 录像拖放, stepName:13.6.4 发送录像播放请求
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 58
09:49:06|<info> caseName:13 录像回放, groupName:13.6 录像拖放, stepName:13.6.5 等待设备回复200OK
recvMsg:
sendMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 59
09:49:06|<info> caseName:13 录像回放, groupName:13.6 录像拖放, stepName:13.6.6 发送ACK
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 60
09:49:06|<info> caseName:13 录像回放, groupName:13.6 录像拖放, stepName:13.6.7 录像回放
sendMsg:
recvMsg:
09:49:06|<info> CATRunEngine::notifyStepResult errSteps = 61
09:49:06|<info> caseName:13 录像回放, groupName:13.6 录像拖放, stepName:13.6.8 录像拖动
sendMsg:
recvMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 62
09:49:07|<info> caseName:13 录像回放, groupName:13.6 录像拖放, stepName:13.6.9 发送录像停止请求
sendMsg:
recvMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 63
09:49:07|<info> caseName:13 录像回放, groupName:13.6 录像拖放, stepName:13.6.10 关闭媒体端口
sendMsg:
recvMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 1
09:49:07|<info> caseName:14 录像下载, groupName:14.1 录像下载_UDP, stepName:14.1.1 获取录像播放时间
sendMsg:
recvMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 2
09:49:07|<info> caseName:14 录像下载, groupName:14.1 录像下载_UDP, stepName:14.1.2 等待录像(all)
recvMsg:
sendMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 3
09:49:07|<info> caseName:14 录像下载, groupName:14.1 录像下载_UDP, stepName:14.1.3 切换到下载模式
sendMsg:
recvMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 4
09:49:07|<info> caseName:14 录像下载, groupName:14.1 录像下载_UDP, stepName:14.1.4 打开媒体端口
sendMsg:
recvMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 5
09:49:07|<info> caseName:14 录像下载, groupName:14.1 录像下载_UDP, stepName:14.1.5 发送录像下载请求
sendMsg:
recvMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 6
09:49:07|<info> caseName:14 录像下载, groupName:14.1 录像下载_UDP, stepName:14.1.6 等待设备回复200OK
recvMsg:
sendMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 7
09:49:07|<info> caseName:14 录像下载, groupName:14.1 录像下载_UDP, stepName:14.1.7 发送ACK
sendMsg:
recvMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 8
09:49:07|<info> caseName:14 录像下载, groupName:14.1 录像下载_UDP, stepName:14.1.8 录像下载
sendMsg:
recvMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 9
09:49:07|<info> caseName:14 录像下载, groupName:14.1 录像下载_UDP, stepName:14.1.9 等待录像结束
recvMsg:
sendMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 10
09:49:07|<info> caseName:14 录像下载, groupName:14.1 录像下载_UDP, stepName:14.1.10 停止下载
sendMsg:
recvMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 11
09:49:07|<info> caseName:14 录像下载, groupName:14.1 录像下载_UDP, stepName:14.1.11 关闭媒体端口
sendMsg:
recvMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 12
09:49:07|<info> caseName:14 录像下载, groupName:14.1 录像下载_UDP, stepName:14.1.12 切换到播放模式
sendMsg:
recvMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 13
09:49:07|<info> caseName:14 录像下载, groupName:14.2 录像下载_TCP, stepName:14.2.1 获取录像播放时间
sendMsg:
recvMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 14
09:49:07|<info> caseName:14 录像下载, groupName:14.2 录像下载_TCP, stepName:14.2.2 等待录像(all)
recvMsg:
sendMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 15
09:49:07|<info> caseName:14 录像下载, groupName:14.2 录像下载_TCP, stepName:14.2.3 切换到下载模式
sendMsg:
recvMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 16
09:49:07|<info> caseName:14 录像下载, groupName:14.2 录像下载_TCP, stepName:14.2.4 打开媒体端口
sendMsg:
recvMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 17
09:49:07|<info> caseName:14 录像下载, groupName:14.2 录像下载_TCP, stepName:14.2.5 发送录像下载请求
sendMsg:
recvMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 18
09:49:07|<info> caseName:14 录像下载, groupName:14.2 录像下载_TCP, stepName:14.2.6 等待设备回复200OK
recvMsg:
sendMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 19
09:49:07|<info> caseName:14 录像下载, groupName:14.2 录像下载_TCP, stepName:14.2.7 发送ACK
sendMsg:
recvMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 20
09:49:07|<info> caseName:14 录像下载, groupName:14.2 录像下载_TCP, stepName:14.2.8 录像下载
sendMsg:
recvMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 21
09:49:07|<info> caseName:14 录像下载, groupName:14.2 录像下载_TCP, stepName:14.2.9 等待录像结束
recvMsg:
sendMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 22
09:49:07|<info> caseName:14 录像下载, groupName:14.2 录像下载_TCP, stepName:14.2.10 停止下载
sendMsg:
recvMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 23
09:49:07|<info> caseName:14 录像下载, groupName:14.2 录像下载_TCP, stepName:14.2.11 关闭媒体端口
sendMsg:
recvMsg:
09:49:07|<info> CATRunEngine::notifyStepResult errSteps = 24
09:49:07|<info> caseName:14 录像下载, groupName:14.2 录像下载_TCP, stepName:14.2.12 切换到播放模式
sendMsg:
recvMsg:
09:49:08|<info> CATRunEngine::notifyStepResult errSteps = 1
09:49:08|<info> caseName:15 远程启动, groupName:15.1 远程启动, stepName:15.1.1 发送重启命令
sendMsg:
recvMsg:
09:49:08|<info> CATRunEngine::notifyStepResult errSteps = 2
09:49:08|<info> caseName:15 远程启动, groupName:15.1 远程启动, stepName:15.1.2 等待注销1
recvMsg:
sendMsg:
09:49:08|<info> CATRunEngine::notifyStepResult errSteps = 3
09:49:08|<info> caseName:15 远程启动, groupName:15.1 远程启动, stepName:15.1.3 等待注销2
recvMsg:
sendMsg:
09:49:08|<info> CATRunEngine::notifyStepResult errSteps = 4
09:49:08|<info> caseName:15 远程启动, groupName:15.1 远程启动, stepName:15.1.4 等待注册1
recvMsg:
sendMsg:
09:49:08|<info> CATRunEngine::notifyStepResult errSteps = 5
09:49:08|<info> caseName:15 远程启动, groupName:15.1 远程启动, stepName:15.1.5 等待注册2
recvMsg:
sendMsg:
09:49:08|<info> CATConnObjManager::stop 
09:49:08|<info> CATConnObj::stop capture(ID:3)
09:49:08|<info> CATConnObjManager::stop 
09:49:08|<info> CATRunEngine::stop 
09:49:08|<info> total case is 15, sucessed case is 0, failed case is 15,
                total step is 184, sucessed step is 7, failed step is 177
09:49:08|<info> CATCoreImp::stop 
09:49:09|<info> CATCoreImp::TestScene is end
09:50:05|<info> CATCoreImp::start 
