THE FOLLOWING PARAMS ARE GLOBAL - THEY HAVE THE SAME VALUE IN ALL LOADED DOCUMENTS, ALWAYS.

INTEGERS
======================================
1       0 for demo, 1 for CimLITE, 2 for CimPACK/CimCAD
2       Digitizer Output Format.  0=WinTab, 1..=Same as DOS (direct port read)
3       tablet datacom parameters: 0=COM1, 1=COM2, 2=COM3, 3=COM4
4          0=110, 1=150, 2=300, 3=600, 4=1200, 5=2400 6=4800, 7=9600
5          0=none, 1=odd, 3=even
6          data bits:  2=7, 3=8
7          stop bits:  0=1, 1=2
8       tablet: 0=none, 1=pointer, 2=digitizer
9       number of mouse buttons (0 if no mouse)
20      default attribute (line type)
21      autosave frequency
22      program: CimLITE/Simple=0, CimCAD=1, CimLITE/Dies=2, CimDIE=3, CimPACK=4
24      1 if lines can have Z values, else 0
25      1 = bridges, 2 = bridge positions, 4 = bridge ends, 8 = bridge spacing
37      1 for Japanese style pointage, 0 for normal pointage
38      maximum number of elements in a DDES file - if 0, no maximum
39      0 if subs start/end at origin, 1 if they omit first and last moves
40      number of decimals to use in fformat
41      default tuck position for MixMatch
52      Bridges : 0 = DDESII, 1-4 = default of special style
53      Bridges : 0 = ignore arcs, 1 = process them
54      Bridges : 0 = no line-line bridges, 1 = line-line bridges
55      Bleeds corners : 0 = either (bleeds) or sharp (cut adjust),
						 1 = always sharp, 2 = either, 3 = always round
61      Style of LPH, 0 = square, 1 = octagon, 2 = Elcede hexagon etc.
62      Style of reference name, 0 = full cut, 1 = etched
63      0 if Dieboard Edge tacks are to be used, 1 if not
64      style of L-L dim., 0 = regular, 1 = angled, 2 = unbroken arrow off. tex
67      default positioning of die in chase (0,1,2)
70      Style of Punch, 0 = round, 1 = octagon/10 sided
71      UNC sub calling for attr/point:
        0 = output in sub header + in main after sub call (safe)
        1 = switch to default state before sub call, and in sub before returning
        others = sub header only (old method, and dangerous)
72      0 for normal outside strip rules, 1 for hooks
73      method of edge treatment on stripping rules, ie 1 = past sheet
74      0 if CimPACK adds bridges to standards, 1 = no bridges (54=1 overrides)
75      Dieboard Edge : 0 if default to hash on dieboard edge, 1 if centerline, 2 if none
76      Dieboard Edge : 0 if uses a radius, 1 for a chamfer, 2 = neither
77      Rotary Bridging - teeth to skip at beginning
78      Rotary Bridging - bridge every nth tooth (ie 6)
79      Getvalues, 1 if no rounding on metric numbers
80      1 if arrows are to be filled
81      Number of decimals in linear dimensions
82      Number of decimals in angular dimensions
83      1 if construction menu does not repeat
84      1 if sketch menu does not repeat
85      1 if copy menu does not repeat
86      auto-refresh: 0 always, 1 never, 2 delete
87      FSB = 0 if prompted for offset each time, else 1
88      FSB = 0 if tackbridges used, 1 if not, 2 if ask each time
89      FSB = 0 if zoom up on windows, 1 if not
90      leadins: 0 = arc, 2 = straight/angle, 4 = corner. Add 1 for no leadout.
91      Stripping rules, direction of hook on left side (flat)
92      Stripping rules, direction of hook on right side (flat)
93      Stripping rules, direction of hook on back edge (flat)
94      Stripping rules, type of hook style used          
95      Female Stripper tack style, 0 = double, 1 = single, 2 = bridge
96      Easyset die holes, 0 = circles, 1 = "V"           
97      0 if no conversion on HPGL Import, 1 if asks to remap 

101     MSB : 1 if no bridges are placed on the rules created
102     Counters : 1 of solvent lines only use Tool3 (no Tool4)
103     Counters : option to specify a different tool number for the name
104     Counters : 1 if auto bridging is to be done on solvent lines
105     Counters : 1 if a local counter hole shape is to be used
106     Names : 1 if extra lines are centered instead of left side
108     1 to turn on parametrics automatically
112     End-to-End Dimension extensions (0 for short, 1 for extended to design)
113     1 to use par(1093) (which can be zero), 0 to use default (1/4", 6mm)
114     Counters - 1 if using Tool4 instead of Tool3 for solvent lines
115     Tackbridges - default style of tackbridge to use
        1 = double, 2 = single, 3 = bridge
119     Laser / Jig = 0 = Ask, 1 = Laser, 2 = Jig
121     Tackbridges : 1 forces same attribute as line for regular menu tacks
122     Imported subs: 0 = Ask, 1 = Internal, 2 = External
123     1 for PICK to add an initial prompt for a name, 2 to force typing
124     1 for auto-creation of X/Y axes in Construction/Lines/Sketch
125     Chase registration holes : 1 = Print Side, 2 = Die Side, 0 asks still
126     Balance Rules : 1 if added to the sides of the die also
131     0 draws only Straights, Arcs, Circles, Holes, Text inside a sub.
        1 draws Dimensions, 2 draws NC Text, 4 draws Points, 8 draws Dwells,
        16 draws Slews, 32 do NOT draw text, 64 draws Missing Sub Symbols
        (can be combined - e.g. 3 for NC Text and Dimensions).
132     date format: 0 = mm/dd/yy, 1 = dd/mm/yy, 2 = yy/mm/dd
135     Chase registration holes = 1 if gripper fingers flipper vertically
136     FSB / Guillotine - default pointage for outside edge only
        (Takes precedence over 3021 for these things)
137     MixMatch - 1 if not using slitlock radii
138     Counters - tool to use for cross on counter holes
139     Standards - 1 if the Blanksize macro is not to be run at the end
140     Stripping Rules - scrap style to use
141     Customer Specs - if customer specs are allowed
142     Standards / MM - 0 if want sizes shown, 1 if disabled
143     Layout - 1 if filenames shown when in layout menu only
144     Punches - 1 if base sizes are to be drawn for jig punches
145     1 if check dropouts is not to try to hide tack bridges
149     1 to disable Special and enable Tpc Tool
152     2 - always 2D, 3 - always 3D, 0 - Clear sets to 2D, Open matches file
153     1 if dashes are to be fixed size on paper, 0 if they scale with design
154     1 if parametric dims are fixed size, 2 if scaleable, 0 = scaleable
155     1 if files sort in reverse order for pick
156     Chaseholes - style of second pattern holes (0/1 same)
158     Dieboard Edge : if adding hanging pins to Center w/Grip style
159     Counters : 1 if want skiving after cutout (TOOL4 then TOOL5)
160     Counters : if don't want connections on skiving (TOOL5)
                   0 = old method (don't connect if Elcede)
                   1 = connect lines, 2 = don't connect
161     Counters : 1 if using end mill for counter holes
162     1 to ignore warnings about short move in UNC
163     Names : 1 if side name letters are rotated
165     1 to force tack bridges to be output using slot code (normally 2pt)
166     Dieboard Edge, 0 uses real tacks, 1 uses bridges instead
167     Layout order: 0/1 row/column, 0/2 zigzag/straight, 0/4/8/12 corner
168     Counters : 1 if bowties are to add tacks automatically
169     1 if UNC outputs zero length lines as #ON\X0Y0\#OFF instead of #ON\#OFF
170     File/Merge to retain section names: 0 ask, 1 yes, 2 no
171     1 to use dots instead of arrows for end-to-end linear dimensions
174     1 if DDES/CFF2 are exported without bridges
175     Number of line types to cycle through for hotkey R
176     default dash style for creases, perf (*16), and cut-crease (*256)
177     0 to plot Kanji as vectors, 1 to plot as characters, 2 to plot as octal
178     1 if hard-coded tackbridges are enabled
179     0 if Dieboard Edge uses one-sided tacks, 1 if uses double-sided
180     1 if don't add bridges to COMMON lines
181     Dieboard Edge - 1 if ignore stripping rules when sizing
182     Rotary Joints - 1 if disable "V"'s on joints
183     default options for Optimize (bit mask: 1=cw, 2=ccw, 4=sections, etc)
185     1 if buttons on digitizer start with 0, e.g. Calcomp
186     FSB - 1 if the support rails are just marked at each end with etch
187     Crosses - 1 if the crosses are to be etched
188     1 to disable automatic origin shift with negative skew
189     Punches - 1 if use 2 tacks instead of 1 on round punches
191     Dieboard Edge - 1 if put origin at 0 0 rather than -.014, -.014
192     attribute to use for leadins/leadouts (0 for same as line)
193     Striprules - 1 of ignore non-cutting lines when doing keep
194     Female Stripping Boards - 0 for circle (spacer pin), 1 = octagon
195     Attribute for dimension notes (text or text+arrow)
196     1 to supress default bridging on Trim/Keep/Intersect (see (28) on 9.10).
197     Folder Standards - 0 as is uses 9 for back panel, 9+1/64 front
                           1 uses 8+63/64 for back panel, 9 for front
198     Nicks - attribute to use (other than 24)
199     Rubber - 1 if start of line is to be split off as fake leadin
200     0 or 1 to force new section names to upper case, 2 for as typed
202     Handles : 0 if normal oval, 1 if using own shape
        uses \cimex\local\shapes\HANDLE.CIM otherwise  (flat)
        uses \cimex\local\shapes\RHANDLE.CIM otherwise (rotary)
203     Easyset : 1 if also pulling in blue holes
204     Female Stripping Board : 0 if use 3 holes on orange alignment jigs
											1 if use 4 holes
											2 if use no holes
                                 3 if use both 3 + 4 hole patterns
205     Default number of lines for Ellipse (0 = use 8)
206     1 if Dimensions Line-Line does not automatically start dragging
207     DTRLASER - pen number for Pen
208     DTRLASER - pen number for Pointer
209     DTRLASER - pen number for Etching
210     DTRLASER - pen number for Drill
211     FSB / MSB - 1 if using a local file for vacuum holes not SKETCH
        uses \cimex\local\shapes\VACUUM.CIM otherwise
212     Advanced Rotary Rule Types - 1 if allowed
214     MixMatch - 1 if printing bleeds added to glueflap
215     Suppress all beeps if 1
216     Advanced Rubber Rule Types - 1 if allowed
217     DXF dims: 0 = dim + con block, 1 = construction block only,
                  2 = dim + reg block, 3 = regular block (att 17), 4 = dim only
218     DT Rotary - 1 if large shell portion on front not back
219     Rubber - 1 if machine supports angled cutting
220     Dovetails - 1 if no tacks are added
221     Counters - 1 if bowties run right to the end of the cut
222     Attribute stored in Windows color chip
223     MSB - 1 if using menu of special pins
224     Simple Layout - 1 if lists out all the possible Simple L/O's
225     Counters - 1 of MULTISCO uses both crease channels, not just 1
226     Dashes - 1 turned on for screen display, 2 turned off
227     Dashes - 1 turned on for hardcopy device output, 2 turned off
228     1 to ignore ALL blank lines in DXF
        (normally ignores any except strings)
229     Rubber (flat) - 1 if adding radii to inside edges 
230     Rubber (flat) - default tab style number
231     Rubber (flat) - 1 if adding tabs
232     Rubber (flat) - 1 if adding text
233     Dieboard Edge - 1 if run handles & balance rules etc. at end
234     Stripping rules, direction of hook on left side  (rotary)
235     Stripping rules, direction of hook on right side (rotary)
236     Stripping rules, direction of hook on back edge  (rotary)
237     Stripping rules, direction of hook on lead edge  (rotary)
238     Balance rules - 1 if using fixed length rules
239     Balance rules - 1 if using fixed number of bridges
240     Balance rules - 1 if they go around the handles, not below
241     Left mouse snap preference - 0 = point, 1 = cursor
242     Samples - 1 if ask for bridges on matrix lines
243     Left mouse select preference - 0 = line, 1 = link
244     SelectTool - 0 use SM_CXDOUBLECLK, > 0 = use given value for x tolerance when deciding if this is a box select or click select
245     SelectTool - 0 use SM_CYDOUBLECLK, > 0 = use given value for y tolerance when deciding if this is a box select or click select
246     Runbys : 1 if hashmarks are added to the ends automatically
247     Dieboard Edge : 1 if the centerline hashmark is etched, not full cut
250     Layouts+Subs - 0 insert subroutines as external, 1 insert as internal
251     Section for copied lines - 0 = ask, 1 = same as original, 2 = current
252     tabs - 0 = edge straight, 1 = edge arc, 2 = corner
257     saving a file - 0 = print confirmation, 1 = omit
258     autosave depth (0 = 99)
260     duplicate default - 0 = move, 1 = copy
261     initial value for color chip ( par(222) ) - if 0, assume 1
262     scrollbars - 0 = on, 1 = off
263     FirstAid checks: 1=lengths 2=overlaps 4=gaps 8=rads 16=sections 1024=none
272     1 to supress pricing info in demo mode dialog
274     FSB's / Guillotines / Blankers - if automatic spacer pins added
275     Chaseholes : approximate number of holes to keep
276     Counters   : set to 1 if no "smart" snap on TOOL4 shape endpoints
                     set to 2 if yes, 0 assumed yes
277     0 unspecified computer, 1 on a network, 2 running locally
278     0 use regular MAC OPEN, 1 use custom macro
279     0 use regular MAC SAVE, 1 use custom macro
280     DT Rotary Laser #1, 0 = ask etch/draw, 1=draw all, 2=etch all
281     DT Rotary Laser #1, 0 = ask etch/draw, 1=draw all, 2=etch all
282     DT Rotary Laser #1, 0 = ask etch/draw, 1=draw all, 2=etch all
283     DXF Bender Output 0 if use Polylines, 1 of No Polylines
284     DXF Bender Output 0 if output in current units, 1 = inches, 2=metric
285     1 to omit version header on DXF export
286	    copy file locally when importing files (useful on NOVELL networks where I/O redirection can fail accross the network)
		  1 = smart copy (i.e. check if file is remote, and copy only if so)
		  2 = brute copy (i.e. don't bother checking, just always move to local folder)
287     Bender Output, 0 = DXF, 1 = CFF2, 2 = DDESII
288	    0 = default = 1 = autorepeat text insert, 2 = single text insert
289	    1 disables the parametrics pop-up notification window
290     No. of entries to save in the history list buffer (0 = default count)
291	    No. of files shown in the most recently used list in the file menu (0 = default count)
293     1 if Rule Quantities changed to 1 on each piece
295     Line Info lists bridges (0=no 1=yes)
296     Spacer Pins 1 if uses a local shape instead of CimPACK circles etc.
298     DTRLASER - 1 if prompt for deletion of existing files,
        0 will automatically overwrite
299     Re-Bridging : number of passes to use through the design
300     Forms (and print using form) confirms that default scale is OK:
          1 = show scale as decimals, 2 = show scale as fraction if >1
302     Rubber (flat) - if adding flattening breaks to rubber pieces
303     Rotary - 1 if default to not adding 3 point segments on output
304     DT Rotary - 1 if default to not moving up one hole as needed
305     Rubber breaks (flat) - 0 undefined, 1 match both,
        2 = match either length
306     "L" Hotkey - 1 if use a menu based version instead of dialog
307     Rubber (rotary) - 1 if adding radii to inside edges 
308     Rubber (rotary) - default tab style number
309     Rubber (rotary) - 1 if adding tabs
310     Rubber (rotary) - 1 if adding text
311     Rubber (rotary) - if adding flattening breaks to rubber pieces
312     Rubber breaks (rotary) - 0 undefined, 1 match both,
        2 = match either length
313     Select By Properties - 1 if use a menu version instead of dialog
314     FSB's / Guillotines / Blankers - if automatic tackbridges added
315     Rule Segments - 1 if remembered text is enabled
316     Rotary - 1 if use a wiggle profile as opposed to simple 3pt


REALS - UNITS DEPENDENT
======================================
1000    FUZZ (tolerance)
1002    tablet X corner
1003    tablet Y corner
1004    tolerance for printing out fractions
1005    default text size for parametric dimensions
1009    width of tabs
1010    length of tabs
1011    radius of loops
1012    hole center radius
1013    length of lead-ins
1014    size of tack bridges
1015    minimum length of arc in DDES file  (.003)
1016    default bridge width
1017    maximum radius of an arc in DDES file  (100)
1018    minimum chord deviation in DDES file   (.0001)
1019    default pointage
1020    standard sheet size in X (40)
1021    standard sheet size in Y (28)
1022    standard sheet gripper (1/2)
1023    standard left sheet margin (1/4)
1024    standard right sheet margin (1/4)
1025    standard top sheet margin (1/4)
1026    max number of inches of dieboard edge without a tackbridge (18)
1027    default tuck flap height used by MixMatch
1028    default glueflap width used by MixMatch
1034    bstyle 0..2 : length per bridge for 4+ bridges
1035    bstyle 0 : minimum length for 1 bridge
1036    bstyle 0 : minimum length for 2 bridges
1037    bstyle 0 : minimum length for 3 bridges
1038    bstyle 0 : minimum length for 4+ bridges
1039    bstyle 1 : minimum length for 1 bridge
1040    bstyle 1 : minimum length for 2 bridges
1041    bstyle 1 : minimum length for 3 bridges
1042    bstyle 1 : minimum length for 4+ bridges
1043    bstyle 2 : minimum length for 1 bridge
1044    bstyle 2 : minimum length for 2 bridges
1045    bstyle 2 : minimum length for 3 bridges
1046    bstyle 2 : minimum length for 4+ bridges
1047    bstyle 2 : bridge end distance
1048    bstyle 3 : minimum length for 1 bridge
1049    bstyle 3 : bridge spacing
1050    bstyle 3 : minimum amount of rule on the bridge-ends
1051    bstyle 4 : bridge end distance
1052    bstyle 4 : bridge spacing
1053    bstyle 4 : minimum amount of rule on the opposite end
1054    default X value used by SARN
1055    default Y value used by SARN
1057    default X value used by Chase Holes
1058    default Y value used by Chase Holes
1059    Stripping rules : hook size on outside strip rules   (flat)
1060    Stripping rules : hook radius on outside strip rules (flat)
1061    Stripping rules : end offset for stripping rules     (flat)
1062    Stripping rules : distance stripping rules go past sheet etc.
1063    Dieboard Edge : left wood
1064    Dieboard Edge : right wood
1065    Dieboard Edge : front wood
1066    Dieboard Edge : back wood
1067    Dieboard Edge : wood size in X
1068    Dieboard Edge : wood size in Y
1069    Dieboard Edge : radius to use
1070    Dieboard Edge : grip value to use
1071    Dieboard Edge : left / right offset to use
1072    Printing Blanket : Y stretch factor
1073    Printing Blanket : size in X
1074    Printing Blanket : size in Y
1075    Printing Blanket : gripper
1076    Rotary Bridging - bridge size in X
1077    Rotary Bridging - bridge size in Y
1078    Rotary Bridging - bridge spacing in X
1079    Rotary Bridging - bridge spacing in Y
1080    Rotary Bridging - tooth to tooth actual distance (ie .512)
1081    Stripping Boards - FSB Internal Offset
1082    Stripping Boards - FSB External Offset
1083    Chase Holes etc. - Final size to use for 6mm holes
1084    Chase Holes etc. - Final size to use for 9.5mm holes
1085    Stripping Boards - Inside diameter for spacer pin
1086    Stripping Boards - Outside diameter for spacer pin
1087    Stripping Boards - Default offset for gripper
1088    Laser - what to use for 2point slot compensation (ie. .028 beam)
1089    Laser - pwidth value used for lines expected to be 2 point
1090    Stripping rules - minimum line length to have bridges
1091    Rotary - joint setback amount
1092    Rotary - joint length
1093    Layout double cut default for X - see also par(113)
1094    Counters - default 3rd spindle width
1095    Counters - default 4th spindle width
1096    Counters - default 5th spindle width
1097    Counters - fixed distance for TW4 away from creases
1098    Punches - additional amount to subtract from the diameter for laser
1099    Pointage width (PWIDTH) to use for crease lines (Japan only)
1100    Stripping Boards - opening width for male blocks at tab area
1101    Stripping Boards - FSB Male Block offset
1102    Move origin when adding crosses: 0 ask first time, 1 ask, 2 no, 3 yes
1103    Handles - size in the X (flat)
1104    Handles - size in the Y (flat)
1105    Counters - size of counter hole cross
1106    Counters - default crease pullback for TOOL3
1107    Handles - amount of wood around handle (flat)
1108    FSB / Guillotine - default slot width for outside edges only
1109    Stripping Rules - scrap size in X
1110    Stripping Rules - scrap size in Y
1111    Stripping Rules - tilt amount for scrap edges
1112    Punches - amount to add to base sizes of jigged punches
1113    Crosses - default length for lines
1114    Crosses - default length for crosses
1115    Crosses - default offset from design edge
1119    Dieboard Edge : hanging pin diameter
1120    Dieboard Edge : hanging pin side offset
1121    Dieboard Edge : hanging pin top offset
1122    Names    : default height
1123    Printing Blankets : Border Size in X
1124    Printing Blankets : Border Size in Y
1125    Printing Blankets : Border Grip Value X
1126    High Tolerance Menu : Default runby length
1127    High Tolerance Menu : Default T-Knife length
1128    High Tolerance Menu : Default airtrack width
1129    Punches : size of smallest punch to be tacked in
1130    Punches : default wall thickness for plugs
1131    Stripping Boards : default CL Notch hole size
1133    Dieboard Edge - amount to use for dieboard edge laser beam only
1134    Text - forces text in dimensions to always be this size
1135    Rubber - minimum length of 1st line to split off
1136    Rubber - amount of 1st line to split off
1137    Bleeds - default offset to use
1138    FSB - default wood offset for edges
1139    FSB - default block width for edges
1140    MSB - default wood offset for edges
1141    Ratio of linear dimension short extension to text size (default 1:1)
1142    Ratio of linear dimension long extension to text size (default 1:1)
1143    Ratio of linear dimension long extension pull-back to text size (default 1:1)
1144    Chase Holes etc. - Final size to use for 10mm holes
1145    Rotary - bolt step to use for Ward 50 inch (1st menu page)
1146    Rotary - bolt step to use for generic 66 inch (1st menu page)
1147    Rotary - bolt step to use for generic 52 inch (2nd menu page)
1148    Rotary - bolt step to use for generic 86 inch (2nd menu page)
1149    FSB - diameter to use for red dog holes
1150    Data Tech - default size for text
1151    Data Tech - default shell size for 33 inch half shell
1152    Rubber (flat) - spacing between tabs
1153    Rubber (flat) - offset from top of rubber to edge of knife
1154    Rubber (flat) - offset from base of rubber to edge of crease
1155    Rubber (flat) - offset from base of rubber to edge of perf
1156    Rubber (flat) - offset from base of rubber to edge of knife
1157    Rubber (flat) - width at base
1158    Rubber (flat) - maximum amount to follow a crease
1159    Rubber (flat) - default height for numbers
1160    Rubber (flat) - minimum inside radius to add
1161    Minimum distance allowed by POINT and CLOSEST functions
1162    Nicks - length of nicks
1163    Nicks - nick end amount
1164    Nicks - gap between nicks
1165    Nicks - gap between double sets of nicks
1166    Rotary - default wood thickness
1167    Rotary - value to switch from partial to full shell, e.g. 19 inches
1168    Dieboard Edge - front to back dimension (for sides option)
1169    Dieboard Edge - wood on sides
1170    Handles - size in the X (rotary)
1171    Handles - size in the Y (rotary)
1172    Handles - amount of wood around handle (rotary)
1173    Handles - shell width to switch to 3 handles (rotary)
1174    Handles - shell width to switch to 4 handles (rotary)
1175    Stripping rules : hook size on outside strip rules   (rotary)
1176    Stripping rules : hook radius on outside strip rules (rotary)
1177    Stripping rules : end offset for stripping rules     (rotary)
1178    Stripping rules : spacing between stripping rules
1179    Stripping rules : length of spaced rules
1180    Balance rules - length of fixed segments
1181    FSB - amount to shorten wooden support rails on front
1182    FSB - amount to shorten wooden support rails on rear
1183    Handles - amount to avoid balance rules by
1184    Layout double cut default for Y - see also par(113)
1185    FSB - default size of orange jigs
1186    Grid size (for view options)
1187    Folders - default glueflap taper
1188    Folders - default pocket height
1189    Folders - default glueflap width
1190    Stripping Rules - Spaced rules taper amount
1191    FirstAid - maximum gap size
1192    FirstAid - maximum radius
1193    FirstAid - mimimum length
1194    CD's - default glueflap width
1195    CD's - default front panel offset
1196    Stripping Boards - approximate tackbridge spacing on long lines
1197    Stripping Boards - approximate spacing between spacer pins
1198    Rack Hanging Pins - distance to switch to 3 pins
1199    Blankers - default female offset
1200    Blankers - default male offset
1201    Blankers - default steel support plate offset
1202    Blankers - default vacuum hole offset
1203    Dieboard Edge - minimum size allowed front to back (Y)
1204    Dieboard Edge - maximum size allowed front to back (Y)
1205    Dieboard Edge - minimum size allowed left to right (X)
1206    Dieboard Edge - maximum size allowed left to right (X)
1207    Re-Bridging : lower end of bridge range to check
1208    Re-Bridging : higher end of bridge range to check
1209    Re-Bridging : expected bridge size to look for
1210    FirstAid - overlap tolerance
1211    FirstAid - overlap minimum length of new lines
1212    Rubber (flat) - default size of break to add
1213    Rubber (flat) - amount of material to leave on flattening V's
1214    Rubber (flat) - minimum line length surrounding a flattening break
1215    Rotary - amount of line to split off seam for 3pt segments
1216    Rotary - width of laser beam for trimming shell edges (.017)
1217    Rubber (flat) - maximum radius length for breaks
1218    Rubber (rotary) - spacing between tabs
1219    Rubber (rotary) - offset from top of rubber to edge of knife
1220    Rubber (rotary) - offset from base of rubber to edge of crease
1221    Rubber (rotary) - offset from base of rubber to edge of perf
1222    Rubber (rotary) - offset from base of rubber to edge of knife
1223    Rubber (rotary) - width at base
1224    Rubber (rotary) - maximum amount to follow a crease
1225    Rubber (rotary) - default height for numbers
1226    Rubber (rotary) - minimum inside radius to add
1227    Rubber (rotary) - default size of break to add
1228    Rubber (rotary) - amount of material to leave on flattening V's
1229    Rubber (rotary) - minimum line length surrounding a flattening break
1230    Rubber (rotary) - maximum radius length for breaks
1231    Rubber (rotary) - width of the slot wave
1232    Rubber (rotary) - pitch of the slot rubber
1233    Rubber (rotary) - amount to chop back the trail edge
1234    Rubber (flat) - width of the slot wave
1235    Rubber (flat) - pitch of the slot rubber
1236    Rubber - sheet size in X
1237    Rubber - sheet size in Y
1238    Rubber - sheet margin on outside edge
1239    Rotary - width of the tightening wiggle
1240    Rotary - pitch of the tightening wiggle


STRINGS
======================================
2001    digitizer initialization
2014    default text for Sample Labels, ie CAD Carton Design by Cimex
2019    default (start-up) directory
2020    country
2021    prefix and suffix for radius
2022    prefix and suffix for diameter
2023    prefix and suffix for degrees
2026    Rotary : default directory to merge files from
2027    Corrugated MixMatch : String of allowances for panel # 1
2028    Corrugated MixMatch : String of allowances for panel # 2
2029    Corrugated MixMatch : String of allowances for panel # 3
2030    Corrugated MixMatch : String of allowances for panel # 4
2031    Counters : string for calculation of &TW1
2032    Counters : string for calculation of &TW2
2033    Default directory for import  !NO LONGER USED!
2034    Plotter config file name for hotkey form plot
2035    Form file name for hotkey form plot
2036    Dieboard Edge - default filename to pull in for a logo
2037    Top directory for customer specs
2038    Sent to a DOS Shell command when switching to a new hardcopy device
2039    Default directory for export  !NO LONGER USED!
2040    Default directory for merge/include  !NO LONGER USED!
2042    Default file extension for .CIM files other than CIM
2043    Plotter name for hotkey print screen
2044    Digitizer buttons
2045    List of directories to search when a filename is typed
2046    Text editor to use for Notes (default = "cimedit /numbers=no")
2047    Top directory for Advanced Rotary Rule Types
2048    Top directory for Advanced Rubber Rule Types
2049    Dieboard Edge - default formula for LRTB Grip calculation
2050    Dieboard Edge - default formula for Gripctr w / Grip calculation
2051    MSB - menu name for custom pin #1
2052    MSB - menu name for custom pin #2
2053    MSB - menu name for custom pin #3
2054    MSB - menu name for custom pin #4
2055    MSB - menu name for custom pin #5
2056    MSB - menu name for custom pin #6
2057    MSB - menu name for custom pin #7
2058    MSB - menu name for custom pin #8
2059    MSB - menu name for custom pin #9
2060    MSB - menu name for custom pin #10
2066    Sideup Menu - text for F1 (Print Side)
2067    Sideup Menu - text for F2 (Die Side)
2068    DT Rotary - default drive / directory for files (Laser #1)
2069    "GET" string to use from menus for picking a style
         e.g. GET for DOS, or GET DOUBLE for Windows
2071    Default screen map
2076    Override: "magic" hardcopy plotting macro (for custom macros that don't go through the normal plot logic)
2077    Override: plotter to load (i.e. don't show dialog, just load this)
2078    Override: samplemaker to load (i.e. don't show dialog, just load this)
2082    ODBC Data Source Name
2083    Name of the printer to use for Sample Labels
2084    Face name for dimensions (defaults to "Courier New")
2086    Rule Segments Output : Default Folder to save files to
2087    DXF Bender Output : Default Folder to save files to
2088    Argument string for TRANSMIT when CimLite is to be used as an HPGL front-end (e.g. COM2:19200,8,N,1 echo)
2089    Rubber - folder to output waterjet files to
2090    DT Rotary - default drive / directory for files (Laser #2)
2091    DT Rotary - default drive / directory for files (Laser #3)
2092    Format line for generating CFF2 autoprint statement (can be used to do anything via shell command) (e.g. notepad.exe /p %s)
2103    Flat (Layout Options Menu) : default directory to merge files from


REALS - INDEPENDENT OF UNITS
======================================
3001    tablet scale
3002    mouse speed
3006    minimum subtended angle of arcs in DDES file (.5)
3007    current pointage being used, 0 same as 2
3019    pointage to use for the lasercut names, 0 assumed as 2
3020    pointage to use for the dieboard edge, 0 assumed to be 2   
3021    pointage for chase holes, punches, handles, FSB, MSB etc.
3022    Stripping rules : angle of hook in degrees
3023    Counters : Angle of the skive tool
3024    Counters : Angle of the cutout tool
3025    Bridge Menu - (width1 / F9)  default bridge width Imperial
3026    Bridge Menu - (width2 / F10) default bridge width Imperial
3027    Bridge Menu - (width3 / F11) default bridge width Imperial
3028    SARN Drawing - stretch factor to use in Y axis (0 same as 1)
3029    Max percentage of line which can be used for bridges (def 100%)
3030    angle of straight lead-ins (90 is perpendicular)
3031    Bridge Menu - (width1 / F9)  default bridge width Metric
3032    Bridge Menu - (width2 / F10) default bridge width Metric
3033    Bridge Menu - (width3 / F11) default bridge width Metric
3035    Animate speed, if non-zero (.5 means 1/2 the default speed)
3036    Balance rules - fixed number of bridges on fixed length segments
3037    Bridge Menu - (width4) default bridge width Imperial
3038    Bridge Menu - (width5) default bridge width Imperial
3039    Bridge Menu - (width6) default bridge width Imperial
3040    Bridge Menu - (width7) default bridge width Imperial
3041    Bridge Menu - (width8) default bridge width Imperial
3042    Bridge Menu - (width9) default bridge width Imperial
3043    Bridge Menu - (width4) default bridge width Metric
3044    Bridge Menu - (width5) default bridge width Metric
3045    Bridge Menu - (width6) default bridge width Metric
3046    Bridge Menu - (width7) default bridge width Metric
3047    Bridge Menu - (width8) default bridge width Metric
3048    Bridge Menu - (width9) default bridge width Metric
3049    Timer delay (in seconds) for right mouse pop-ups
3050    Default view flags (can be too large for an int)
3053    Program version number that ran most recently
3055    autosave interval (0.0 = 1.0 min.)
3056    position of circle lead-ins, less 90 (i.e. 0 positions at 90)
3057	  Default Dimension Color (2-byte RGB)
3058    Default Dimension BIUM
3059    Rubber (flat) - minimum angle change to use flattening break up at
3060    Rubber (rotary) - minimum angle change to use flattening break up at
