* PARAMS.TXT parameter documentation file
* Version W10.3.0.0 09/27/02
*
* Current ranges -
*
*    Integers - 0..500
*    Unit Dependent Reals - 1000..1500
*    Strings (maximum of 500 characters) - 2000..2150
*    Unit Independent Reals - 3000..3100


INTEGERS  (0..500)
========
0       1 if any parameters have been updated
1       0 for demo, 1 for CimLITE, 2 for CimPACK/CimCAD
2       Digitizer Output Format.  0=WinTab, 1+ =Same as DOS (direct port read)
3       tablet datacom parameters: 0=COM1, 1=COM2, 2=COM3, 3=COM4
4          bit rate:   0=110, 1=150, 2=300, 3=600, 4=1200, 5=2400 6=4800, 7=9600
5          parity:     0=none, 1=odd, 3=even
6          data bits:  2=7, 3=8
7          stop bits:  0=1, 1=2
8       tablet: 0=none, 1=pointer, 2=digitizer
9       number of mouse buttons (0 if no mouse)
10      hardcopy device port:           0=COM1, 1=COM2, 2=COM3, 3=COM4, 11=LPT1, 12=LPT2, 13=LPT3
11      hardcopy device baud:           0=110, 1=150, 2=300, 3=600, 4=1200, 5=2400 6=4800, 7=9600
12      hardcopy device parity:         0=none, 1=odd, 3=even
13      hardcopy device data bits:  2=7, 3=8
14      hardcopy device stop bits:  0=1, 1=2
15      hardcopy device driver:
                        HCD_HPGL                1
                        HCD_DATA_TECH_IPC       2       // aka IPC
                        HCD_HOUSTON             3   // aka DMP
                        HCD_DALE                4
                        HCD_WILD                5
                        HCD_GPGL                6
                        HCD_MAX                 7
                        HCD_PRINTGLD            8  // not used in Windows product
                        HCD_SPEEDPLOT           9
                        HCD_ELCEDE_VECTOCUT    10
                        HCD_ELCEDE_IBH         11
                        HCD_ELCEDE_IBH_SUBS    12
                        HCD_GCODE              13
                        HCD_GCODE_SUBS         14
                        HCD_WINDOWS           255
16      hardcopy device arc support: 0 no support, 1 supports arcs and circles, 2 for arcs but not circles
17      hardcopy device handshaking: 0 = xon/xoff, 1 = software, 2 = CTS, 3 = DSR
18      plot justification
19      plot speed
20      default attribute (line type)
21      autosave frequency
22      program: CimLITE/Simple=0, CimCAD=1, CimLITE/Dies=2, CimDIE=3, CimPACK=4
23      plotted text justification: 0 = always lower left, 1 = various
24      1 if lines can have Z values, else 0
25      1 = bridges, 2 = bridge positions, 4 = bridge ends, 8 = bridge spacing
26      Samples : If want nicks option (1 = Yes, 2 = No)
27      Samples : If want inside lines first (1 = Yes, 2 = No)
28      Samples : If want reverse lines option (1 = Yes, 2 = No)
29      Samples : If want doublecut option (1 = Yes, 2 = No)
30      Samples : Matrix Option, (1-10), 0 = Ask
31      Samples : If want vacuum holes option (1 = Yes, 2 = No)
32      Samples : If want layout option (1 = Yes, 2 = No, 3 = Ask)
33      Samples : 0 if running directly, 1 if default to file
34      Samples : reserved for future use
35      Samples : if printside or dieside (1 = PS, 2 = DS, 3 = Ask)
36      Samples : If want delete any lines option (1 = Yes, 2 = No)
37      1 for Japanese style pointage, 0 for normal pointage
38      maximum number of elements in a DDES file - if 0, no maximum
39      0 if subs start/end at origin, 1 if they omit first and last moves
40      number of decimals to use in fformat
41      default tuck position for MixMatch
42      NA (was: hardcopy device is Speedplot)
43      Plotters :  which side up the plot is, As Shown / Flipped, 1,2 or 0
44      Plotters :  X accuracy scale to use, 1 = default
45      Plotters :  Y accuracy scale to use, 1 = default
46      Plotters :  plotting speed to use,   1 = default
47      Plotters :  # of pens to use, 1-12
48      Plotters :  Paper size to use, 1-36
49      Plotters :  If the Bridges are to plot, YES = 1, NO = 2
50      Plotters :  If the hardcopy device is to be run Directly, YES = 1, NO = 2
51      Plotters :  If all lines are to be plotted, or to prompt 1 = ALL
52      Bridges : 0 = DDESII, 1-4 = default of special style
53      Bridges : 0 = ignore arcs, 1 = process them
54      Bridges : 0 = no line-line bridges, 1 = line-line bridges
55      Bleeds corners : 0 = either (bleeds) or sharp (cut adjust),
                         1 = always sharp, 2 = either, 3 = always round
56-60   Distributor parameters
61      Style of LPH, 0 = square, 1 = octagon, 2 = Elcede hexagon etc.
62      Style of reference name, 0 = full cut, 1 = etched
63      0 if Dieboard Edge tacks are to be used, 1 if not
64      style of L-L dim., 0 = regular, 1 = angled, 2 = unbroken arrow off. tex
65      1 if hardcopy device does not attempt to get P1/P2
66      1 if hardcopy device pen changes are to be ignored (omit SP1 etc.)
67      default positioning of die in chase (0,1,2)
68      0 if plots direct to com port (3F8), 1 if plots to file ("COM1")
69      1 or 2 for Mimaki origin fix (new machines, 1 = lower left, 2 = center)
70      Style of Punch, 0 = round, 1 = octagon/10 sided
71      UNC sub calling for attr/point:
        0 = output in sub header + in main after sub call (safe)
        1 = switch to default state before sub call, and in sub before returning
        others = sub header only (old method, and dangerous)
72      0 for normal outside strip rules, 1 for hooks (flat)
73      method of edge treatment on stripping rules, ie 1 = past sheet
74      0 if CimPACK adds bridges to standards, 1 = no bridges (54=1 overrides)
75      Dieboard Edge : 0 if default to hashmark only on dieboard edge
        1 = centerline notch, 2 = neither, 3 = both
76      Dieboard Edge : 0 if uses a radius, 1 for a chamfer, 2 = neither
77      Rotary Bridging - teeth to skip at beginning
78      Rotary Bridging - bridge every nth tooth (ie 6)
79      Getvalues, 1 if no rounding on metric numbers
80      0 or 1 if arrows are to be filled on printer/screen, 2 if not filled
81      Number of decimals in linear dimensions
82      Number of decimals in angular dimensions
83      1 if construction menu does not repeat
84      1 if sketch menu does not repeat
85      1 if copy menu does not repeat
86      auto-refresh: 0 always, 1 never, 2 delete
87      FSB = 0 if prompted for offset each time, else 1
88      FSB = 0 if tackbridges used, 1 if not, 2 if ask each time
89      FSB = 0 if zoom up on windows, 1 if not
90      leadins: 0 = arc, 2 = straight/angle, 4 = corner. Add 1 for no leadout.
91      Stripping rules, direction of hook on left side (flat)
92      Stripping rules, direction of hook on right side (flat)
93      Stripping rules, direction of hook on back edge (flat)
94      Stripping rules, type of hook style used (flat)
95      Female Stripper tack style, 0 = double, 1 = single, 2 = bridge
96      Easyset die holes, 0 = circles, 1 = "V"           
97      0 if no conversion on HPGL Import, 1 if asks to remap 
98      1 for a hardcopy device with the origin in the center (typical for a drum)
99      Used as a temp by BLEEDS and others - always reset to 0 after use
100     Plotters : 0 for laser or PrintGL/D to fill page, 1 if scale 1 desired
101     MSB : 1 if no bridges are placed on the rules created
102     Counters : 1 of solvent lines only use Tool3 (no Tool4)
103     Counters : option to specify a different tool number for the name
104     Counters : 1 if auto bridging is to be done on solvent lines
105     Counters : 1 if a local counter hole shape is to be used
106     Names : 1 if extra lines are centered instead of left side
107 ** No longer needed       0/1 don't use hotkey and macro speed-up features, 2 do use them (faster)
108     1 to turn on parametrics automatically
109     Mimaki : 1 if the partial cuts go to the swivel blade
110 ** No longer needed   Common Knife : 1 if prompt for filename on .K files
111 ** No longer needed   Common Knife : 1 if subroutines are to be always saved
112     End-to-End Dimension extensions (0 for short, 1 for extended to design)
113     1 to use par(1093) (which can be zero), 0 to use default (1/4", 6mm)
114     Counters - 1 if using Tool4 instead of Tool3 for solvent lines
115     Tackbridges - default style of tackbridge to use
        1 = double, 2 = single, 3 = bridge
116 ** No longer needed   Max screen res for Alt-F (0=1024x768, 1 = 800x600, 2=640x480)
117 ** No longer needed   1 to ask for Plot Options menu, 2 to skip this
118     Graphtec : 1 if the partial cuts go to a second blade
119     Laser / Jig = 0 = Ask, 1 = Laser, 2 = Jig
120     Samples : If want option to combine creases (1 = Yes, 2 = No)
121     Tackbridges : 1 forces same attribute as line for regular menu tacks
122     Imported subs: 0 = Ask, 1 = Internal, 2 = External
123 ** No longer needed (see 2045)    1 for PICK to add an initial prompt for a name, 2 to force typing
124     1 for auto-creation of X/Y axes in Construction/Lines/Sketch
125     Chase registration holes : 1 = Print Side, 2 = Die Side, 0 asks still
126     Balance Rules : 1 if added to the sides of the die also
127 ** No longer needed   1 if prompts default to overstrike, 0 if they default to insert
128     SARN Drawing :  1 if all lines are to be plotted
129     Counters : Number of tools supported by the machine
130     Samples : 1 if the perf shortening is just done automatically
131     0 draws only Straights, Arcs, Circles, Holes, Text inside a sub.
        1 draws Dimensions, 2 draws NC Text, 4 draws Points, 8 draws Dwells,
        16 draws Slews, 32 do NOT draw text, 64 draws Missing Sub Symbols
        (can be combined - e.g. 3 for NC Text and Dimensions).
132     date format: 0 = mm/dd/yy, 1 = dd/mm/yy, 2 = yy/mm/dd
133 ** No longer needed    Clear before any import. 1 = clear, 2 = don't clear, 0 = ask.
134 ** No longer needed    Full Size plot position: 0 = always lower left, 1 = from setup menu
135     Chase registration holes = 1 if gripper fingers flipper vertically
136     FSB / Guillotine - default pointage for outside edge only
        (Takes precedence over 3021 for these things)
137     MixMatch - 1 if not using slitlock radii
138     Counters - tool to use for cross on counter holes
139     Standards - 1 if the Blanksize macro is not to be run at the end
140     Stripping Rules - scrap style to use
141     Customer Specs - if customer specs are allowed
142     Standards / MM - 0 if want sizes shown, 1 if disabled
143     Layout - 1 if filenames shown when in layout menu only
144     Punches - 1 if base sizes are to be drawn for jig punches
145     1 if check dropouts is not to try to hide tack bridges
146 ** No longer needed    1 if check dropouts is to automatically switch to full screen (Alt-F)
147 ** No longer needed    1 if Save/New and Alt-N are NOT to unget the current name
148 ** No longer needed    1/2 = &DB vars, 3/4 = &DB vars and database, 1/3 = only after Alt-I
149     1 to disable Special and enable Tpc Tool
150     1 for plots and samples to prompt for a hardcopy device origin offset
151     Graphtec : 1 if Dipswitch #7 is turned on so pens (1 1 2 2)
152     2 - always 2D, 3 - always 3D, 0 - Clear sets to 2D, Open matches file
153     1 if dashes are to be fixed size on paper, 0 if they scale with design
154     1 if parametric dims are fixed size, 2 if scaleable, 0 = scaleable
155     1 if files sort in reverse order for pick
156     Chaseholes - style of second pattern holes (0/1 same)
157     Samples : If want all the creases shortened (1 = Yes, 2 = No)
158     Dieboard Edge : if adding hanging pins to Center w/Grip style
159     Counters : 1 if want skiving after cutout (TOOL4 then TOOL5)
160     Counters : if don't want connections on skiving (TOOL5)
                   0 = old method (don't connect if Elcede)
                   1 = connect lines, 2 = don't connect
161     Counters : 1 if using end mill for counter holes
162     1 to ignore warnings about short move in UNC
163     Names : 1 if side name letters are rotated
164     Auto-review on open: 0 page up/down following space, 1 always, 2 never
165     1 to force tack bridges to be output using slot code (normally 2pt)
166     Dieboard Edge, 0 uses real tacks, 1 uses bridges instead
167     Layout order: 0/1 row/column, 0/2 zigzag/straight, 0/4/8/12 corner
168     Counters : 1 if bowties are to add tacks automatically
169     1 if UNC outputs zero length lines as #ON\X0Y0\#OFF instead of #ON\#OFF
170     File/Merge to retain section names: 0 ask, 1 yes, 2 no
171     1 to use dots instead of arrows for end-to-end linear dimensions
172 ** No Longer Used    1 to hide the File/Delete menu
173     Plotters - 1 if the machine has programmable Z-heights
174     1 if DDES/CFF2 are exported without bridges
175     Number of line types to cycle through for hotkey R
176     default dash style for creases, perf (*16), and cut-crease (*256)
177     2 to plot extended characters as octal
178     1 if hard-coded tackbridges are enabled
179     0 if Dieboard Edge uses one-sided tacks, 1 if uses double-sided
180     1 if don't add bridges to COMMON lines
181     Dieboard Edge - 1 if ignore stripping rules when sizing
182     Rotary Joints - 1 if disable "V"'s on joints
183     default options for Optimize (bit mask: 1=cw, 2=ccw, 4=sections, etc)
184 ** No Longer Used    1 if CONFIRM button is moved down the menu (not underneath CLEAR)
185     1 if buttons on digitizer start with 0, e.g. Calcomp
186     FSB - 1 if the support rails are just marked at each end with etch
187     Crosses - 1 if the crosses are to be etched
188     1 to disable automatic origin shift with negative skew
189     Punches - 1 if use 2 tacks instead of 1 on round punches
190     Plotters - 1 if add filename comment to Data Tech HPGL files
191     Dieboard Edge - 1 if put origin at 0 0 rather than -.014, -.014
192     attribute to use for leadins/leadouts (0 for same as line)
193     Striprules - 1 of ignore non-cutting lines when doing keep
194     Female Stripping Boards - 0 for circle (spacer pin), 1 = octagon
195     Attribute for dimension notes (text or text+arrow)
196     1 to supress default bridging on Trim/Keep/Intersect (see (28) on 9.10).
197     Folder Standards - 0 as is uses 9 for back panel, 9+1/64 front
                           1 uses 8+63/64 for back panel, 9 for front
198     Nicks - attribute to use (other than 24)
199     Rubber - 1 if start of line is to be split off as fake leadin
200     0 or 1 to force new section names to upper case, 2 for as typed
201     Plotting Text : 1 if hardcopy device supports text,
                        0 if 'DIM' and 'TEXT' not output by CIMCAD.EXE
202     Handles : 0 if normal oval, 1 if using own shape
        uses \cimex\local\shapes\HANDLE.CIM otherwise  (flat)
        uses \cimex\local\shapes\RHANDLE.CIM otherwise (rotary)
203     Easyset : 1 if also pulling in blue holes
204     Female Stripping Board : 0 if use 3 holes on orange alignment jigs
                                 1 if use 4 holes
                                 2 if use no holes
                                 3 if use both 3 + 4 hole patterns
205     Default number of lines for Ellipse (0 = use 8)
206     1 if Dimensions Line-Line does not automatically start dragging
207     DTRLASER - pen number for Pen
208     DTRLASER - pen number for Pointer
209     DTRLASER - pen number for Etching
210     DTRLASER - pen number for Drill
211     FSB / MSB - 1 if using a local file for vacuum holes not SKETCH
        uses \cimex\local\shapes\VACUUM.CIM otherwise
212     Advanced Rotary Rule Types - 1 if allowed
213     Samples - 1 to optimize sample (all except matrix)
214     MixMatch - 1 if printing bleeds added to glueflap
215     Suppress all beeps if 1
216     Advanced Rubber Rule Types - 1 if allowed
217     DXF dims: 0 = dim + con block, 1 = construction block only,
                  2 = dim + reg block, 3 = regular block (att 17), 4 = dim only
218     DT Rotary - 1 if large shell portion on front not back
219     Rubber - 1 if machine supports angled cutting
220     Dovetails - 1 if no tacks are added
221     Counters - 1 if bowties run right to the end of the cut
222     Attribute stored in Windows color chip
223     MSB - 1 if using menu of special pins
224  ** no longer used 09/27/02
225     Counters - 1 of MULTISCO uses both crease channels, not just 1
226     Dashes - 1 turned on for screen display, 2 turned off
227     Dashes - 1 turned on for hardcopy device output, 2 turned off
228     1 to ignore ALL blank lines in DXF
        (normally ignores any except strings)
229     Rubber (flat) - 1 if adding radii to inside edges 
230     Rubber (flat) - default tab style number
231     Rubber (flat) - 1 if adding tabs
232     Rubber (flat) - 1 if adding text
233     Dieboard Edge - 1 if run handles & balance rules etc. at end
234     Stripping rules, direction of hook on left side  (rotary)
235     Stripping rules, direction of hook on right side (rotary)
236     Stripping rules, direction of hook on back edge  (rotary)
237     Stripping rules, direction of hook on lead edge  (rotary)
238     Balance rules - 1 if using fixed length rules
239     Balance rules - 1 if using fixed number of bridges
240     Balance rules - 1 if they go around the handles, not below
241     Left mouse snap preference - 0 = point, 1 = cursor
242     Samples - 1 if ask for bridges on matrix lines
243     Left mouse select preference - 0 = line, 1 = link
244     SelectTool - 0 use SM_CXDOUBLECLK, > 0 = use given value for x tolerance when deciding if this is a box select or click select
245     SelectTool - 0 use SM_CYDOUBLECLK, > 0 = use given value for y tolerance when deciding if this is a box select or click select
246     Runbys : 1 if hashmarks are added to the ends automatically
247     Dieboard Edge : 1 if the centerline hashmark is etched, not full cut
248     Resize pen hardcopy device text to match width of screen fonts
249     Current Logical hardcopy device - plot relative to (0 = center, 1 = origin, 2 = lower left, 3 = lower right, 4 = upper left, 5 upper right, 
           6 = left center, 7 = right center, 8 = top center, 9 = bottom center)
250     Layouts+Subs - 0 insert subroutines as external, 1 insert as internal
251     Section for copied lines - 0 = ask, 1 = same as original, 2 = current
252     tabs - 0 = edge straight, 1 = edge arc, 2 = corner
253     current hardcopy map is configured for 1 = plotter, 2 = samplemaker (0 = not known)
254     currently loaded hardcopy device type (0 nothing loaded, 1 printer, 2 plotter, 3 samplemaker)
255     temporary hardcopy device type (as per 254, but for the temporary saved one)
256     currently loaded hardcopy device driver type [q.v. param 15]
257     warnings bit flags - 0 for all, to suppress: 1 file saved, 2 subs int<->ext, 4 overlaps int<->ext,
           8 sections lines moves/copied, 16 cutter comp, 32 optimized, 64 order menu
258     autosave depth (0 = 99)
259     flag: 2081 has been run for the current hardcopy device (0 = false, 1 = true)
260     duplicate default - 0 = move, 1 = copy
261     initial value for color chip ( par(222) ) - if 0, assume 1
262     scrollbars - 0 = on, 1 = off
263     FirstAid checks: 1=lengths 2=overlaps 4=gaps 8=rads 16=sections 1024=none
264     1 to review matrix channel widths in samples
265     sharp-end matrix to be cut out of order, to avoid catching
266     Create sample relative to: 0 = lower left, 1 = origin, 2 = center, 3 = lower right, 4 = upper left,
			5 = upper right, 6 = left center, 7 = right center, 8 = top center, 9 = bottom center
267     1 to add corner marks on samples matrix
268     1 to optimize matrix
269     1 to mirror sample
270     1 to generate a "size" plot or sample plot
271     samples crease style
272     1 to supress pricing info in demo mode dialog
273     bit flags for tangential tools on Vectocut/IBH/NC_PLOT (1=1,2=2,4=3,8=4,etc)
274     Stripping Boards - if automatic spacer pins added
275     Chaseholes : approximate number of holes to keep
276     Counters   : set to 1 if no "smart" snap on TOOL4 shape endpoints
                     set to 2 if yes, 0 assumed yes
277     0 unspecified computer, 1 on a network, 2 running locally
278     File Storage - 1 to enable CimPACK numeric file storage system
279     File Storage - 1 to put year digits at end of filename, not front
280     DT Rotary Laser #1, 0 = ask etch/draw, 1=draw all, 2=etch all
281     DT Rotary Laser #1, 0 = ask etch/draw, 1=draw all, 2=etch all
282     DT Rotary Laser #1, 0 = ask etch/draw, 1=draw all, 2=etch all
283     DXF Bender Output 0 if use Polylines, 1 of No Polylines
284     DXF Bender Output 0 if output in current units, 1 = inches, 2=metric
285     1 to omit version header on DXF export
286     copy file locally when importing files (useful on NOVELL networks where I/O redirection can fail accross the network)
          1 = smart copy (i.e. check if file is remote, and copy only if so)
          2 = brute copy (i.e. don't bother checking, just always move to local folder)
287     Bender Output, 0 = DXF, 1 = CFF2, 2 = DDESII
288     1 = autorepeat text insert, 0 or 2 = single text insert
289     1 disables the parametrics pop-up notification window
290     No. of entries to save in the history list buffer (0 = default count)
291     No. of files shown in the most recently used list in the file menu (0 = default count)
292     Paper orientation for printing (0=portrait, 1=landscape)
293     1 if Rule Quantities changed to 1 on each piece
294     No. of copies to print (0 defaults to 1 copy)
295     Line Info lists bridges (0=no 1=yes)
296     Spacer Pins 1 if uses a local shape instead of CimPACK circles etc.
297
298     DTRLASER - 1 if prompt for deletion of existing files,
        0 will automatically overwrite
299     Re-Bridging : number of passes to use through the design
300     Forms (and print using form) confirms that default scale is OK:
          1 = show scale as decimals, 2 = show scale as fraction if >1
301     Whether or not to optimize line direction for Gerber Profile suggested by Mr Obayashi
        1 = optimize  0 = not optimized  (optimized line direction only Lines/Arcs/Circles)
302     Rubber (flat) - if adding flattening breaks to rubber pieces
303     Rotary - 1 if default to not adding 3 point segments on output
304     DT Rotary - 1 if default to not moving up one hole as needed
305     Rubber breaks (flat) - 0 undefined, 1 match both,
        2 = match either length
306     "L" Hotkey - 1 if use a menu based version instead of dialog
307     Rubber (rotary) - 1 if adding radii to inside edges 
308     Rubber (rotary) - default tab style number
309     Rubber (rotary) - 1 if adding tabs
310     Rubber (rotary) - 1 if adding text
311     Rubber (rotary) - if adding flattening breaks to rubber pieces
312     Rubber breaks (rotary) - 0 undefined, 1 match both,
        2 = match either length
313     Select By Properties Menu - 1 to always use this instead of standard Select Menu
314     FSB's / Guillotines / Blankers - if automatic tackbridges added
315     Rule Segments - 1 if remembered text is enabled
316     Rotary - 1 if use a wiggle profile as opposed to simple 3pt
317     Translate Plotter output (use DOS extended characters)  0 = false, 1 = true
318     Rule Processor, default cut type to use
        0 default, 1 mitre, 2 straight, 3 tapered, 4 notched, 5 butt 
319     Rule Processor, default end treatment to use
        0 default, 1 rule end, 2 rule end+0, 3 joint, 4 joint plus
320     Striprules : 1 if the auto-copy option is not set by default, 0 yes
321     Blankers : 0 = BSI presser bars, 1 = Speed Bars
322     Dynamic menu minimum width in pixels (0 = accept default menu width)
323     Dynamic menu minimum height in pixels (0 = accept default menu height)
324     Dynamic menu minimum row height in pixels (0 = accept default row height)
325     1 = turn off Smart Snap (ignore any SNAP ON/OFF/ENABLE/DISABLE commands)
326     Dynamic menu minimum row width in (avg) chars
327     Maximum #entries in Select/Properties dropdowns (-1 for no dropdowns)
328     Balance Rules : 1 if they stop at the edge of the cartons
329     Laser out - if flipping over               0 = no, 1 if yes
330     Laser out - if rotating                    0 = no, 1 if yes
331     Laser out - if outputting just valid lines 0 = no, 1 if yes
332     Laser out - if depressing bridges          0 = no, 1 if yes
333     Laser out - units to output in, 0 = current, 1 inches, 2 metric
334     Laser out - if optimizing output           0 = no, 1 if yes
335     Laser out - output as 0 undefined, 1 dxf, 2 cff2, 3 ddes, 4 nc
336     Rotary wiggle - 0 < 1pt 1 = 2pt, 2 = 3pt, 3 = 4pt
337     Creo DTP Output 0 if output in current units, 1 = inches, 2=metric
338     Creo DTP Output, 0 = CFF2, 1 = DDESII
339     Balance Rules - 1 if the back ones run vertically instead
340     System Speed - comparative system speed integer
341     0 for normal outside strip rules, 1 for hooks (rotary)
* take snapshot params
342	default width of a design snapshot
343	default height of a design snapshot
344	include background in snapshot? 2 = yes, 1 = no (only for metafiles right now)
*344	default percent width of snapshot  * not used right now
345	snapshot of whole design? 2 = yes, 1 = visible portion only
346	copy snapshot to clipboard? 2 = yes, 1 = no
347	save snapshot to file? 2 = yes, 1 = no
* trace options params
348     whether to trace in the interpreter. 1 = yes, 0 = no  
349	whether to trace in the View. 1 = yes, 0 = no  
350 	whether to trace in the Mainframe. 1 = yes, 0 = no  
351	whether to trace in the Digitizer. 1 = yes, 0 = no  
352     whether to trace in the CBTHook. 1 = yes, 0 = no  
353     whether to trace in the Macro Tool stuff. 1 = yes, 0 = no  
354     File Storage - 1 don't separate ranges of jobs into folders
355     File Storage - 1 allow letters following job numbers
356     File Storage - 1 don't use fixed digit length
357     File Storage - 1 force manual creation of folders
358     File Storage - use short name for additional saves of jobs
359     File Storage - prompt to confirm filenames if digits but non-job
360     File Storage - last job number saved
361     Forms - 1 bypasses the change any option at end of form
362     Screw holes 1 if uses a local shape instead of CimPACK circles etc.
363     Blankers - if automatic spacer pins added
364     Blankers - 0 if add amount per gutter (tape stackers)
                   1 add amount per blank instead
365     Blankers - 0 if stop horizontal bars at edge of frame, 1 past
366     Blankers - 0 if run bar channels to rails, 1 if stop short
367     Blankers - 0 if block variations use filename, 1 short version
368     Blankers - 0 front to back allowance on rear, 1 = split with front
* thumbnail params
369	default width of thumbnail
370	default height of thumbnail
371	bu default include background in thumbnail? 2 = yes, 1 = no (only for metafiles right now)
372	whether to by default save thumbnails in the same folder as design = 2; 1 = save in default thumbnail path
373	whether to by default save a thumbnail with every design = 2; 1 = no auto save
374     Blankers - 0 = blanker layouts use .FBL, .MBL, .SBL
                   1 = use FBL.CIM, MBL.CIM, SBL.CIM
                   2 = use FB.CIM, MB.CIM, SB.CIM
375     Blankers - 0 = blanker oneups use .BM, .BF, .BS 
                   1 = use BM.CIM, BF.CIM, BS.CIM
376	Snapshot - whether to by default keep the proportions of the width and height the same as the window, 2=yes, 1 = no
377	Snapshot - whether to by default save the snapshot with the design or in the saved path 2=yes, 1=no
378	Thumbnail - whether to by default keep the proportions of the width and height the same as the window; 2=yes, 1=no
379     Striping Boards - 1 if leave partial die at end, not full subroutine
380     File Storage - 1 to enable dialog on File Save As as well
381     DTP Output 0 if output in current units, 1 = inches, 2=metric
382     DTP Output, 0 = CFF2, 1 = DDESII
383     DTP Output, 1 = flip the design over
384     DTP Output, 1 = discard reference crosses
385     DTP Output, 1 = discard non-knife lines
386     DTP Output, 1 = keep just an edge profile
387     DTP Output, 1 = rename subroutines that are negated
388     DTP Output, 1 = rename groups of subroutines with the same name
389     DTP Output, 1 = add filenames
390     0 or 1 for non-repeating Layout/Add One and Add Nest, 2 for repeating


REALS - UNITS DEPENDENT (Inch/Metric)  (1000..1500)
=======================
1000    FUZZ (tolerance)
1001    inch/metric (25.4 for metric, 1 for inch)
1002    tablet X corner
1003    tablet Y corner
1004    tolerance for printing out fractions
1005    default text size for parametric dimensions
1006    nominal X size of screen's graphics area
1007    nominal Y size of screen's graphics area
1008    hardcopy device arc tolerance
1009    width of tabs
1010    length of tabs
1011    radius of loops
1012    hole center radius
1013    length of lead-ins
1014    size of tack bridges
1015    minimum length of arc in DDES file  (.003)
1016    default bridge width (flat)
1017    maximum radius of an arc in DDES file  (100)
1018    minimum chord deviation in DDES file   (.0001)
1019    default pointage
1020    standard sheet size in X (40)
1021    standard sheet size in Y (28)
1022    standard sheet gripper (1/2)
1023    standard left sheet margin (1/4)
1024    standard right sheet margin (1/4)
1025    standard top sheet margin (1/4)
1026    max number of inches of dieboard edge without a tackbridge (18)
1027    default tuck flap height used by MixMatch
1028    default glueflap width used by MixMatch
1029..1033 Distributor parameters
1034    bstyle 0..2 : length per bridge for 4+ bridges
1035    bstyle 0 : minimum length for 1 bridge
1036    bstyle 0 : minimum length for 2 bridges
1037    bstyle 0 : minimum length for 3 bridges
1038    bstyle 0 : minimum length for 4+ bridges
1039    bstyle 1 : minimum length for 1 bridge
1040    bstyle 1 : minimum length for 2 bridges
1041    bstyle 1 : minimum length for 3 bridges
1042    bstyle 1 : minimum length for 4+ bridges
1043    bstyle 2 : minimum length for 1 bridge
1044    bstyle 2 : minimum length for 2 bridges
1045    bstyle 2 : minimum length for 3 bridges
1046    bstyle 2 : minimum length for 4+ bridges
1047    bstyle 2 : bridge end distance
1048    bstyle 3 : minimum length for 1 bridge
1049    bstyle 3 : bridge spacing
1050    bstyle 3 : minimum amount of rule on the bridge-ends
1051    bstyle 4 : bridge end distance
1052    bstyle 4 : bridge spacing
1053    bstyle 4 : minimum amount of rule on the opposite end
1054    default X value used by SARN
1055    default Y value used by SARN
1056    default Y value compensation for Graphtec Dieboard Plots
1057    default X value used by Chase Holes
1058    default Y value used by Chase Holes
1059    Stripping rules : hook size on outside strip rules   (flat)
1060    Stripping rules : hook radius on outside strip rules (flat)
1061    Stripping rules : end offset for stripping rules     (flat)
1062    Stripping rules : distance stripping rules go past edge (flat)
1063    Dieboard Edge : left wood
1064    Dieboard Edge : right wood
1065    Dieboard Edge : front wood
1066    Dieboard Edge : back wood
1067    Dieboard Edge : wood size in X
1068    Dieboard Edge : wood size in Y
1069    Dieboard Edge : radius to use
1070    Dieboard Edge : grip value to use
1071    Dieboard Edge : left / right offset to use
1072    Printing Blanket : Y stretch factor
1073    Printing Blanket : size in X
1074    Printing Blanket : size in Y
1075    Printing Blanket : gripper
1076    Rotary Bridging - bridge size in X
1077    Rotary Bridging - bridge size in Y
1078    Rotary Bridging - bridge spacing in X
1079    Rotary Bridging - bridge spacing in Y
1080    Rotary Bridging - tooth to tooth actual distance (ie .512)
1081    Stripping Boards - FSB Internal Offset
1082    Stripping Boards - FSB External Offset
1083    Chase Holes etc. - Final size to use for 6mm holes
1084    Chase Holes etc. - Final size to use for 9.5mm holes
1085    Stripping Boards - Inside diameter for spacer pin
1086    Stripping Boards - Outside diameter for spacer pin
1087    Stripping Boards - Default offset for gripper
1088    Laser - what to use for 2point slot compensation (ie. .028 beam)
1089    Laser - pwidth value used for lines expected to be 2 point
1090    Stripping rules - minimum line length to have bridges (flat)
1091    Rotary - joint setback amount
1092    Rotary - joint length
1093    Layout double cut default for X - see also par(113)
1094    Counters - default 3rd spindle width
1095    Counters - default 4th spindle width
1096    Counters - default 5th spindle width
1097    Counters - fixed distance for TW4 away from creases
1098    Punches - additional amount to subtract from the diameter for laser
1099    Pointage width (PWIDTH) to use for crease lines (Japan only)
1100    Stripping Boards - opening width for male blocks at tab area
1101    Stripping Boards - FSB Male Block offset
1102    Move origin when adding crosses: 0 ask first time, 1 ask, 2 no, 3 yes
1103    Handles - size in the X (flat)
1104    Handles - size in the Y (flat)
1105    Counters - size of counter hole cross
1106    Counters - default crease pullback for TOOL3
1107    Handles - amount of wood around handle (flat)
1108    FSB / Guillotine - default slot width for outside edges only
1109    Stripping Rules - scrap size in X
1110    Stripping Rules - scrap size in Y
1111    Stripping Rules - tilt amount for scrap edges
1112    Punches - amount to add to base sizes of jigged punches
1113    Crosses - default length for lines
1114    Crosses - default length for crosses
1115    Crosses - default offset from design edge
1116    Samples - amount to shorten all creases by
1117    Default hardcopy device X offset to use if par(150) is 1
1118    Default hardcopy device Y offset to use if par(150) is 1
1119    Dieboard Edge : hanging pin diameter
1120    Dieboard Edge : hanging pin side offset
1121    Dieboard Edge : hanging pin top offset
1122    Names    : default height
1123    Printing Blankets : Border Size in X
1124    Printing Blankets : Border Size in Y
1125    Printing Blankets : Border Grip Value X
1126    High Tolerance Menu : Default runby length
1127    High Tolerance Menu : Default T-Knife length
1128    High Tolerance Menu : Default airtrack width
1129    Punches : size of smallest punch to be tacked in
1130    Punches : default wall thickness for plugs
1131    Stripping Boards : default CL Notch hole size
1132    Samples - amount to shorten a matrix channel
1133    Dieboard Edge - amount to use for dieboard edge laser beam only
1134    Text - forces text in dimensions to always be this size
1135    Rubber - minimum length of 1st line to split off
1136    Rubber - amount of 1st line to split off
1137    Bleeds - default offset to use
1138    FSB - default wood offset for edges
1139    FSB - default block width for edges
1140    MSB - default wood offset for edges
1141    Ratio of linear dimension short extension to text size (default 1:1)
1142    Ratio of linear dimension long extension to text size (default 1:1)
1143    Ratio of linear dimension long extension pull-back to text size (default 1:1)
1144    Chase Holes etc. - Final size to use for 10mm holes
1145    Rotary - bolt step to use for Ward 50 inch (1st menu page)
1146    Rotary - bolt step to use for generic 66 inch (1st menu page)
1147    Rotary - bolt step to use for generic 52 inch (2nd menu page)
1148    Rotary - bolt step to use for generic 86 inch (2nd menu page)
1149    FSB - diameter to use for red dog holes
1150    Data Tech - default size for text
1151    Data Tech - default shell size for 33 inch half shell
1152    Rubber (flat) - spacing between tabs
1153    Rubber (flat) - offset from top of rubber to edge of knife
1154    Rubber (flat) - offset from base of rubber to edge of crease
1155    Rubber (flat) - offset from base of rubber to edge of perf
1156    Rubber (flat) - offset from base of rubber to edge of knife
1157    Rubber (flat) - width at base
1158    Rubber (flat) - maximum amount to follow a crease
1159    Rubber (flat) - default height for numbers
1160    Rubber (flat) - minimum inside radius to add
1161    Minimum distance allowed by POINT and CLOSEST functions
1162    Nicks - length of nicks
1163    Nicks - nick end amount
1164    Nicks - gap between nicks
1165    Nicks - gap between double sets of nicks
1166    Rotary - default wood thickness
1167    Rotary - value to switch from partial to full shell, e.g. 19 inches
1168    Dieboard Edge - front to back dimension (for sides option)
1169    Dieboard Edge - wood on sides
1170    Handles - size in the X (rotary)
1171    Handles - size in the Y (rotary)
1172    Handles - amount of wood around handle (rotary)
1173    Handles - shell width to switch to 3 handles (rotary)
1174    Handles - shell width to switch to 4 handles (rotary)
1175    Stripping rules : hook size on outside strip rules   (rotary)
1176    Stripping rules : hook radius on outside strip rules (rotary)
1177    Stripping rules : end offset for stripping rules     (rotary)
1178    Stripping rules : spacing between stripping rules
1179    Stripping rules : length of spaced rules
1180    Balance rules - length of fixed segments
1181    FSB - amount to shorten wooden support rails on front
1182    FSB - amount to shorten wooden support rails on rear
1183    Handles - amount to avoid balance rules by
1184    Layout double cut default for Y - see also par(113)
1185    FSB - default size of orange jigs
1186    Grid size (for view options)
1187    Folders - default glueflap taper
1188    Folders - default pocket height
1189    Folders - default glueflap width
1190    Stripping Rules - Spaced rules taper amount
1191    FirstAid - maximum gap size
1192    FirstAid - maximum radius
1193    FirstAid - mimimum length
1194    CD's - default glueflap width
1195    CD's - default front panel offset
1196    Stripping Boards - approximate tackbridge spacing on long lines
1197    Stripping Boards - approximate spacing between spacer pins
1198    Rack Hanging Pins - distance to switch to 3 pins
1199    Blankers - default female offset
1200    Blankers - default male offset
1201    Blankers - default steel support plate offset
1202    Blankers - default vacuum hole offset
1203    Dieboard Edge - minimum size allowed front to back (Y)
1204    Dieboard Edge - maximum size allowed front to back (Y)
1205    Dieboard Edge - minimum size allowed left to right (X)
1206    Dieboard Edge - maximum size allowed left to right (X)
1207    Re-Bridging : lower end of bridge range to check
1208    Re-Bridging : higher end of bridge range to check
1209    Re-Bridging : expected bridge size to look for
1210    FirstAid - overlap tolerance
1211    FirstAid - overlap minimum length of new lines
1212    Rubber (flat) - default size of break to add
1213    Rubber (flat) - amount of material to leave on flattening V's
1214    Rubber (flat) - minimum line length surrounding a flattening break
1215    Rotary - amount of line to split off seam for 3pt segments
1216    Rotary - width of laser beam for trimming shell edges (.017)
1217    Rubber (flat) - maximum radius length for breaks
1218    Rubber (rotary) - spacing between tabs
1219    Rubber (rotary) - offset from top of rubber to edge of knife
1220    Rubber (rotary) - offset from base of rubber to edge of crease
1221    Rubber (rotary) - offset from base of rubber to edge of perf
1222    Rubber (rotary) - offset from base of rubber to edge of knife
1223    Rubber (rotary) - width at base
1224    Rubber (rotary) - maximum amount to follow a crease
1225    Rubber (rotary) - default height for numbers
1226    Rubber (rotary) - minimum inside radius to add
1227    Rubber (rotary) - default size of break to add
1228    Rubber (rotary) - amount of material to leave on flattening V's
1229    Rubber (rotary) - minimum line length surrounding a flattening break
1230    Rubber (rotary) - maximum radius length for breaks
1231    Rubber (rotary) - width of the slot wave
1232    Rubber (rotary) - pitch of the slot rubber
1233    Rubber (rotary) - amount to chop back the trail edge
1234    Rubber (flat) - width of the slot wave
1235    Rubber (flat) - pitch of the slot rubber
1236    Rubber - sheet size in X
1237    Rubber - sheet size in Y
1238    Rubber - sheet margin on outside edge
1239    Rotary wiggle - width of the tightening wiggle
1240    Rotary wiggle - pitch of the tightening wiggle
1241    StrippingClip - internal stripping offset
1242    StrippingClip - external stripping offset
1243    StrippingClip - inactive offset to use
1244    StrippingClip - inactive offset to use (outside)
1245    StrippingClip - clip offset to use
1246    StrippingClip - distance from end of line for clips
1247    StrippingClip - fixed angle to use for a part
1248    StrippingClip - PickRod (PR10) width
1249    StrippingClip - Default stripping pin diameter to use with spring clip
1250    StrippingClip - base size for the default pin
1251    StrippingClip - distance to maintain from the design edge
1252    Counters  - skivedown clearance (&SB5), 999 = 0
1253    Blankers  - default component end distance
1254    Rotary    - default bolthole size for lasercutting
1255    Bleeds    - default offset for offset lines, side bevel
1256    Side Name - nail diameter to use for flat and rotary
1257    Rotary - default width for bolt slots
1258    Rule Segments - shortening amount (flat)
1259    Rule Segments - shortening amount (rotary)
1260    Rule Segments - default wood thickness (if no rotary shell wood set)
1261    Rotary wiggle - length of the flat spot around bridges, 999 = 0
1262    BSI - size of screw holes to use
1263    Print Grip - default value for blanker print grip
1264    Blankers - default hole shrink wood to steel
1265    Blankers - default screw hole size for wood
1266    Counters - amount of material to leave below skiving tool #5
1267    Rotary Bridging - rotary micro bridge width
1268    Rubber (flat)   - offset from base of rubber to edge of knife (#2)
1269    Rubber (rotary) - offset from base of rubber to edge of knife (#2)
1270    Blankers - additional wood to add to the rear of the blanker
1271    Blankers - amount to run horizontal frame past the vertical edge
1272    Blankers - StrippingClip clip offset to use
1273    Blankers - frame bar width
1274    StrippingClip - offset to use when adding prong offset from existing
1275    Side Name - additional amount of wood taken out in name cavity
1276    Blankers - amount of space around the outside for joggers etc.
1277    Spline tolerance
1278    Stripping rules, distance stripping rules go past edge (rotary)
1279    Stripping rules, minimum line length to have bridges   (rotary)
1280    bstyle 0 (rotary) : length per bridge for 4+ bridges
1281    bstyle 0 (rotary) : minimum length for 1 bridge
1282    bstyle 0 (rotary) : minimum length for 2 bridges
1283    bstyle 0 (rotary) : minimum length for 3 bridges
1284    bstyle 0 (rotary) : minimum length for 4+ bridges
1285    bstyle 0 (rotary) : default bridge width
1286    circle radius for Ends in view menu (default .015")
1287    Counters - expected size of dieboard counter holes
1288    bstyle 0,2 : length per bridge for 4+ bridges (2nd configuration)
1289    bstyle 0,2 : minimum length for 1 bridge
1290    bstyle 0,2 : minimum length for 2 bridges
1291    bstyle 0,2 : minimum length for 3 bridges
1292    bstyle 0,2 : minimum length for 4+ bridges
1293    bstyle 0,2 : default bridge width
1294    bstyle 0,3 : length per bridge for 4+ bridges (3rd configuration)
1295    bstyle 0,3 : minimum length for 1 bridge
1296    bstyle 0,3 : minimum length for 2 bridges
1297    bstyle 0,3 : minimum length for 3 bridges
1298    bstyle 0,3 : minimum length for 4+ bridges
1299    bstyle 0,3 : default bridge width
1300    Stripping Boards - spacing between male stripping pins (inside)
1301    Stripping Boards - spacing between male stripping pins (outside)
1302    Stripping Boards - spacer pin edge to block clearance
1303    Blankers - approximate spacing between spacer pins
1304    Blankers - amount to add per gutter for tape stackers
1305    Blankers - amount to add per blank instead
1306    Blankers - amount to run side bars past edge of rail
1307    Blankers - shorten bar channels by, where possible (sides)
1308    Blankers - amount of wood left off lead edge of frame
1309    Blankers - shorten bar channels by, where possible (front/rear)
1310    Rotary - distance from lead edge shell to first row bolts


STRINGS (500 chars each)  (2000..2150)
=======
2001    digitizer initialization
2002    sent to hardcopy device at start of every plot
2003    sent to hardcopy device at end of every plot
2004    hardcopy device model name
2005    sent to hardcopy device at pen pen 1   In DOS product, if these start with ";",
2006    sent to hardcopy device at pen pen 2   they represent integer expressions
2007    sent to hardcopy device at pen pen 3   giving speed:
2008    sent to hardcopy device at pen pen 4         ;straights;arcs;text
2009    sent to hardcopy device at pen pen 5     or  ;straights;arcs       (text same as arcs)
2010    sent to hardcopy device at pen pen 6     or  ;straights            (all are the same)
2011    sent to hardcopy device at pen pen 7   Each expression can be constant or variable:
2012    sent to hardcopy device at pen pen 8    e.g.  ;len(*)<3.5?6:10;rad(*)<1?3:5
2013    sent to hardcopy device at pen moves   Speed is output only if it is changed.
2014    default text for Sample Labels, ie CAD Carton Design by Cimex
2015    if a filename here, plots to this instead of to port (for networks)
          (Note: to plot to \\server\@plotter, par(2015) = "\","\server...")
2016    string to send to HPGL plotter instead of OP;
2017    brand of counter cutter (e.g. Elcede)
2018    brand of samplemaker (e.g. Elcede)
2019    NO LONGER USED!!! You must setup your Windows Desktop Shortcut Icon Instead! [used to be: default (start-up) directory]
2020    country
2021    prefix and suffix for radius
2022    prefix and suffix for diameter
2023    prefix and suffix for degrees
2024    hardcopy device name
2025    Plotters : default prefix for indirect filenames, ie T:
2026    Rotary : default directory to merge files from
2027    Corrugated MixMatch : String of allowances for panel # 1
2028    Corrugated MixMatch : String of allowances for panel # 2
2029    Corrugated MixMatch : String of allowances for panel # 3
2030    Corrugated MixMatch : String of allowances for panel # 4
2031    Counters : string for calculation of &TW1
2032    Counters : string for calculation of &TW2
2033    Default directory for import  !NO LONGER USED!
2034    Plotter config file name for hotkey form plot
2035    Form file name for hotkey form plot
2036    Dieboard Edge - default filename to pull in for a logo
2037    Top directory for customer specs
2038    Sent to a DOS Shell command when switching to a new hardcopy device
2039    Default directory for export  !NO LONGER USED!
2040    Default directory for merge/include  !NO LONGER USED!
2041    Plotters : default extension for indirect filenames, e.g. HPG
2042    Default file extension for cimex files other than CIM (e.g. LAY) (note: doesn't include the . (dot) separator)
2043    Plotter name for hotkey print screen
2044    Digitizer buttons
2045    List of directories to search when a filename is typed
2046    Text editor to use for Notes (default = "cimedit /numbers=no")
2047    Top directory for Advanced Rotary Rule Types
2048    Top directory for Advanced Rubber Rule Types
2049    Dieboard Edge - default formula for LRTB Grip calculation
2050    Dieboard Edge - default formula for Gripctr w / Grip calculation
2051    MSB - menu name for custom pin #1
2052    MSB - menu name for custom pin #2
2053    MSB - menu name for custom pin #3
2054    MSB - menu name for custom pin #4
2055    MSB - menu name for custom pin #5
2056    MSB - menu name for custom pin #6
2057    MSB - menu name for custom pin #7
2058    MSB - menu name for custom pin #8
2059    MSB - menu name for custom pin #9
2060    MSB - menu name for custom pin #10
2061-2065 Distributor parameters
2066    Sideup Menu - text for F1 (Print Side)
2067    Sideup Menu - text for F2 (Die Side)
2068    DT Rotary - default drive / directory for files (Laser #1)
2069    "GET" string to use from menus for picking a style
         e.g. GET for DOS, or GET DOUBLE for Windows
2070    Current hardcopy device driver macro (use this macro command line in place of the normal hardcopy device code)
2071    Default screen map
2072    Current hardcopy device form name
2073    Current hardcopy device physical configuration spooler folder (or windows printer name, depending on param 15)
2074    Current hardcopy device pen map name
2075    Temporary hardcopy device name (used to track the currently saved "temporary" hardcopy device)
2076    Override: "magic" hardcopy plotting macro (for custom macros that don't go through the normal plot logic)
2077    Override: plotter to load (i.e. don't show dialog, just load this)
2078    Override: samplemaker to load (i.e. don't show dialog, just load this)
2079    Current hardcopy device "tweak" macro name
2080    Current hardcopy device "properties" macro name - a dialog macro to be run when user presses properties button for this device
2081    Current hardcopy device "setup" macro name - this dialog is for asking for additional plotter parameters that aren't part of the standard plot dialog
2082    ODBC Data Source Name
2083    Name of the printer to use for Sample Labels
2084    Face name for dimensions (defaults to "Courier New")
2085    "Using" file for NC plotters (note: not automatically loaded by device command)
2086    Rule Segments Output : Default Folder to save files to
2087    DXF Bender Output : Default Folder to save files to
2088    Argument string for TRANSMIT when CimLite is to be used as an HPGL front-end (e.g. COM2:19200,8,N,1 echo)
2089    Rubber - folder to output waterjet files to
2090    DT Rotary - default drive / directory for files (Laser #2)
2091    DT Rotary - default drive / directory for files (Laser #3)
2092    Format line for generating CFF2 autoprint statement (can be used to do anything via shell command) (e.g. notepad.exe /p %s)
2093    Additional Cimex file extensions.  These are in addition to .cim, .fsb, .msb, etc.  Each extension is stored WITH the dot (.) separator, and each is semicolon (;) separated
2094    (Custom) Import/Export File extensions -- no longer used
2095    Selection to use for Overlaps (bypassing Select menu)
2096    Laser out - default folder to output to
2097    Creo DTP Output - Default Folder to save files to
2098    Gerber Output   - Default Folder to save files to
2099    Dieboard Merge  - Default Folder to save files to
2100    Common dimensions menu
2101    Standard sheet sizes for Pick Size, stored in mm

2103    Flat (Layout Options Menu) : default directory to merge files from    
2104    Rubber - default prefix to use on layout files
2105    Fix Layout - User section name #1
2106    Fix Layout - User section name #2
2107    Fix Layout - User section name #3
2108	default format for a snapshot (bmp, gif, jpg, emf)
2109	default way to size a snapshot (EXACT = window size, or CUSTOM = user choice)
2110	default folder for auto snapshot
2111    File Storage - root level folder for job files
2112    File Storage - root level for non job files
2113	Email address to mail bug reports to: i.e. support@cimexcorp.com
2114    File Storage - root level for imported files
2115    Current hardcopy device form name (PDF)
2116    Current hardcopy device (windows printer name) (PDF)
2117    Current hardcopy device pen map name (PDF)

// thumbnail stuff
2118	default format for a thumbnail (bmp, gif, jpg, emf)
2119	default way to size a thumbnail (EXACT = window size, or CUSTOM = user choice)
2120	path of default thumbail folder, if empty then thumbnail will go into same folder as the design

2121	Snapshot - the path to save snapshots to if not saved with the design
2122    Bolthole Merge  - Default Folder to save files to
2123    DTP Output - Default Folder to save files to


REALS - INDEPENDENT OF UNITS  (3000..3060)
============================
3001    tablet scale
3002    mouse speed
3003    hardcopy device X accuracy scale
3004    hardcopy device Y accuracy scale
3005    increment size, in mm. (if 0, uses default for hardcopy device)
3006    minimum subtended angle of arcs in DDES file (.5)
3007    current pointage being used, 0 same as 2
3008    maximum X or Y allowed for hardware arc center (0 = safe defaults)
3009    skew ratio for plotters, 0 = 90 degrees, (tangent of skew angle)
3010-3016 Distributor parameters
3017    X hardcopy device offset (in hardcopy device increments - added to all hardcopy device output)
3018    Y hardcopy device offset (use a positive X offset if there is negative skew)
3019    pointage to use for the lasercut names, 0 assumed as 2
3020    pointage to use for the dieboard edge, 0 assumed to be 2   
3021    pointage for chase holes, punches, handles, FSB, MSB etc.
3022    Stripping rules, angle of hook in degrees (flat)
3023    Counters : Angle of the skive tool
3024    Counters : Angle of the cutout tool
3025    Bridge Menu - (width1 / F9)  default bridge width Imperial
3026    Bridge Menu - (width2 / F10) default bridge width Imperial
3027    Bridge Menu - (width3 / F11) default bridge width Imperial
3028    SARN Drawing - stretch factor to use in Y axis (0 same as 1)
3029    Max percentage of line which can be used for bridges (def 100%)
3030    angle of straight lead-ins (90 is perpendicular)
3031    Bridge Menu - (width1 / F9)  default bridge width Metric
3032    Bridge Menu - (width2 / F10) default bridge width Metric
3033    Bridge Menu - (width3 / F11) default bridge width Metric
3034    logical hardcopy device Y stretch factor (0 implies 1.000)
3035    Animate speed, if non-zero (.5 means 1/2 the default speed)
3036    Balance rules - fixed number of bridges on fixed length segments
3037    Bridge Menu - (width4) default bridge width Imperial
3038    Bridge Menu - (width5) default bridge width Imperial
3039    Bridge Menu - (width6) default bridge width Imperial
3040    Bridge Menu - (width7) default bridge width Imperial
3041    Bridge Menu - (width8) default bridge width Imperial
3042    Bridge Menu - (width9) default bridge width Imperial
3043    Bridge Menu - (width4) default bridge width Metric
3044    Bridge Menu - (width5) default bridge width Metric
3045    Bridge Menu - (width6) default bridge width Metric
3046    Bridge Menu - (width7) default bridge width Metric
3047    Bridge Menu - (width8) default bridge width Metric
3048    Bridge Menu - (width9) default bridge width Metric
3049    Timer delay (in seconds) for right mouse pop-ups
3050    Default view flags (can be too large for an int)
3051    logical hardcopy device X stretch
3052    logical hardcopy device scale factor (0 implies 'to fit')
3053    Program version number that ran most recently
3054    current hardcopy device flags (stored identically to the view flags)
3055    autosave interval (0.0 = 1.0 min.)
3056    position of circle lead-ins, less 90 (i.e. 0 positions at 90)
3057    Default Dimension Color (2-byte RGB)
3058    Default Dimension BIUM
3059    Rubber (flat) - minimum angle change to use flattening break up at
3060    Rubber (rotary) - minimum angle change to use flattening break up at
3061    Rubber - default angle to rotate by in autolay
3062    Stripping rules, angle of hook in degrees (rotary)
3063	Version number last time EULA was displayed/approved
3064    File Storage - number of folders to store per folder
3065    File Storage - number of digits in job number without year
3066    File Storage - number of digits in job number for year
