* SPECIAL.TXT listing of use of special versions of common linetypes
* Version W10.2.6.7 07/16/02

1   = punches (attr 10 base & attr 17 cutting edge)
2   = balance knives (attr 13)
3   = floats (attr 10)
4   = stripping knives (attr 13)
5   = tick marks between changes of cut/crease for example (attr 10/16)
6   = sheet (attr 18 physical, 19 usable)
7   = rotary shells (attr 18 outside, 19 seams)
8   = reference crosses from menus (attr 17, attr 10 burn on crossbrn)
9   = high tolerance runbys (attr 10)
10  = high tolerance stopper rule (attr 10)
11  = crease matrix lines (attr 36)
12  = counter holes (attr 10)
13  = hanger holes (attr 1 cuts, 17/23 on Pace ones)
14  = business card (attr 1 cuts, attr 17 size)
15  = lasercut name (attr 10 full cut, 16 etched)
16  = dieboard edge (attr 12)
17  = rotary slot marking lines (attr 10 chopout, 16 outside of slot)
18  = rotary horizontal / vertical joints (attr 16)
19  = bridge hash marks (attr 16)
20  = "V" slot has markers (attr 16)
21  = dovetail die edge lines (attr 12)
22  = jigged double lines (attr 22)
23  = standard printing bleeds (attr 22)
24  = bridge depression lines (attr 20)
25  = jigged drill holes (attr 20)
26  = rotary boltholes (attr 18 outside, 17 cross, 11 central laser hole)
27  = rotary hashmarks on shell edge (attr 10)
28  = rotary boltholes center crosses (or chase reg. holes) (attr 17)
29  = rotary keyhole (attr 5)
30  = handles (attr 10, 17 tacks)
31  = chase registration holes (attr 11)
32  = gripper finger marks (attr 16)
33  = Easyset (attr 7 - 4 slots/circles, 10 holes, 17 reference clamps)
34  = shortening circles, temporary (attr 19)
35  = Steel makeready (attr 17 reference, 6 actual lines)
36  = Guillotine (attr 10)
37  = FSB Internal Windows (attr 12)
38  = FSB External Profile (attr 12)
39  = FSB Alignments (attr 10 red/orange, 25 "T")
40  = FSB Etched Bar Line (attr 16)
41  = FSB Spacer Pin (attr 10 center, 17 profile)
42  = FSB Internal Block (attr 14, 6 vacuum)
43  = FSB External Block (attr 14, 6 vacuum)
44  = FSB Support bars (attr 12 holes / ends), 17 profile)
45  = FSB Slot Shortening chamfer (attr 17)
46  = FSB 1 x 4 blocks (attr 12 circles, 17 profile)
47  = FSB Press alignment holes (attr 10, 17 profiles)
48  = MSB 1600 Honeycomb pattern (attr 6)
49  = MSB Internal Windows (attr 14, 17 pin sizes)
50  = MSB External Profile (attr 14)
51  = MSB Vacuum Holes (attr 6)
52  = MSB Alignments (attr 25 "T", 12 die holes, 10 Orange Jig / 203 hooks)
53  = MSB T knife stoppers (attr 14)
54  = MSB Chamfer Lines from FSB (attr 13)
55  = MSB FSB pulled in lines (attr 10 / 17 blocks)
56  = Blankers, female profile (attr 12)
57  = Blankers, male profile (attr 14)
58  = Blankers, vacuum (attr 6)
59  = Blankers, steel reinforcing plate (attr 12)
60  = Blankers, spacer pins (attr 10, 17)
61  = Blankers, outside edge reference (attr 33, 17)
62  = TE Rule (attr 1, 10 slot)
63  = Rotary shell lines to be lasercut (attr 12)
64  = Rotary Bolthole slots (attr 10,17)
65  = Nicks (attr 16 or 24)
66  = stripping rule hook lines (10,13), actual rule is still 4
67  = FSB Bobst tab breakers on bar line etc. (attr 10, 17)
68  = Blankers, (Male) buttons / presser bars (attr 10,17)
69  = Blankers, (Female) holes / mounting bars (attr 10,17)
70  = Blankers, (Male) holes / mounting bars (attr 10,17)
71  = Strip-Clip, Female Openings for clips (attr 10,17,18)
72  = Strip-Clip, Male Prong / Pin Lines (attr 5,10,17,18)
73  = Strip-Clip, Female Subroutine
74  = Strip-Clip, Male Subroutine
75  = Hangholes, body of the hanger hole lines (construction 17)
76  = Hangholes, base size and cut profile (attr 10, 17)
77  = Thomson Diecutter, chase holes / sheet guides, corners (1,10,11)
78  = Rotary Boltholes, Serrapid Mounting Holes (10,11,12,17)
79  = Strip-Clip, Female / Male Combination Subroutine
80  = Strip-Clip, SR10 break-apart lines
81  = Strip-Clip, Pin and Pick Rod Lines (14)
82  = Wagner 'Le Gard' lead edge reinforcers
83  = Blankers - LF Components (subs)
84  = Blankers - steel frame, outside rail lines (17)
85  = Blankers - steel frame, inside bar lines (17)
86  = Blankers - text that is to be substituted with names later (23)
87  = Rotary - tape marking lines
88  = Blankers - non-stop bars / swords (16,17)
89  = Blankers - routed profile, eg. skive down perimeter board, grip (17)
90  = Blankers - screw holes for mounting wood and steel together
91  = Blankers - stacking bar, bascially when jogger too big
92  = Strip-Clip, distance bolts (10,17)
93  = Screw Holes - top board lines (10,17)
94  = Screw Holes - base board lines (10)

Airtracks were 11, changed back to 0
Hanger holes were 13, changed back to 0
Business Cards were 14, changed back to 0
TE Rule was 62, changed back to 0
