ªªªªíýº°ªªíýº°ªªªªíýº°ªªªíýº°ªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªStarting fastboot ...


System startup
DDRS
Reg Version:  v1.1.0
Reg Time:     2016/12/11 22:54:35
Reg Name:     hi3798mdmo1f_hi3798mv100_ddr3_1gbyte_16bitx2_2layers_emmc.reg

Jump to DDR


Fastboot 3.3.0-00007-gb5b796c-dirty (shaoqiang.yu@ubuntu) (Sep 18 2017 - 18:01:28)

Fastboot:      Version 3.3.0
Build Date:    Sep 18 2017, 18:02:23
CPU:           Hi3798Mv100 
Boot Media:    eMMC
DDR Size:      1GB

Check nand flash controller v610. found
Special NAND id table Version 1.36
Nand ID: 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00
No NAND device found!!!

MMC/SD controller initialization.
MMC/SD Card:
    MID:         0x15
    Read Block:  512 Bytes
    Write Block: 512 Bytes
    Chip Size:   3728M Bytes (High Capacity)
    Name:        "4FPD3"
    Chip Type:   MMC
    Version:     5.0
    Speed:       52000000Hz
    Bus Width:   8bit
    Boot Addr:   0 Bytes

Boot Env on eMMC
    Env Offset:          0x00100000
    Env Size:            0x00010000
    Env Range:           0x00010000
HI_OTP_LockIdWord,327: ID_WORD have already been locked
product_init,284
start download process.
bootdelay=0
verify=n
baudrate=115200
ipaddr=192.168.1.10
serverip=192.168.1.1
netmask=255.255.255.0
bootfile="uImage"
phy_intf=mii,rgmii
use_mdio=0,1
phy_addr=2,1
gmac_debug=0
bootcmd=mmc read 0 0x1FFBFC0 0x50000 0x5000; bootm 0x1FFBFC0
factory_bootargs=console=ttyAMA0,115200 root=/dev/mmcblk0p16 rootfstype=ext3 rootwait blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs=console=ttyAMA0,115200 lpj=974848 quiet blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs_512M=mem=512M mmz=ddr,0,0,112M
bootargs_768M=mem=768M mmz=ddr,0,0,300M
bootargs_1G=mem=1G mmz=ddr,0,0,435M
bootargs_2G=mem=2G mmz=ddr,0,0,620M
signature_check=sign:recovery,recovery,0x200000 sign:kernel,kernel,0x700000
stdin=serial
stdout=serial
stderr=serial

Environment size: 1335/65532 bytes
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)[EOT](OK)
[EOT](OK)
[EOT](OK)[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)

MMC write: dev # 0, block # 24576, count 1 ... 1 blocks written: OK
[EOT](OK)
Starting fastboot ...


System startup
DDRS
Reg Version:  v1.1.0
Reg Time:     2016/12/11 22:54:35
Reg Name:     hi3798mdmo1f_hi3798mv100_ddr3_1gbyte_16bitx2_2layers_emmc.reg

Jump to DDR


Fastboot 3.3.0-00007-gb5b796c-dirty (shaoqiang.yu@ubuntu) (Sep 18 2017 - 18:01:28)

Fastboot:      Version 3.3.0
Build Date:    Sep 18 2017, 18:02:23
CPU:           Hi3798Mv100 
Boot Media:    eMMC
DDR Size:      1GB

Check nand flash controller v610. found
Special NAND id table Version 1.36
Nand ID: 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00
No NAND device found!!!

MMC/SD controller initialization.
MMC/SD Card:
    MID:         0x15
    Read Block:  512 Bytes
    Write Block: 512 Bytes
    Chip Size:   3728M Bytes (High Capacity)
    Name:        "4FPD3"
    Chip Type:   MMC
    Version:     5.0
    Speed:       52000000Hz
    Bus Width:   8bit
    Boot Addr:   0 Bytes

Boot Env on eMMC
    Env Offset:          0x00100000
    Env Size:            0x00010000
    Env Range:           0x00010000
HI_OTP_LockIdWord,327: ID_WORD have already been locked
product_init,284
start download process.
bootdelay=0
verify=n
baudrate=115200
ipaddr=192.168.1.10
serverip=192.168.1.1
netmask=255.255.255.0
bootfile="uImage"
phy_intf=mii,rgmii
use_mdio=0,1
phy_addr=2,1
gmac_debug=0
bootcmd=mmc read 0 0x1FFBFC0 0x50000 0x5000; bootm 0x1FFBFC0
factory_bootargs=console=ttyAMA0,115200 root=/dev/mmcblk0p16 rootfstype=ext3 rootwait blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs=console=ttyAMA0,115200 lpj=974848 quiet blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs_512M=mem=512M mmz=ddr,0,0,112M
bootargs_768M=mem=768M mmz=ddr,0,0,300M
bootargs_1G=mem=1G mmz=ddr,0,0,435M
bootargs_2G=mem=2G mmz=ddr,0,0,620M
signature_check=sign:recovery,recovery,0x200000 sign:kernel,kernel,0x700000
stdin=serial
stdout=serial
stderr=serial

Environment size: 1335/65532 bytes
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)[EOT](OK)
[EOT](OK)
[EOT](OK)[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)

MMC write: dev # 0, block # 24576, count 1 ... 1 blocks written: OK
[EOT](OK)
Starting fastboot ...


System startup
DDRS
Reg Version:  v1.1.0
Reg Time:     2016/12/11 22:54:35
Reg Name:     hi3798mdmo1f_hi3798mv100_ddr3_1gbyte_16bitx2_2layers_emmc.reg

Jump to DDR


Fastboot 3.3.0-00007-gb5b796c-dirty (shaoqiang.yu@ubuntu) (Sep 18 2017 - 18:01:28)

Fastboot:      Version 3.3.0
Build Date:    Sep 18 2017, 18:02:23
CPU:           Hi3798Mv100 
Boot Media:    eMMC
DDR Size:      1GB

Check nand flash controller v610. found
Special NAND id table Version 1.36
Nand ID: 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00
No NAND device found!!!

MMC/SD controller initialization.
MMC/SD Card:
    MID:         0x15
    Read Block:  512 Bytes
    Write Block: 512 Bytes
    Chip Size:   3728M Bytes (High Capacity)
    Name:        "4FPD3"
    Chip Type:   MMC
    Version:     5.0
    Speed:       52000000Hz
    Bus Width:   8bit
    Boot Addr:   0 Bytes

Boot Env on eMMC
    Env Offset:          0x00100000
    Env Size:            0x00010000
    Env Range:           0x00010000
HI_OTP_LockIdWord,327: ID_WORD have already been locked
product_init,284
start download process.
bootdelay=0
verify=n
baudrate=115200
ipaddr=192.168.1.10
serverip=192.168.1.1
netmask=255.255.255.0
bootfile="uImage"
phy_intf=mii,rgmii
use_mdio=0,1
phy_addr=2,1
gmac_debug=0
bootcmd=mmc read 0 0x1FFBFC0 0x50000 0x5000; bootm 0x1FFBFC0
factory_bootargs=console=ttyAMA0,115200 root=/dev/mmcblk0p16 rootfstype=ext3 rootwait blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs=console=ttyAMA0,115200 lpj=974848 quiet blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs_512M=mem=512M mmz=ddr,0,0,112M
bootargs_768M=mem=768M mmz=ddr,0,0,300M
bootargs_1G=mem=1G mmz=ddr,0,0,435M
bootargs_2G=mem=2G mmz=ddr,0,0,620M
signature_check=sign:recovery,recovery,0x200000 sign:kernel,kernel,0x700000
stdin=serial
stdout=serial
stderr=serial

Environment size: 1335/65532 bytes
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)[EOT](OK)
[EOT](OK)
[EOT](OK)[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)

MMC write: dev # 0, block # 24576, count 1 ... 1 blocks written: OK
[EOT](OK)
ªªªíýº°ªªªªªªªíýº°ªªªíýº°ªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªStarting fastboot ...


System startup
DDRS
Reg Version:  v1.1.0
Reg Time:     2016/12/11 22:54:35
Reg Name:     hi3798mdmo1f_hi3798mv100_ddr3_1gbyte_16bitx2_2layers_emmc.reg

Jump to DDR


Fastboot 3.3.0-00007-gb5b796c-dirty (shaoqiang.yu@ubuntu) (Sep 18 2017 - 18:01:28)

Fastboot:      Version 3.3.0
Build Date:    Sep 18 2017, 18:02:23
CPU:           Hi3798Mv100 
Boot Media:    eMMC
DDR Size:      1GB

Check nand flash controller v610. found
Special NAND id table Version 1.36
Nand ID: 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00
No NAND device found!!!

MMC/SD controller initialization.
MMC/SD Card:
    MID:         0x15
    Read Block:  512 Bytes
    Write Block: 512 Bytes
    Chip Size:   3728M Bytes (High Capacity)
    Name:        "4FPD3"
    Chip Type:   MMC
    Version:     5.0
    Speed:       52000000Hz
    Bus Width:   8bit
    Boot Addr:   0 Bytes

Boot Env on eMMC
    Env Offset:          0x00100000
    Env Size:            0x00010000
    Env Range:           0x00010000
HI_OTP_LockIdWord,327: ID_WORD have already been locked
product_init,284
start download process.
bootdelay=0
verify=n
baudrate=115200
ipaddr=192.168.1.10
serverip=192.168.1.1
netmask=255.255.255.0
bootfile="uImage"
phy_intf=mii,rgmii
use_mdio=0,1
phy_addr=2,1
gmac_debug=0
bootcmd=mmc read 0 0x1FFBFC0 0x50000 0x5000; bootm 0x1FFBFC0
factory_bootargs=console=ttyAMA0,115200 root=/dev/mmcblk0p16 rootfstype=ext3 rootwait blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs=console=ttyAMA0,115200 lpj=974848 quiet blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs_512M=mem=512M mmz=ddr,0,0,112M
bootargs_768M=mem=768M mmz=ddr,0,0,300M
bootargs_1G=mem=1G mmz=ddr,0,0,435M
bootargs_2G=mem=2G mmz=ddr,0,0,620M
signature_check=sign:recovery,recovery,0x200000 sign:kernel,kernel,0x700000
stdin=serial
stdout=serial
stderr=serial

Environment size: 1335/65532 bytes
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)

MMC write: dev # 0, block # 24576, count 1 ... 1 blocks written: OK
[EOT](OK)
Starting fastboot ...


System startup
DDRS
Reg Version:  v1.1.0
Reg Time:     2016/12/11 22:54:35
Reg Name:     hi3798mdmo1f_hi3798mv100_ddr3_1gbyte_16bitx2_2layers_emmc.reg

Jump to DDR


Fastboot 3.3.0-00007-gb5b796c-dirty (shaoqiang.yu@ubuntu) (Sep 18 2017 - 18:01:28)

Fastboot:      Version 3.3.0
Build Date:    Sep 18 2017, 18:02:23
CPU:           Hi3798Mv100 
Boot Media:    eMMC
DDR Size:      1GB

Check nand flash controller v610. found
Special NAND id table Version 1.36
Nand ID: 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00
No NAND device found!!!

MMC/SD controller initialization.
MMC/SD Card:
    MID:         0x15
    Read Block:  512 Bytes
    Write Block: 512 Bytes
    Chip Size:   3728M Bytes (High Capacity)
    Name:        "4FPD3"
    Chip Type:   MMC
    Version:     5.0
    Speed:       52000000Hz
    Bus Width:   8bit
    Boot Addr:   0 Bytes

Boot Env on eMMC
    Env Offset:          0x00100000
    Env Size:            0x00010000
    Env Range:           0x00010000
HI_OTP_LockIdWord,327: ID_WORD have already been locked
product_init,284
start download process.
bootdelay=0
verify=n
baudrate=115200
ipaddr=192.168.1.10
serverip=192.168.1.1
netmask=255.255.255.0
bootfile="uImage"
phy_intf=mii,rgmii
use_mdio=0,1
phy_addr=2,1
gmac_debug=0
bootcmd=mmc read 0 0x1FFBFC0 0x50000 0x5000; bootm 0x1FFBFC0
factory_bootargs=console=ttyAMA0,115200 root=/dev/mmcblk0p16 rootfstype=ext3 rootwait blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs=console=ttyAMA0,115200 lpj=974848 quiet blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs_512M=mem=512M mmz=ddr,0,0,112M
bootargs_768M=mem=768M mmz=ddr,0,0,300M
bootargs_1G=mem=1G mmz=ddr,0,0,435M
bootargs_2G=mem=2G mmz=ddr,0,0,620M
signature_check=sign:recovery,recovery,0x200000 sign:kernel,kernel,0x700000
stdin=serial
stdout=serial
stderr=serial

Environment size: 1335/65532 bytes
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)

MMC write: dev # 0, block # 24576, count 1 ... 1 blocks written: OK
[EOT](OK)
Starting fastboot ...


System startup
DDRS
Reg Version:  v1.1.0
Reg Time:     2016/12/11 22:54:35
Reg Name:     hi3798mdmo1f_hi3798mv100_ddr3_1gbyte_16bitx2_2layers_emmc.reg

Jump to DDR


Fastboot 3.3.0-00007-gb5b796c-dirty (shaoqiang.yu@ubuntu) (Sep 18 2017 - 18:01:28)

Fastboot:      Version 3.3.0
Build Date:    Sep 18 2017, 18:02:23
CPU:           Hi3798Mv100 
Boot Media:    eMMC
DDR Size:      1GB

Check nand flash controller v610. found
Special NAND id table Version 1.36
Nand ID: 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00
No NAND device found!!!

MMC/SD controller initialization.
MMC/SD Card:
    MID:         0x15
    Read Block:  512 Bytes
    Write Block: 512 Bytes
    Chip Size:   3728M Bytes (High Capacity)
    Name:        "4FPD3"
    Chip Type:   MMC
    Version:     5.0
    Speed:       52000000Hz
    Bus Width:   8bit
    Boot Addr:   0 Bytes

Boot Env on eMMC
    Env Offset:          0x00100000
    Env Size:            0x00010000
    Env Range:           0x00010000
HI_OTP_LockIdWord,327: ID_WORD have already been locked
product_init,284
start download process.
bootdelay=0
verify=n
baudrate=115200
ipaddr=192.168.1.10
serverip=192.168.1.1
netmask=255.255.255.0
bootfile="uImage"
phy_intf=mii,rgmii
use_mdio=0,1
phy_addr=2,1
gmac_debug=0
bootcmd=mmc read 0 0x1FFBFC0 0x50000 0x5000; bootm 0x1FFBFC0
factory_bootargs=console=ttyAMA0,115200 root=/dev/mmcblk0p16 rootfstype=ext3 rootwait blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs=console=ttyAMA0,115200 lpj=974848 quiet blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs_512M=mem=512M mmz=ddr,0,0,112M
bootargs_768M=mem=768M mmz=ddr,0,0,300M
bootargs_1G=mem=1G mmz=ddr,0,0,435M
bootargs_2G=mem=2G mmz=ddr,0,0,620M
signature_check=sign:recovery,recovery,0x200000 sign:kernel,kernel,0x700000
stdin=serial
stdout=serial
stderr=serial

Environment size: 1335/65532 bytes
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)

MMC write: dev # 0, block # 24576, count 1 ... 1 blocks written: OK
[EOT](OK)
ªªªªíýº°ªªªíýº°ªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªStarting fastboot ...


System startup
DDRS
Reg Version:  v1.1.0
Reg Time:     2016/12/11 22:54:35
Reg Name:     hi3798mdmo1f_hi3798mv100_ddr3_1gbyte_16bitx2_2layers_emmc.reg

Jump to DDR


Fastboot 3.3.0-00007-gb5b796c-dirty (shaoqiang.yu@ubuntu) (Sep 18 2017 - 18:01:28)

Fastboot:      Version 3.3.0
Build Date:    Sep 18 2017, 18:02:23
CPU:           Hi3798Mv100 
Boot Media:    eMMC
DDR Size:      1GB

Check nand flash controller v610. found
Special NAND id table Version 1.36
Nand ID: 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00
No NAND device found!!!

MMC/SD controller initialization.
MMC/SD Card:
    MID:         0x15
    Read Block:  512 Bytes
    Write Block: 512 Bytes
    Chip Size:   3728M Bytes (High Capacity)
    Name:        "4FPD3"
    Chip Type:   MMC
    Version:     5.0
    Speed:       52000000Hz
    Bus Width:   8bit
    Boot Addr:   0 Bytes

Boot Env on eMMC
    Env Offset:          0x00100000
    Env Size:            0x00010000
    Env Range:           0x00010000
HI_OTP_LockIdWord,327: ID_WORD have already been locked
product_init,284
start download process.
bootdelay=0
verify=n
baudrate=115200
ipaddr=192.168.1.10
serverip=192.168.1.1
netmask=255.255.255.0
bootfile="uImage"
phy_intf=mii,rgmii
use_mdio=0,1
phy_addr=2,1
gmac_debug=0
bootcmd=mmc read 0 0x1FFBFC0 0x50000 0x5000; bootm 0x1FFBFC0
factory_bootargs=console=ttyAMA0,115200 root=/dev/mmcblk0p16 rootfstype=ext3 rootwait blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs=console=ttyAMA0,115200 lpj=974848 quiet blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs_512M=mem=512M mmz=ddr,0,0,112M
bootargs_768M=mem=768M mmz=ddr,0,0,300M
bootargs_1G=mem=1G mmz=ddr,0,0,435M
bootargs_2G=mem=2G mmz=ddr,0,0,620M
signature_check=sign:recovery,recovery,0x200000 sign:kernel,kernel,0x700000
stdin=serial
stdout=serial
stderr=serial

Environment size: 1335/65532 bytes
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)

MMC write: dev # 0, block # 24576, count 1 ... 1 blocks written: OK
[EOT](OK)
Starting fastboot ...


System startup
DDRS
Reg Version:  v1.1.0
Reg Time:     2016/12/11 22:54:35
Reg Name:     hi3798mdmo1f_hi3798mv100_ddr3_1gbyte_16bitx2_2layers_emmc.reg

Jump to DDR


Fastboot 3.3.0-00007-gb5b796c-dirty (shaoqiang.yu@ubuntu) (Sep 18 2017 - 18:01:28)

Fastboot:      Version 3.3.0
Build Date:    Sep 18 2017, 18:02:23
CPU:           Hi3798Mv100 
Boot Media:    eMMC
DDR Size:      1GB

Check nand flash controller v610. found
Special NAND id table Version 1.36
Nand ID: 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00
No NAND device found!!!

MMC/SD controller initialization.
MMC/SD Card:
    MID:         0x15
    Read Block:  512 Bytes
    Write Block: 512 Bytes
    Chip Size:   3728M Bytes (High Capacity)
    Name:        "4FPD3"
    Chip Type:   MMC
    Version:     5.0
    Speed:       52000000Hz
    Bus Width:   8bit
    Boot Addr:   0 Bytes

Boot Env on eMMC
    Env Offset:          0x00100000
    Env Size:            0x00010000
    Env Range:           0x00010000
HI_OTP_LockIdWord,327: ID_WORD have already been locked
product_init,284
start download process.
bootdelay=0
verify=n
baudrate=115200
ipaddr=192.168.1.10
serverip=192.168.1.1
netmask=255.255.255.0
bootfile="uImage"
phy_intf=mii,rgmii
use_mdio=0,1
phy_addr=2,1
gmac_debug=0
bootcmd=mmc read 0 0x1FFBFC0 0x50000 0x5000; bootm 0x1FFBFC0
factory_bootargs=console=ttyAMA0,115200 root=/dev/mmcblk0p16 rootfstype=ext3 rootwait blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs=console=ttyAMA0,115200 lpj=974848 quiet blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs_512M=mem=512M mmz=ddr,0,0,112M
bootargs_768M=mem=768M mmz=ddr,0,0,300M
bootargs_1G=mem=1G mmz=ddr,0,0,435M
bootargs_2G=mem=2G mmz=ddr,0,0,620M
signature_check=sign:recovery,recovery,0x200000 sign:kernel,kernel,0x700000
stdin=serial
stdout=serial
stderr=serial

Environment size: 1335/65532 bytes
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)

MMC write: dev # 0, block # 24576, count 1 ... 1 blocks written: OK
[EOT](OK)
Starting fastboot ...


System startup
DDRS
Reg Version:  v1.1.0
Reg Time:     2016/12/11 22:54:35
Reg Name:     hi3798mdmo1f_hi3798mv100_ddr3_1gbyte_16bitx2_2layers_emmc.reg

Jump to DDR


Fastboot 3.3.0-00007-gb5b796c-dirty (shaoqiang.yu@ubuntu) (Sep 18 2017 - 18:01:28)

Fastboot:      Version 3.3.0
Build Date:    Sep 18 2017, 18:02:23
CPU:           Hi3798Mv100 
Boot Media:    eMMC
DDR Size:      1GB

Check nand flash controller v610. found
Special NAND id table Version 1.36
Nand ID: 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00
No NAND device found!!!

MMC/SD controller initialization.
MMC/SD Card:
    MID:         0x15
    Read Block:  512 Bytes
    Write Block: 512 Bytes
    Chip Size:   3728M Bytes (High Capacity)
    Name:        "4FPD3"
    Chip Type:   MMC
    Version:     5.0
    Speed:       52000000Hz
    Bus Width:   8bit
    Boot Addr:   0 Bytes

Boot Env on eMMC
    Env Offset:          0x00100000
    Env Size:            0x00010000
    Env Range:           0x00010000
HI_OTP_LockIdWord,327: ID_WORD have already been locked
product_init,284
start download process.
bootdelay=0
verify=n
baudrate=115200
ipaddr=192.168.1.10
serverip=192.168.1.1
netmask=255.255.255.0
bootfile="uImage"
phy_intf=mii,rgmii
use_mdio=0,1
phy_addr=2,1
gmac_debug=0
bootcmd=mmc read 0 0x1FFBFC0 0x50000 0x5000; bootm 0x1FFBFC0
factory_bootargs=console=ttyAMA0,115200 root=/dev/mmcblk0p16 rootfstype=ext3 rootwait blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs=console=ttyAMA0,115200 lpj=974848 quiet blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs_512M=mem=512M mmz=ddr,0,0,112M
bootargs_768M=mem=768M mmz=ddr,0,0,300M
bootargs_1G=mem=1G mmz=ddr,0,0,435M
bootargs_2G=mem=2G mmz=ddr,0,0,620M
signature_check=sign:recovery,recovery,0x200000 sign:kernel,kernel,0x700000
stdin=serial
stdout=serial
stderr=serial

Environment size: 1335/65532 bytes
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)

MMC write: dev # 0, block # 24576, count 1 ... 1 blocks written: OK
[EOT](OK)
ªªªíýº°ªªªªíýº°ªªíýº°ªªªªíýº°ªªíýº°ªªªªªªíýº°ªªªíýº°ªªªªíýº°ªªíýº°ªªªíýº°ªªªªíýº°ªªíýº°ªªªªªªíýº°ªªªªíýº°ªªíýº°ªªªªíýº°ªªíýº°ªªªªíýº°ªªªªªªíýº°ªªíýº°ªªªíýº°ªªªªíü™ ªªªªíýº°ªªªíýº°ªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªªStarting fastboot ...


System startup
DDRS
Reg Version:  v1.1.0
Reg Time:     2016-12-13 14:16:22
Reg Name:     hi3798mdmo1f_hi3798mv100_ddr3_768mbyte_16bitx2_2layers_emmc.reg

Jump to DDR


Fastboot 3.3.0-dirty (wentong.cen@tmajor) (Dec 15 2016 - 15:08:35)

Fastboot:      Version 3.3.0
Build Date:    Dec 15 2016, 15:09:30
CPU:           Hi3798Mv100 
Boot Media:    eMMC
DDR Size:      1GB

Check nand flash controller v610. found
Special NAND id table Version 1.36
Nand ID: 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00
No NAND device found!!!

MMC/SD controller initialization.
MMC/SD Card:
    MID:         0x15
    Read Block:  512 Bytes
    Write Block: 512 Bytes
    Chip Size:   3728M Bytes (High Capacity)
    Name:        "4FPD3"
    Chip Type:   MMC
    Version:     5.0
    Speed:       52000000Hz
    Bus Width:   8bit
    Boot Addr:   0 Bytes

Boot Env on eMMC
    Env Offset:          0x00100000
    Env Size:            0x00010000
    Env Range:           0x00010000
HI_OTP_LockIdWord,327: ID_WORD have already been locked
start download process.
bootdelay=0
verify=n
baudrate=115200
ipaddr=192.168.1.10
serverip=192.168.1.1
netmask=255.255.255.0
bootfile="uImage"
phy_intf=mii,rgmii
use_mdio=0,1
phy_addr=2,1
gmac_debug=0
bootcmd=mmc read 0 0x1FFBFC0 0x50000 0x5000; bootm 0x1FFBFC0
factory_bootargs=console=ttyAMA0,115200 root=/dev/mmcblk0p16 rootfstype=ext3 rootwait blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs=console=ttyAMA0,115200 lpj=974848 quiet blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs_512M=mem=512M mmz=ddr,0,0,112M
bootargs_768M=mem=768M mmz=ddr,0,0,300M
bootargs_1G=mem=1G mmz=ddr,0,0,435M
bootargs_2G=mem=2G mmz=ddr,0,0,620M
signature_check=sign:recovery,recovery,0x200000 sign:kernel,kernel,0x700000
stdin=serial
stdout=serial
stderr=serial

Environment size: 1335/65532 bytes
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)

MMC write: dev # 0, block # 24576, count 1 ... 1 blocks written: OK
[EOT](OK)
ªStarting fastboot ...


System startup
DDRS
Reg Version:  v1.1.0
Reg Time:     2016-12-13 14:16:22
Reg Name:     hi3798mdmo1f_hi3798mv100_ddr3_768mbyte_16bitx2_2layers_emmc.reg

Jump to DDR


Fastboot 3.3.0-dirty (wentong.cen@tmajor) (Dec 15 2016 - 15:08:35)

Fastboot:      Version 3.3.0
Build Date:    Dec 15 2016, 15:09:30
CPU:           Hi3798Mv100 
Boot Media:    eMMC
DDR Size:      1GB

Check nand flash controller v610. found
Special NAND id table Version 1.36
Nand ID: 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00
No NAND device found!!!

MMC/SD controller initialization.
MMC/SD Card:
    MID:         0x15
    Read Block:  512 Bytes
    Write Block: 512 Bytes
    Chip Size:   3728M Bytes (High Capacity)
    Name:        "4FPD3"
    Chip Type:   MMC
    Version:     5.0
    Speed:       52000000Hz
    Bus Width:   8bit
    Boot Addr:   0 Bytes

Boot Env on eMMC
    Env Offset:          0x00100000
    Env Size:            0x00010000
    Env Range:           0x00010000
HI_OTP_LockIdWord,327: ID_WORD have already been locked
start download process.
bootdelay=0
verify=n
baudrate=115200
ipaddr=192.168.1.10
serverip=192.168.1.1
netmask=255.255.255.0
bootfile="uImage"
phy_intf=mii,rgmii
use_mdio=0,1
phy_addr=2,1
gmac_debug=0
bootcmd=mmc read 0 0x1FFBFC0 0x50000 0x5000; bootm 0x1FFBFC0
factory_bootargs=console=ttyAMA0,115200 root=/dev/mmcblk0p16 rootfstype=ext3 rootwait blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs=console=ttyAMA0,115200 lpj=974848 quiet blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs_512M=mem=512M mmz=ddr,0,0,112M
bootargs_768M=mem=768M mmz=ddr,0,0,300M
bootargs_1G=mem=1G mmz=ddr,0,0,435M
bootargs_2G=mem=2G mmz=ddr,0,0,620M
signature_check=sign:recovery,recovery,0x200000 sign:kernel,kernel,0x700000
stdin=serial
stdout=serial
stderr=serial

Environment size: 1335/65532 bytes
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)

MMC write: dev # 0, block # 24576, count 1 ... 1 blocks written: OK
[EOT](OK)
Starting fastboot ...


System startup
DDRS
Reg Version:  v1.1.0
Reg Time:     2016-12-13 14:16:22
Reg Name:     hi3798mdmo1f_hi3798mv100_ddr3_768mbyte_16bitx2_2layers_emmc.reg

Jump to DDR


Fastboot 3.3.0-dirty (wentong.cen@tmajor) (Dec 15 2016 - 15:08:35)

Fastboot:      Version 3.3.0
Build Date:    Dec 15 2016, 15:09:30
CPU:           Hi3798Mv100 
Boot Media:    eMMC
DDR Size:      1GB

Check nand flash controller v610. found
Special NAND id table Version 1.36
Nand ID: 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00
No NAND device found!!!

MMC/SD controller initialization.
MMC/SD Card:
    MID:         0x15
    Read Block:  512 Bytes
    Write Block: 512 Bytes
    Chip Size:   3728M Bytes (High Capacity)
    Name:        "4FPD3"
    Chip Type:   MMC
    Version:     5.0
    Speed:       52000000Hz
    Bus Width:   8bit
    Boot Addr:   0 Bytes

Boot Env on eMMC
    Env Offset:          0x00100000
    Env Size:            0x00010000
    Env Range:           0x00010000
HI_OTP_LockIdWord,327: ID_WORD have already been locked
start download process.
bootdelay=0
verify=n
baudrate=115200
ipaddr=192.168.1.10
serverip=192.168.1.1
netmask=255.255.255.0
bootfile="uImage"
phy_intf=mii,rgmii
use_mdio=0,1
phy_addr=2,1
gmac_debug=0
bootcmd=mmc read 0 0x1FFBFC0 0x50000 0x5000; bootm 0x1FFBFC0
factory_bootargs=console=ttyAMA0,115200 root=/dev/mmcblk0p16 rootfstype=ext3 rootwait blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs=console=ttyAMA0,115200 lpj=974848 quiet blkdevparts=mmcblk0:1M(fastboot),1M(bootargs),10M(recovery),2M(deviceinfo),8M(baseparam),8M(pqparam),20M(logo),20M(logobak),10M(loaderdb),40M(fastplay),40M(fastplaybak),40M(kernel),20M(misc),1M(stbid),10M(fackernel),100M(facrootbox),8M(userapi),8M(hibdrv),8M(qbflag),300M(qbdata),600M(cache),700M(system),50M(keydata),-(userdata) coherent_pool=1M
bootargs_512M=mem=512M mmz=ddr,0,0,112M
bootargs_768M=mem=768M mmz=ddr,0,0,300M
bootargs_1G=mem=1G mmz=ddr,0,0,435M
bootargs_2G=mem=2G mmz=ddr,0,0,620M
signature_check=sign:recovery,recovery,0x200000 sign:kernel,kernel,0x700000
stdin=serial
stdout=serial
stderr=serial

Environment size: 1335/65532 bytes
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)
[EOT](OK)

MMC write: dev # 0, block # 24576, count 1 ... 1 blocks written: OK
[EOT](OK)
