Caterpillar 345 GC Excavator

Caterpillar 345 GC Excavator
354 Oakridge Lane, Camden NJ 08102 - USA
View or Download Brochure Favourite This Equipment
Description

##### Best Yanmar powered hydraulic excavator for rent.

Sed ut perspiciatis unde omnis iste natus error sit voluptatem accusantium dolore mque laud antium, totam rem aperiam, eaque ipsa quae ab illo inventore veritatis et quasi architecto be atae vitae dicta sunt explicabo. Nemo enim ipsam voluptatem quia voluptas sit aspernatur aut odit aut fugit, sed quia consequuntur magni dolores.

Eos qui ratione voluptatem sequi nesciunt. Neque porro quisquam es qui dolorem ipsum quia dolor sit amet consectetur, adipisci velit sed quia non numquam eius modiy.

- Nostrud exercitation ullamco laboris
- Ut aliquip ex ea reprehen deritin voluptate
- Adipisicing elit sed eiusmod tempor incididunt
- Labore dolore magna aliqua veniam nostrud

Specification

Weight: | 5710kg
Rated power: | 36.9kW / 2200rpm
Standard bucket capacity: | 0.2m3
Standard bucket width: | 775mm
Operation Hydraulic Pressure: | 24.5Mpa
Maximum Digging Force: | 37.4kN
Gradeadility: | 30°
Pressure To The Ground: | 31.4kPa
Walking Speed: | 2.8/4.7 km/h
Maximum Hauling Force: | 44kN
Swing Speed Of Platform: | 10.4 rpm

$250.00Per day
Dates are available
$250.00Per day
Dates are available

- Total Rent$580.00
- Owner Fee$90.00
- Govt. Taxes$45.50
- Total$715.00

We Help Industry To Utilize The
Heavy Equipment Work Better
Get Quick Support
236-799-5500
Get started