DynamipsGUI 1.6 README
First thanks to Chris.
Pardon my poor English.
Function List
1.use dynamips 0.2.6-RC2
2.support 9 routers and 9 switchs
3.support Frame-relay Switch and custom frame-relay switch,ATM Switch and Sim CCIE-BB.
4.auto calc bridge para,support bridge to two NIC
5.support 4 Rack 
6.creat bat files,and creat device support reload.
7.auto copy ios files to target dir
8.auto calc idle-pc
9.7200 type support PA-POS-OC3,ATM
10.support disconnect
11.support multi-language
12.any more para,please use ex: in ram input box 96 -X --disk0 4

DynamipsGUI 2.4 README
1.support 44 routers and 44 switchs
2.support distribute Dynamips (9 PCS)
3.support 2691,3725,3745,2610,2611,2620,2621,2610XM,2620XM,2650XM
4.use dynamips 0.2.7-RC2
5.support 10 nics to bridge 
6.add direct output
7.add linux output script
8.add Pemu
9.support Pemu communication with dynamips
10.add pemu win32
11.add VPCS 1.2.2 (virtual pc tools)
12.add BES 1.2.2

The multi-language use language.ini,you can translate it to any language.
Anyone can re-trans,this English version must have many syntax ERRER because of my poor English.
Modified language=EN or any other language.Then trans the text. 

any question and suggestion mailto:xiaofan4444@yahoo.com.cn
last update 2007-07-15
It will auto-install Winpcap 4.0 after intall.
