cenrep
version 1
[owner]
0x1020507E
[defaultmeta]
 0
[platsec]
 cap_rd=alwayspass
[Main]
0x1 int 1 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x2 int 10 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x3 int 0 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x4 int 10 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x5 int 1 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x6 int 10 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x7 int 10 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x8 int 10 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x9 int 10 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0xA int 30 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0xB int 10 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0xC int 30 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0xD int 10 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0xE int 100 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0xF int 10 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x10 int 30 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x11 int 10 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x12 int 30 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x13 int 30 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x14 int 30 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x15 int -5 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x16 int 50 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x17 int 10 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x18 int 30 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x19 int -5 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x1A int 50 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x1B int 20 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x1C int 30 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x1D int 10 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x1E int 30 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x1F int 10 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x20 int 30 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x21 int 50 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x22 int 30 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x23 int 10 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x24 int 30 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x25 int 20 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x26 int 10 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x27 int 5 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x28 int 30 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x29 int 10 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x2A int 30 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x2B int 10 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x2C int 30 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x2D int 10 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x2E int 300 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x2F int 30 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x30 int 300 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x31 int 30 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x32 int 300 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x33 int 12 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x34 int 150 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x35 int 30 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x36 int 300 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x37 int 10 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x38 int 50 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x39 int 30 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x3A int 300 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x3B int 30 0 cap_rd=alwayspass cap_wr=WriteDeviceData
0x3C int 300 0 cap_rd=alwayspass cap_wr=WriteDeviceData
