
          DigitalChina DCN-530TX Fast Ethernet Adapter
                    Diagnostic Program Usage

Starting the Program
====================

At the DOS prompt (not from Windows DOS shell), insert driver
disk, enter the following command to start the program:

   X:\DIAG\DCNTEST    <Enter>

Notice: X: means the floppy drive containing the driver,
        such as: A:, or B: etc.

If there is more than one adapter installed inside your PC,
please select the specific adapter from the "Select LAN Board"
menu to enter the Main Menu of the diagnostic program. After
entering this diagnostic program, there will show messages and
methods of using this tool.
