
        D-Link DFE-530TX PCI Fast Ethernet Adapter Installation
                 for NetWare Server v4.10, v4.11, v4.2 

 Contents
 --------
    - Compatibility List
    - Getting Started
       - First time installation from the install menu
       - The other time installation from the install menu
       - Modifying an existing NetWare 4.x Server

 Compatibility List
 ------------------
      Because this driver  follows  Novell  ODI  Driver Specification
      version 3.31, the NetWare version 4.10 NetWare server must be
      patched to work with this driver. The servers of NetWare version
      4.11 and above do not need to be patched. The patching method is
      described as below:

       1. Copy LOADER.EXE and LSWAP.EXE to the NetWare 4.10 server
          directory.

       2. Execute LSWAP.EXE at MS-DOS prompt from server directory.

          Usage: LSWAP [loaderFilePath [serverFilePath]]
                 Default loaderFilePath = C:\NWSERVER\LOADER.EXE
                 Default serverFilePath = C:\NWSERVER\SERVER.EXE

        PS. Both LSWAP.EXE and LOADER.EXE files provide by Novell.

       ****************************************************************
       Note: This ODI update is for English only.
       ****************************************************************

       Before installing, make sure the following items have been
       completed.

       410PTx.EXE (Where "x" is 6 or higher) must be installed on
       NetWare v4.10 file servers prior to installing ODI driver.
       Without this patch the following message may be displayed
       when NBI.NLM loads.

       "Warning: This version of NetWare does not support protected mode
       BIOS accesses. Without a loader patch some PCI drivers may fail."

 Getting Started
 ---------------
    First time installation from the install menu
    ---------------------------------------------
       1. Start the NetWare Server.

          > CD \NWSERVER
          > SERVER

       2. Execute "LOAD INSTALL" after booting up.  Type,
          : LOAD INSTALL

       3. Select "Driver Options", -> "Configure network drivers", and
          -> "Select a driver".

       4. Press <Insert> key to install an unlisted driver.

       5. Please insert release driver diskette into floppy disk.

       6. Press <F3> to specify a different <PATH>. <PATH> is directory
          which include both DLKFET.LAN and DLKFET.LDI

          Ex. A:\NETWARE\32BITLAN

       7. Select "DLKFET.LAN ....".

          Note: Please don't copy the NLM files to system, if disk's
                NLM files version older than system.

       8. Specify "SLOT", "Media and Line Speed" and "Node Address"
          if necessary.

       9. Select "Save parameters and load driver" after configure
          adapter setting.

       10. NetWare server will loading/binding driver automatically.


    The other time installation from the install menu
    -------------------------------------------------
        1. Start the NetWare Server.

           > CD \NWSERVER
           > SERVER

        2. Execute "LOAD INSTALL" after booting up.  Type,
           : LOAD INSTALL

        3. Select "Driver Options", -> "Configure network drivers", and
           -> "Select a driver".

        4. Select "DLKFET.LAN ...." in Select a driver windows.

        5. Specify "SLOT", "Media and Line Speed" and "Node Address"
           if necessary.

        6. Select "Save parameters and load driver" after configure adpter
           setting.

        7. NetWare server will loading/binding driver automatically.


    Modifying an existing NetWare 4.x Server
    ----------------------------------------
        1. Make a sub-directory NLMS.OLD under NWSERVER directory.

           Ex. >MD \NWSERVER\NLMs.OLD

        2. Save NBI.NLM, MSM.NLM and ETHERTSM.NLM to NLMS.OLD
           sub-directory. (v4.10, v4.11 server only)

        3. Please insert release driver diskette into floppy disk.

        4. Copy all provided NLM and LAN files into your dos directory
           which include SERVER.EXE. (v4.10, v4.11 server only)

            Ex. >COPY A:\NETWARE\32BITLAN\NBI.NLM      C:\NWSERVER
                >COPY A:\NETWARE\32BITLAN\MSM.NLM      C:\NWSERVER
                >COPY A:\NETWARE\32BITLAN\ETHERTSM.NLM C:\NWSERVER
                >COPY A:\NETWARE\32BITLAN\DLKFET.LAN   C:\NWSERVER
                >COPY A:\NETWARE\32BITLAN\DLKFET.LDI   C:\NWSERVER

           <PATH> here is the directory where support NLMs and
           DLKFET.LAN reside.

        5. Start the NetWare Server.

            > CD \NWSERVER
            > SERVER

        6. From the Novell Server side, execute "LOAD INSTALL".  Type:
           :LOAD INSTALL
           Select <NCF files options>
           Select <Edit AUTOEXEC.NCF file>

        7. Add below item into the server's AUTOEXEC.NCF file.

           LOAD C:\NWSERVER\NBI.NLM
           LOAD C:\NWSERVER\MSM.NLM
           LOAD C:\NWSERVER\ETHERTSM.NLM

           LOAD C:\NWSERVER\DLKFET SLOT=1 FRAME=Ethernet_802.3
                NAME=DLKFET_1_E83
           BIND IPX DLKFET_1_E83 NET=xxxx

           LOAD C:\NWSERVER\DLKFET SLOT=1 FRAME=Ethernet_802.2
                NAME=DLKFET_1_E82
           BIND IPX DLKFET_1_E82 NET=xxxx

           LOAD C:\NWSERVER\DLKFET SLOT=1 FRAME=Ethernet_II
                NAME=DLKFET_1_EII
           BIND IPX DLKFET_1_EII NET=xxxx

           LOAD C:\NWSERVER\DLKFET SLOT=1 FRAME=Ethernet_SNAP
                NAME=DLKFET_1_ESP
           BIND IPX DLKFET_1_ESP NET=xxxx

       8. Restart the server again.


       Parameters supported by the DLKFET.LAN driver
       ---------------------------------------------
       SLOT     1      - Forces the driver to search for the specified board

       AUTOSENSE       - This keyword configures the adapter to conduct
                         NWay Auto-negotiation to determine the network
                         speed and the duplex mode of the network connection.

       10BASET         - Force driver to 10Mbps half duplex mode.

       10BASETFD       - Force driver to 10Mbps full duplex mode.

       100BASETX       - Force driver to 100Mbps half duplex mode.

       100BASETXFD     - Force driver to 100Mbps full duplex mode.


