
          DigitalChina DCN-530TX Fast Ethernet Adapter
               Windows 95 OSR2 Driver Installation

  Contents:
  ---------
   (A) Installing the driver in Microsoft Windows 95 OSR2
   (B) Configuring the driver in Microsoft Windows 95 OSR2
   
(A) Installing the driver in Microsoft Windows 95 OSR2
================================================================
Notice: The Windows 95 OSR2 installation CD are needed to
        complete this install.

    1. Make sure your computer is power-off.
    2. Plug the adapter into one of the PCI slots of your PC.
    3. Turn the power ON, then boot into Windows 95 OSR2.
    4. Windows 95 will find the new hardware automatically, then
       "Update Device Driver Wizard" dialog box will appear.
    5. Insert the Driver Diskette and click the "Next >" button.
    6. A screen will appear stating that Windows 95 OSR2 was
       unable to locate the driver. Click "Other Locations..."
       button.
    7. Type Path "X:\WIN95SR2" in the text box, then click "OK".

      Notice: X: means the floppy drive containing the drivers,
      such as: A:, or B: etc.

    8. Windows 95 OSR2 will prompt with "DigitalChina DCN-530TX
       Fast Ethernet Adapter" in the dialog box.
    9. Click the "Finish" button, then Windows 95 OSR2 will copy
       the driver.

       Notice: During this copying procedure, Windows 95 OSR2
               may request for Windows 95 OSR2 installation CD.

       1)When Windows 95 OSR2 asks for the "DigitalChina
         DCN-530TX Fast Ethernet Adapter Driver Diskette",
         click "OK".
       2)When Windows 95 OSR2 prompts a "Copying Files..."
         dialog box asking for "DCN530N4.SYS", type
         "X:\WIN95SR2" in the text box, then click "OK".
	     
	     Notice: X: means the floppy drive with driver disk,
                 such as: A:, or B: etc.
       3)When Windows 95 OSR2 asks for the "Windows 95 CD-ROM",
         click "OK".
       4)When Windows 95 OSR2 prompts a "Copying Files..."
         dialog box asking for files on Windows 95 CD-ROM, type
         "X:\WIN95" in the text box, then click "OK".
	     
	     Notice: X: means CD-ROM drive with Windows 95 CD-ROM,
                 such as: D:, or E: etc.
       
   10. After finishing file copying, Windows 95 OSR2 will ask
       you to restart the system. Remove the Driver Diskette
       and click "Yes" to reboot.

(B) Configuring the driver on Microsoft Windows 95 OSR2
================================================================

    1. Double click the "My Computer" icon.
    2. Double click the "Control Panel" icon.
    3. Double click the "Network" icon.
    4. Select the "DigitalChina DCN-530TX Fast Ethernet Adapter"
       item, then click the "Properties" button.
    5. Click the "Advanced" tab.
    6. There are 1 items in the "Property" box.

       ------Media Type      
       .Specify the media type for the adapter.
       .Default: AutoSense
       
    7. Click "OK" button to return to "Network" dialog box.
    8. Click "OK" button and restart your PC to make the new
       configuration take effect.

Trademarks:
Microsoft Windows 95 OSR2 is a trademark of Microsoft Corporation.


