
          DigitalChina DCN-530TX Fast Ethernet Adapter
                 UnixWare7 Driver Installation

  Contents:
  ---------
   
   (A) Installing the driver on UnixWare 7
   (B) Configuring the driver on UnixWare 7

(A) Installing the driver on UnixWare 7
================================================================
Notice: Please strictly follow the case of those commands and
        files' name, because UnixWare 7 is case-sensitive.

    1. Login to UNIX system as supervisor (root).
    2. Please follow the following steps to copy the package file:
       (1)Insert the driver disk.
       (2)Mount the floppy disk by the following command:
      
          # mount -F dosfs /dev/fd0 /mnt
      
       (3)Copy the driver package file to /tmp directory.
   
          # cp /mnt/UW7/DCN530.PKG /tmp

    3. Install the driver package by following command:
   
       # pkgadd -d /tmp/DCN530.PKG

    4. Select the number of "d53n" and press <ENTER>.
    5. After package is added, run "netcfg".

       # netcfg

    6. Choose from menu "Hardware"->"Add new LAN adapter...".
    7. UnixWare 7 will automatically find the adapter and prompt
       "Ethernet-DigitalChina DCN-530TX Fast Ethernet
       Adapter(1.0)". Click "Continue".
    8. Choose required Link Mode from the "Network Driver
       Configuration" dialog box and click "OK".
    9. Choose your required protocol from the "Add Protocol"
       dialog box and continue to set your networking
       configuration. Refer to related document in UnixWare 7
       for detail.
   10. After configuration is completed, a "Configure networking
       product" dialog box will appear to indicate successful
       configuration. Click "OK".
   11. "DigitalChina DCN-530TX Fast Ethernet Adapter" will be
       added to the list.
   12. Exit "Network Configuration Manager" and reboot system to
       make new configuration effect.

(B) Configuring the driver on UnixWare 7
================================================================
    1. Login to UNIX system as supervisor (root).
    2. Run "netcfg".

       # netcfg
       
    3. Highlight "DigitalChina DCN-530TX Fast Ethernet Adapter".
    4. Select from menu
       "Hardware"->"modify hardware configuration...".
    5. Choose required Link Mode from the "Network Driver
       Configuration" dialog box and click "OK".
    6. After configuration, a "Configure networking product"
       dialog box will appear to indicate successful
       configuration. Click "OK".
    7. Exit "Network Configuration Manager" and reboot system to
       make new configuration effect.
