
           D-Link DFE-530TX PCI Fast Ethernet Adapter Installation
                     for the NetWare Server 5.0 Driver

 Contents
 --------
    -Getting Started
        -First time installation from the install menu
        -The other time installation from the install menu
        
 Getting Started
 ---------------

    First time installation from the install menu
    ----------------------------------------------------
        - Start the NetWare Server.

          > CD \NWSERVER
          > SERVER

        - Execute "NWCONFIG" after booting up.  Type,
          : NWCONFIG

        - Select "Driver Options", -> "Configure network drivers", and
          -> "Select a driver".

        - Press <Insert> key to install an unlisted driver.

        -  Please insert released driver CD into CD-ROM drive.

        - Press <Enter> key to continue install or press <F3> to specify
          the directory which includes DLKFET.LDI, DLKFET.LAN.

          Ex. <CD drive>:\NETWARE\32BITLAN

        - Select "DLKFET.LAN ....".

          Note: Please don't copy the NLM files to system, if disk's
                NLM files version older than system.

        - Specify "SLOT", "Node Address", "Media and Line Speed", and 
	  "Flow control ability" if necessary.

        - Select "Save parameters and load driver" after configuring
          adapter setting.

        - NetWare server will load/bind driver automatically.


    The other time installation from the install menu
    ----------------------------------------------------
        - Start the NetWare Server.

          > CD \NWSERVER
          > SERVER

        - Execute "NWCONFIG" after booting up.  Type,
          : NWCONFIG

        - Select "Driver Options", -> "Configure network drivers", and
          -> "Select a driver".

        - Select "DLKFET.LAN ...." in Select a driver windows.

        - Specify "SLOT", "Media and Line Speed" and "Node Address"
          if necessary.

        - Select "Save parameters and load driver" after configuring adpter
          setting.

        - NetWare server will load/bind driver automatically.
   
       Parameters supported by the DLKFET.LAN driver

        The following keywords are for driver v5.10 or later.
        ----------------------------------------------------------------
        CONNECTIONTYPE                  This keyword is used to specify media type.
        
            CONNECTIONTYPE=AutoSense
            CONNECTIONTYPE=10BASET
            CONNECTIONTYPE=10BASETFD
            CONNECTIONTYPE=100BASETX
            CONNECTIONTYPE=100BASETXFD
            
        FLOW_CONTROL                    This keyword is used to specify flow control
                                        ability.(Not supported in force mode)
            FLOW_CONTROL=DISABLE
            FLOW_CONTROL=ENABLE
            FLOW_CONTROL=HARDWARE_DEFAULT   (default)
        

	The following keywords are for driver v5.10 previously(v5.10 not included).
        ------------------------------------------------------------------------	
        SLOT     1      - Force the driver to search for the specified board

        AUTOSENSE       - This keyword configures the adapter to conduct
                          NWay Auto-negotiation to determine the network
                          speed and the duplex mode of the network connection.

        10BASET         - Force driver to 10Mbps half duplex mode.

        10BASETFD       - Force driver to 10Mbps full duplex mode.

        100BASETX       - Force driver to 100Mbps half duplex mode.

        100BASETXFD     - Force driver to 100Mbps full duplex mode.
            
 



