
          DigitalChina DCN-530TX Fast Ethernet Adapter
              NetWare DOS ODI Driver installation

  Contents:
  ---------
  (A) Installation Procedure
  (B) Configuration Files

(A) Installation Procedure
================================================================
  1. Assume you have finished installing the NetWare Client 
     for DOS on your computer, and the path you installed it
     is "C:\NWCLIENT".

  2. Copy the X:\NETWARE\DOSODI\DCNODI.COM file to the Netware
     client directory "C:\NWCLIENT".

     Notice: X: means the floppy drive containing the driver,
             such as: A:, or B: etc.

  3. Copy the X:\NETWARE\DOSODI\NET.CFG file to the Netware
     client directory "C:\NWCLIENT" and overwrite the existing
     NET.CFG.

     Notice: X: means the floppy drive containing the driver,
             such as: A:, or B: etc.

  4. Make sure to add LASTDRIVE=Z in your CONFIG.SYS file.

  5. Enter the following commands to connect to your Novell
     server:
             LSL
             DCNODI
             IPXODI
             VLM
             F:
             LOGIN <user_name>


(B) Configuration Files
================================================================  
  File Name:            NET.CFG

  Sample of configuration file:
-----------------------------------------------------------------------------
Link Driver DCNODI
    FRAME Ethernet_802.2
    FRAME Ethernet_802.3
    FRAME Ethernet_SNAP
    FRAME Ethernet_II

;       No_Early_Rx_Interrupt_Enable
;       Node address      0200e8123456
;       FORCE_MEDIA
;       Connection_Type = 10MFD ; 10M 10MFD 100M 100MFD, default is AUTO
        TX_THRESHOLD    = 0     ; 0..3, 4=Store and forward, default=0
        RX_THRESHOLD    = 1     ; 0..2, 2=Store and forward, default=1
        CAL             = 2     ; 0..3, default = 2
        PBL             = 10    ; 0,1,2,4,8,10,20, default = 10
        Rx_Buffer_Size  = 100   ; Hex number, 100-600
;       Slot  1
        RX_FIFO_SIZE    = 2     ; 0..2, 0 ~ 2:2K, 3:1K; 0 is default

NetWare DOS Requester
        FIRST NETWORK DRIVE = F
        NETWARE PROTOCOL = NDS BIND
;       MAX IPG = 0
;       PBURST READ WINDOW SIZE=45
;       PBURST WRITE WINDOW SIZE=45
-----------------------------------------------------------------------------

All trademarks and brand names mentioned belong to their respective owners.
