
          DigitalChina DCN-530TX Fast Ethernet Adapter
              SCO OpenServer 5 Driver Installation

  Contents:
  ---------
   
   (A) Installing the driver on SCO OpenServer 5
   (B) Configuring the driver on SCO OpenServer 5

(A) Installing the driver on SCO OpenServer 5
================================================================
Notice: Please strictly follow the case of those commands and
        files' name, because SCO OpenServer 5 is case-sensitive.

    1. Login to UNIX system as supervisor (root).
    2. Follow the following steps to copy the package file:
       (1)Insert the driver disk.
       (2)Copy the driver package file to /tmp directory.
      
          # doscp X:/SCO5/DCN530.IMG /tmp/VOL.000.000

          Notice: X: means the floppy drive with driver disk,
                  such as: A:, or B: etc.
    3. Install the driver package.
       (1)Run "custom" utility.
       (2)Select menu "Software" -> "Install New...".
       (3)Select "From <host name>", it should be the first
          option. Then click "Continue".
      
          Notice: <host name> is the actual host name of your
                  SCO OpenServer.

       (4)Select "Media Image" in "Media Device" pull-down menu
          and click "Continue".
       (5)Enter the path "/tmp" containing the driver package
          (VOL.000.000) in the "Image Directory" box.
       (6)It will prompt with "DigitalChina DCN-530TX Device
          Driver(ver 1.0.0)", click "Install".
       (7)When system prompts "installation complete",
          click "OK".
       (8)"DigitalChina DCN-530TX Device Driver(ver 1.0.0)" will
          be added to the software list.
       (9)Exit "custom".
    4. Install the adapter.
       (1)Run "netconfig".
      
          # netconfig
       
       (2)Select from menu "Hardware"->"Add new LAN adapter...".
       (3)SCO OpenServer 5 will automatically find the adapter
          and prompt "DigitalChina DCN-530TX Fast Ethernet
          Adapter Compatible". Click "Continue".
       (4)Choose required protocol from the "Add Protocol"
          dialog box and continue to set your networking
          configuration. Refer to related document in SCO Open
          Server 5.
       (5)After configuration, a "Configure networking product"
          dialog box will appear to indicate successful
          configuration. Click "OK".
       (6)"DigitalChina DCN-530TX Fast Ethernet Adapter
          Compatible" will be added to the hardware list.
       (7)Exit "Network Configuration Manager".
       (8)Click "Yes" when asking "Do you want to re-link the
          kernel now?".
       (9)Type "y" and press <ENTER> when asking "Do you want
          this kernel to boot by default? (y/n)".
      (10)Type "y" and Press <ENTER> when asking "Do you want
          the kernel environment rebuilt? (y/n)".
      (11)Press <ENTER> when re-link is completed.
    5. Reboot system to make new configuration effect.

(B) Configuring the driver on SCO OpenServer 5
================================================================
    1. Login to UNIX system as supervisor (root).
    2. Run "netconfig".

       # netconfig
       
    3. Highlight "DigitalChina DCN-530TX Fast Ethernet Adapter".
    4. Choose from menu
       "Hardware"->"modify hardware configuration".
    5. Choose required Link Mode and click "OK".
    6. When asking "Please verify adapter is set to the
       configuration just entered", click "OK".
    7. After configuration, a "Configure networking product"
       dialog box will appear to indicate successful
       configuration. Click "OK".
    8. Exit "Network Configuration Manager".
    9. Click "Yes" when asking "Do you want to re-link the
       kernel now?".
   10. Type "y" and Press <ENTER> when asking "Do you want this
       kernel to boot by default? (y/n)".
   11. Type "y" and Press <ENTER> when asking "Do you want the
       kernel environment rebuilt? (y/n)".
   12. Press <ENTER> when re-link is finished.
   13. Reboot system to make new configuration effect.
