
        D-Link DFE-530TX PCI Fast Ethernet Adapter Installation
                  for NetWare Server v3.12, v3.2

 Contents
 --------
    - Getting Started

 Getting Started
 ---------------

    Modifying an existing NetWare 3.12/3.2 Server
    ---------------------------------------------
       1. Make a sub-directory NLMS.OLD under <SRVPATH> directory which
          include SERVER.EXE.

          Ex. <SRVPATH> = NWSERVER
              >MD \NWSERVER\NLMs.OLD

       2. Save NBI31X.NLM, MSM31X.NLM and ETHERTSM.NLM to NLMS.OLD
          sub-directory. (v3.12 server only)
	  
       3. Get following files from NOVELL website and put them in floppy disk.
		
		ETHERTSM.NLM        Patch file for Netware 3.12 Server (v3.80).
    		MSM31X.NLM          Patch file for Netware 3.12 Server (v3.95).
    		NBI31X.NLM          Patch file for Netware 3.12 Server (v2.25).

       4. Please insert release driver CD into CD-ROM drive.
						
       5. Copy all provided NLM and LAN files into your dos directory
          which includes SERVER.EXE. (v3.12 server only)

          Ex. >COPY <Floppy drive>:\NBI31X.NLM   C:\SERVER.312
              >COPY <Floppy drive>:\MSM31X.NLM   C:\SERVER.312
              >COPY <Floppy drive>:\ETHERTSM.NLM C:\SERVER.312
              >COPY <CD drive>:\NETWARE\32BITLAN\DLKFET.LAN   C:\SERVER.312

       6. Start the NetWare Server.

          > CD \NWSERVER
          > SERVER

       7. From the Novell Server side, execute "LOAD INSTALL". Type:
          :LOAD INSTALL
           Select <System Option>
           Select <Edit Autoexec.NCF file>

       8. Add below item into the server's AUTOEXEC.NCF file.

          LOAD C:\NWSERVER\NBI31X.NLM
          LOAD C:\NWSERVER\MSM31X.NLM
          LOAD C:\NWSERVER\ETHERTSM.NLM

          LOAD C:\NWSERVER\DLKFET SLOT=1 FRAME=Ethernet_802.3
               NAME=DLKFET_1_E83
          BIND IPX DLKFET_1_E83 NET=xxxx

          LOAD C:\NWSERVER\DLKFET SLOT=1 FRAME=Ethernet_802.2
               NAME=DLKFET_1_E82
          BIND IPX DLKFET_1_E82 NET=xxxx

          LOAD C:\NWSERVER\DLKFET SLOT=1 FRAME=Ethernet_II
               NAME=DLKFET_1_EII
          BIND IPX DLKFET_1_EII NET=xxxx

          LOAD C:\NWSERVER\DLKFET SLOT=1 FRAME=Ethernet_SNAP
               NAME=DLKFET_1_ESP
          BIND IPX DLKFET_1_ESP NET=xxxx

       9. Restart the server again.


       Parameters supported by the DLKFET.LAN driver

        The following keywords are for driver v5.10 or later.
        ----------------------------------------------------------------
        CONNECTIONTYPE                  This keyword is used to specify media type.
        
            CONNECTIONTYPE=AutoSense
            CONNECTIONTYPE=10BASET
            CONNECTIONTYPE=10BASETFD
            CONNECTIONTYPE=100BASETX
            CONNECTIONTYPE=100BASETXFD
            
        FLOW_CONTROL                    This keyword is used to specify flow control
                                        ability.(Not supported in force mode)
            FLOW_CONTROL=DISABLE
            FLOW_CONTROL=ENABLE
            FLOW_CONTROL=HARDWARE_DEFAULT   (default)
        

	The following keywords are for driver v5.10 previously(v5.10 not included).
        ------------------------------------------------------------------------	
        SLOT     1      - Forces the driver to search for the specified board

        AUTOSENSE       - This keyword configures the adapter to conduct
                          NWay Auto-negotiation to determine the network
                          speed and the duplex mode of the network connection.

        10BASET         - Force driver to 10Mbps half duplex mode.

        10BASETFD       - Force driver to 10Mbps full duplex mode.

        100BASETX       - Force driver to 100Mbps half duplex mode.

        100BASETXFD     - Force driver to 100Mbps full duplex mode.
            

