
 ALCOR Recovery Tool V.1.0.0.14 build T-L0703 by tagaraz.

 Инструкцию по ремонту флешек на контроллере  ALCOR AU69xx и клонов  FC8x08, SCx08 можно скачать по
 адресу:  http://www.flashboot.ru/forum/index.php?topic=1293.0
---------------------------------------------------------------------------------------------------

 Список изменений build T-L0703 by tagaraz:

- обновлены прошивки (новые версии + дополнительные) в каталоге 98 для контроллеров 6989\6998:

- обновлены прошивки в каталоге 90 для контроллеров 6990

--------------------------------------------------------------------------------------------------

      Замечания по версии ALCOR Recovery Tool V.1.0.0.14 build T-L0703.

  С помощью данной утилиты  были протестированы  флешки Transcend на контроллерах AU6986, AU6990 и 
AU6998N, успешно  созданы  как обычный (единственный)  раздел, так и CD-раздел + обычный раздел. В
процессе проверки, для успешного завершения работы производственной утилиты, некоторые параметры в
настройках  ALCOR Recovery Tool приходилось менять при подключении флешек с другими контроллерами.
Производственная  утилита построена таким образом что процесс прошивки флешки прерывается в случае
обнаружения некорректного (или неподдерживаемого) параметра или  режима и  выводится  сообщение об
ошибке.  По информации, сопровождающей ошибку, необходимо  подкорректировать настройки в утилите и
попытаться снова обработать флешку. Перед запуском утилиты, необходимо вернуть "нормальный" статус
устройства (флешки) в окне где перед этим была отображена ошибка,  для чего нажать кнопку Refresh,
если кнопка Refresh неактивна, то необходимо нажать STOP.

  В каталоге Import_TS находятся конфигурационные файлы настроек флешек Transcend на  контроллерах

AU6986 (TS4GJFV33) : TS4G_6986.ini,
AU6990 (TS4GJF600) : TS4G_6990.ini,
AU6990 (TS16GJF620): TS16G_6990.ini,

для восстановления обычного раздела флешки. Чтобы загрузить любую из указанных настроек,необходимо
нажать кнопку Setup и Import, в открывшемся  окне  Import MP Job Files  войти в каталог  Import_TS
и указать имя файла настроек,  подтвердить выбор кнопкой  "Открыть" , после чего закрыть утилиту с 
сохранением изменений и снова запустить утилиту для дальнейших настроек согласно типу вашей флешки.  
  
  Для контроллера  AU6989(N\NL)  необходимо  указать  использование CTL: AU6998(N\NL), совместимые
прошивки находятся в каталоге \98.     
  
==================================================================================================
 05 May 2012   SP:2012-05-05  by nat27      http://www.flashboot.ru/forum/index.php?topic=1293.0
==================================================================================================
 03 Jul 2012   build T-L0703  by tagaraz    http://www.usbdev.ru
==================================================================================================



Error Code 	Definition
-----------------------------------------------------------------------------------

0x0E		RESET_ERROR
0x1E		TOO_MANY_BAD_BLOCK        
0x2E		CIS_ERROR
0x3E		RW_ERROR
0x4E		MBR_ERROR
0xAE		CHECK_BOOT_ERROR
0xBE		READ_CAPACITY_ERROR   
0xCE		GET_FLASH_ID_ERROR
0xDE		UNKWONW_FLASH_ERROR
0xFE		CHANNEL_MODE_ERROR
0x01FE		SET_CHANNEL_MODE_ERROR
0x02FE		SUPPORT_CHANNEL_ERROR
0x03FE		MISS_DAT_ERROR
0x04FE		GET_BLOCK0_ERROR
0x05FE		GET_RENBLOCK0_ERROR
0x06FE		ERASE_CMD_ERROR
0x07FE		ERASE_BLOCK0_ERROR
0x08FE		MISS_BIN_ERROR
0x09FE		WRITE_SCRIPT_ERROR
0x0AFE		READ_SCRIPT_ERROR
0x0BFE		READ_BINARY_FILE_ERROR
0x0CFE		WRITE_BINARY_ERROR
0x0DFE		READ_BINARY_ERROR
0x0EFE		WRITE_FW_ERROR
0x0FFE		READ_BLK_ADDRESS_ERROR
0x1FFE		COMPARE_BLK_ADDRESS_ERROR
0x2FFE		COMPARE_SCRIPT_ERROR
0x3FFE		READ_FLASHCODE_ERROR
0x4FFE		COMPARE_FLASHCODE_ERROR
0x5FFE		LOAD_FWCODE_ERROR
0x6FFE		INITIAL_FW_ERROR
0x7FFE		BINARY_CORRUPT_ERROR
0x8FFE		CHECK_DUALDIE_ERROR
0x9FFE		WRONG_FLASH_ERROR
0xAFFE		WRONG_MINIMUM_BADBLOCK
0xBFFE		INITIAL_SIZE_ERROR        
0xE0		MODE_ERROR
0xE1		DEFAULT_SIZE_ERROR
0xE2		PASSWORD_ERROR
0xE3		PASSWORD_1M_ERROR
0xE4		FLASH_SIZE_ERROR
0xE5		BOOT_SECTOR_ERROR
0xE6		FAT_ERROR
0xE7		ROOT_SECTOR_ERROR
0xE8		WRITE_LOADER_ERROR
0xE9		WRITE_RESERVE_ERROR
0xEA		LOADER_SIZE_ERROR
0xEB		CHECK_CONFIG_ERROR
0xEC		CHECK_LOADER_ERROR
0xED		CHECK_RESERVE_ERROR                                
0xEE		WRITE_FILE_ERROR
0xEF		BAD_BLOCK_ERROR
0xFF		GET_HANDLE_ERROR
0xE001		E_WRITE_BAD_BLOCK_TALBE_MAP
0xE002		E_READ_BAD_BLOCK_TALBE_MAP
0xE003		E_NOT_SUPPORT_EIGHT_OVER_DIES
0xE004		E_GET_BLOCK_TABLE_MAP
0xE005		E_GENERATE_MAP_CHECK_SUM
0xE006		E_WRITE_MAP_CHECK_SUM
0xE007		E_READ_MAP_CHECK_SUM
0xE008		E_MAP_CHECK_SUM
0xE009		E_WRITE_BAD_BLOCK_TABLE_FROM_MAP
0xE00A		E_CLEAN_BAD_BLOCK_MAP_BLOCK
0xE00B		E_MARK_DEFAULT_BAD_BLOCK
0xE00C		E_BAD_BLOCK_TABLE_MAP_VERIFY
0xE010		E_COPY_CUSTOM_FOLDER
0xE201		E_INVALID_SIZE_WITH_SPEC
0xE300		PHY_WRITE
0xE301		PHY_READ
0xE302		COMPARE_CONFIG_ERROR
0xE303		COMPARE_FIRMWARE_ERROR
0xE305		COMPARE_BADBLOCKTABLE_ERROR
0xE306		NO_AVAILABLE_FIRMWARE_BLOBK
0xE39A		E_READ_ROM_VERSION
0xE401		E_LLF_READ_PATTERN_SOURCE
0xE501		E_CONTROLLER_NO_SUPPORT
0xE502		E_READ_BUFFER
0xE503		E_WRITE_BUFFER
0xE505		E_ERASE_BLOCK_LOW
0xE508		E_PHYREAD_BUFFER
0xE509		E_FLASH_NO_SUPPORT
0xE50A		E_CHECK_MAPPING_TABLE

-----------------------------------------------------------------------------------

READ_ORIGINALCAPACITY	Read Flash Capacity Fail
WRITEPROTECT		Device Write Protect
ERASE_SERIAL_NO		Erase SN Fail
PASSWORD_ERROR		Clean Password Fail
GETCHIPNUMBER		Get Chip Number Vendor Command Fail
SELECT_FUNCTION		Select Function Vendor Command Fail
LOADER_SIZE_ERROR	The loader Size is conflict with actual Flash size
FLASH_SIZE_ERROR	The reserve size is conflict with actual Flash size
FIRMWARE_CORRUPT	Firmware data is corrupted
CONFIG_CORRUPT		Config data is corrupted
FAT_FORMAT_ERROR	FAT data is error
GET_FAT			Get FAT fail
GETCONFIGURATION	Get Config data fail
DIRECTION_IN		Write Fail
WRITE_LOADER_ERROR	Write Loader disk fail
WRITE_RESERVE_ERROR	Write Reserve disk fail
MBR_ERROR		Write MBR fail 
BOOT_SECTOR_ERROR	Weite Boot Sector fail
FAT_ERROR		Make FAT fail (Check Bad Block Limit)
ROOT_SECTOR_ERROR	Write root directory fail
WRITE_VID		Write VID/PID fail
DLLERR1			No DLL file
DLLERR2			NO DLL function
CHECK_CONFIG_ERROR	Check Config data error
CHECK_LOADER_ERROR	Check Loader data error
WRITE_FILE_ERROR	Write File fail
TOO_MANY_BAD_BLOCK	Too many bad blocks
LLF_TOO_MANY_BAD_BLOCK	Too many bad blocks after LLF
RESET_ERROR		Can't do the reset action
CHECK_BOOT_ERROR	Check Boot sector fail		
CIS_ERROR		Check CIS fail
RW_ERROR		Read/Write Test fail
UNKNOWN_FLASH_ERROR	Unknow flash
DEFAULT_SIZE_ERROR	Default size setting error
WRONG_FLASH_ERROR	Wrong Flash 
WRONG_MINIMUM_BADBLOCK	The bad block setting is less than reserved
INITIAL_SIZE_ERROR	Used disk size error
BADBLOCK_INCREASE	Bad block increased error
FAT Error		Fail to Make FAT (Check Bad Block Limit)
Reset Error		Can't do the reset action
Write Protect		Device is hardware write protected
USB Write Fail		SCSI Write Command Fail (Check Bad Block Limit)
Set Config Fail		Set configuration Command fail
Get Config Fail		Get Configuration fail
Flash Size Error	The reserve size is conflict with actual Flash size
Copy Files Error	The copy files action fail
Boot Sector Error	Can't boot sector
Root Sector Error	Can't root sector
Loader Size Error	The loader Size is conflict with actual Flash size
Check Config Fail	Check Configuration fail 
Check Loader Fail	Get back to check loader size fail
Write Loader Fail	Can't write the loader size
Check Reserve Fail	Get back to check the reserve size fail 
Set Partition Fail	Set partition fail
Read Capacity Fail	Read Capacity Vendor Command Fail
Write Reserve Fail	Can't write the reserve size
Too Many Bad Blocks	The Bad Blocks is too many
Erase Password Fail	Fail to Erase Password
Get Chip Number Fail	Get Chip Number Vendor Command Fail
Select Function Fail	Select Function Vendor Command Fail