This example demonstrates bank switching with the Mentor M8051EW
Memory Extension.  It uses the IBANKING linker/locater directive.

The example is available in two targets:
  LX51:  for the extended LX51 Linker/Locater
  BL51:  for the standard BL51 Linker/Locater
