
                       ----------------------------------------------------
                         Using Guide of Diagnostic Tool NDTOOL for Netdog
                                 (中文版在本文件的后版部分)
                       ----------------------------------------------------

                       Copyrights (c)  1999 , Rainbow Goldensoft Co., Ltd. 

============
About NDTOOL
============

    NDTOOL is a Diagnostic Tool for Netdog, and is a "Dog Client" tool program.
NDTOOL can do the following things.

1) Set mode of communication on "Dog Client" for 32-bit WINDOWS system, and make
   GSNETDOG.INI file. Please refer "Developer's manual" (NETDOG.DOC) to understand 
   the functions and using method of this file.

2) Monitor "Dog Server", and can get the name of "Dog Server", version, computer name 
   running "Dog Server", operating system and its version. And also the status of 
   "Dog Server".

   NDTOOL may be provided to your end-users with your protected application(s).

====================
Suitable environment
====================
   This tool is 32-bit Windows application, and is a "Dog Client". It is suitable for  
1) Windows NT 3.5 and above, Server and WorkSation。
2) Windows 95/98

   This tool supports IPX, TCP/IP and NetBIOS protocol. Thus, it's going to work whenever 
the "Dog Client" and the "Dog Server" is configured with the same protocol. 

=======================
Generating GSNETDOG.INI
=======================

Selecting "Tools" / "Make GSNETDOG.INI" commands from the menu, it will get the default 
option of GSNETDOG.INI. Change these options to suit your own requirements. 

Options Explained:

    Protocol Select         Choose network protocol to be used by NDTOOL
       IPX                  Select IPX 
       TCP/IP               Select TCP/IP 
       NETBOIS              Select NetBios/NetBEUI 

    IPX                     IPX protocol options
       Bindery              Select Bindery mode of IPX
       BroadCast            Select broadcast mode of IPX to communicate with 
                              "Dog Server". 

    NetBIOS                 NetBIOS protocol options
       LanaNum              NetBIOS network device number, ranges from 0 - 9. If only one 
                              network card is used, 0 is the normal selection. 
       NetBIOS Name         The NetBios name of "Dog Server" with the format as: 
                              NetDogSrvXXXXXX, where XXXXXX is the serial number of the Dog. 

    TCP/IP                  TCP/IP protocol options
       BroadCast            Select broadcast mode of TCP/IP to communicate with "Dog Server".
       TCP/UDP              Select TCP/UDP communication mode
       Static IP            Set "Dog Server" static IP address. If the "Dog Server"'s IP 
                              address is not in the same segment with "Dog Client", the 
                              communication will pass through routers. 
       IP Address           "Dog Server" IP address. 

=======================
Monitoring "Dog Server" 
=======================
    Selecting "Tools" / "Monitor Server" from NDTOOL's menu, there are three buttons in the 
operation dialogue box: 
1)  Server Info
    -----------
    Function: Obtain information of "Dog Server".

    If the following result is returned, explanation is at the right:
    DogServer name：NDSRVWNT.EXE          --  Name of "Dog Server"
    DogServer version：1.1                --  Version of "Dog Server"
    DogServer OS name：Windows NT         --  Operating system of "Dog Server"
    DogServer OS version：5.0             --  Version of Operating system of "Dog Server"
    Protocol support：IPX TCP/IP NETBOIS  --  Protocols supported by "Dog Server"

Caution:  If you are not familiar with your network environment, or there isn't enough 
          network knowledge, please do not use the customized searching method come with 
          GSNETDOG.INI.

2)  License Info
    ------------
    Function: Obtain License information of "Dog Server".

    If the following result is returned, explanation is at the right:
         The max license user number is: 10    -- Maximum user number is 10
         The using license user number is: 2   -- Current user number is 2

3)  Delete User
    -----------
    Function: Delete license user number occupied by this computer.
 
    This function deletes license user number occupied by this computer's other 
    application(s) with compulsive method and releases relative resources. This 
    function is only recommended if the protected application is crashed and need 
    to release user resoureces but do not want to reboot "Dog Server".

-------
Caution
-------
A.  NDTOOL tool is also a "Dog Client", but do not to be counted as one user. 
B.  While monitoring "Dog Server", NDTOOL takes some time when searching for "Dog Server"
    at the first time, ranges from 1-20 seconds depending on your network environment. 
C.  NDTOOL can be used as a simple test tool to verify whether "Dog Server" is working 
    properly. 
D.  If you have just finished generating GSNETDOG.INI file, NDTOOL tool will use it to 
    search for "Dog Server". 

=================
Technical Support
=================
    For technical issues, please contact Rainbow GoldenSoft Co., Ltd. or its distributors 
immediately. 
    For contact information, please see Address.txt under installation path.

=========================================================================
  "Dog" is trademarks of Beijing Goldensoft Co., Ltd., which is authorized to 
Rainbow Goldensoft Co., Ltd. in software protection products.



FOLLOWING IS CHINESE VERSION OF THIS FILE.




                       ----------------------------------
                         网络狗诊断工具 NDTOOL 使用说明
                       ----------------------------------

                 版权所有 (c)  1999  ，北京彩虹天地信息技术有限公司
==============
关于NDTOOL工具
==============

    网络狗诊断工具NDTOOL 是一个“狗”客户端的工具软件，它完成以下工作：

     1  设置Win32客户端通信的方式，得到 GSNETDOG.INI 文件。该文件的用处和用法
        见使用说明 NETDOG.DOC
     2  监视“狗”服务器，可以得到“狗”服务器的服务程序名字、版本号，“狗”
        服务器的机器名、操作系统和版本号；可以得到“狗”服务器的状态。

    NDTOOL 工具可以提供给最终用户。

========
适用环境
========

    本模块为 Win32 应用程序（“狗”客户端）。
    适用于IBM PC 386/486/PENTIUM 系列及其兼容系统：

      ⑴ Windows NT 3.5 以上的Server和WorkSation。
      ⑵ Windows 95/98

    本工具支持 IPX 协议、TCP/IP 协议和NetBIOS协议，因此客户端机端（指运行“狗”
    客户端软件的机器）服务器端（指运行“狗”服务器的机器）只要安装设置相同的协议
    即可。


=================
生成 GSNETDOG.INI
=================

    在工具中选择菜单 <Tools>/<Make GSNETDOG.INI>，会得到 GSNETDOG.INI 的默认
    选项，修改这些选项以符合您自己的要求。

    选项解释：

    Protocol Select         选择使用的网络协议
       IPX                  选择使用 IPX 协议
       TCP/IP               选择使用 TCP/IP 协议
       NETBOIS              选择使用 NetBIOS/NetBEUI 协议

    IPX                     IPX 协议选项
       Bindery              使用 IPX 的 Bindery 方式
       BroadCast            使用 IPX 的广播方式与“狗”服务器通信

    NetBIOS                 NetBIOS 协议选项
       LanaNum              NetBIOS 网络设备号，可以选择 0 - 9。如果您只用
                                一个网卡，大多数情况下选择 0。
       NetBIOS Name         “狗”服务器的NetBIOS名，格式为：NetDogSrvXXXXXX，
                                XXXXXX为“狗”的系列号。

    TCP/IP                  TCP/IP 协议选项
       BroadCast            使用TCP/IP的广播方式与“狗”服务器通信。
       TCP/UDP              选择使用 TCP/UDP 方式通信
       Static IP            指定“狗”服务器地址。“狗”服务器地址如果不与“狗”客户端不
                                在同一个网段上，则通信将穿透路由器。
       IP Address           “狗”服务器IP地址。


================
监视“狗”服务器
================

    在 NDTOOL 中选择菜单 Tools / Monitor Server进入操作对话框，有三个按钮：

    1  Server Info
       功能：   得到“狗”服务器的信息

       假设得到以下结果，解释如下：

         DogServer name：NDSRVWNT.EXE          --  “狗”服务器程序名
         DogServer version：1.1                --  “狗”服务器版本号
         DogServer OS name：WindowsNT          --  “狗”服务器操作系统
         DogServer OS version：5.0             --  “狗”服务器操作系统版本号
         Protocol support：IPX TCP/IP NETBOIS  --  “狗”服务器支持的协议

    注意事项：
             如果您不了解您的网络环境，或者没有足够的网络知识，建议您不要使用
       生成GSNETDOG.INI来定制查找。

    2  License Info
       功能：   得到“狗”服务器的用户使用情况信息

       假设得到以下结果，解释如下：

         The max license user number is：10    --  最大用户数为10
         The using license user number is：2   --  目前使用的用户为 2

    3  Delete User
       功能：  删除本机所占用的用户数。

       本功能可以用强制的方法删除本机的其他程序所占用网络狗的用户数和相关资源。
       推荐仅用于本机上的其他客户程序崩溃，需要立即释放用户资源，又不想重新启动
       服务器的情况。

    注意事项：

       1  NDTOOL 工具虽然也是一个“狗”客户端程序，但是不会占一个用户数。
       2  NDTOOL 在监视“狗”服务器的时候，第一次寻找“狗”时将会需要一定时间，
          根据您实际的网络环境可能需要 1 - 20 秒，这是正常现象。
       3  NDTOOL 程序可以作为简单的测试程序来测试网络“狗”是否正常。
       4  如果您刚刚生成了 GSNETDOG.INI，则 NDTOOL 工具将使用 
              GSNETDOG.INI 文件来查找“狗”服务器。


========
技术支持
========

    如果遇到技术问题，请立即与彩虹天地公司或分公司或代理商联系。
    联系地址请看安装目录根目录的Address.txt文件。



	"狗"是北京金天地软件发展有限公司的注册商标，已授权北京彩虹
天地信息技术有限公司使用。
