Silicon Image SiI 3124 SATALink Controller Driver Installation
--------------------------------------------------------------

Table of Contents
-----------------

 1) Windows NT 4.0, Windows 2000/XP or Windows Server 2003 Fresh Installation.

 2) Adding the SiI 3124 controller to an existing Windows NT installation.

 3) Adding the SiI 3124 controller to an existing Windows 2000/XP or
     Windows Server 2003 installation.

 4) Verifying controller installation under Windows NT, Windows 2000/XP or
     Windows Server 2003.

 5) Update SiI 3124 driver on Windows NT 4.0.

 6) Update SiI 3124 driver on Windows 2000.

 7) Update SiI 3124 driver on Windows XP or Windows Server 2003.

 


------------------------------------------------------------------------------
1) Windows NT 4.0, Windows 2000/XP or Windows Server 2003 Fresh Installation
------------------------------------------------------------------------------
Follow the instructions in this section if you are performing a new installation
of Windows NT 4.0, Windows 2000/XP or Windows Server 2003, and you wish
to boot from a device attached to the SiI 3124 SATALink controller.


1. Power off the system.  Insert the SiI 3124 SATALink controller into an
   available PCI slot.  Connect serial ATA cable(s) between the SiI 3124
   controller and the serial ATA device(s).  Power up the system.

2. Put your Windows NT/2000/XP or Windows Server 2003 CD into the
   CD-ROM/DVD drive, or the NT/2000 boot diskette #1 in the floppy
   drive if your system cannot boot from the CD.

3. Press F6 for third party SCSI or driver installation at the beginning
   of text mode installation.  Press 's' when setup asks if you want to
   specify an additional device, and insert the diskette labeled
   'Silicon Image SiI 3124 SATALink Driver Installation Disk'.
   Press 'Enter'.  From the menu presented next, press 'Enter' to select
   the 3124 controller.

4. Press 'Enter' again when prompted to continue on with text mode setup.

5. Follow the setup instructions to select your choice for partition and
   file system.

6. After setup examines your disks, it will copy files from the CD to the
   hard drive selected above and restart the system.  After restart the
   setup process will resume to finish the installation.

7. Once the operating system installation has completed you can follow the
   instructions in section 4 to verify controller was installed correctly.



------------------------------------------------------------------------------
2) Adding the SiI 3124 controller to an existing Windows NT installation
------------------------------------------------------------------------------
Follow the instructions in this section to install the Silicon Image
SiI 3124 SATALink controller into a system already running Windows NT 4.0.


1. Power off the system.  Insert the SiI 3124 SATALink controller into an
   available PCI slot.  Connect serial ATA cable(s) between the SiI 3124
   controller and the serial ATA device(s).  Power up the system.

2. After OS boots up, Click 'Start' 

3. Under 'Settings', click 'Control Panel'.

4. Select 'SCSI Adapters' from the Control Panel.

5. Select the 'Drivers' tab and click 'Add'.

6. Click 'Have Disk'.

7. Insert the diskette labeled 'Silicon Image SiI 3124 SATALink Driver
   Installation Disk' into A: and press 'Enter'.

8. Choose 'Silicon Image SiI 3124 SATALink Controller' and click 'OK'.

9. After the driver installation has completed you can follow the
   instructions in section 4 to verify controller was installed
   correctly.



------------------------------------------------------------------------------
3) Adding the SiI 3124 controller to an existing Windows 2000/XP or
    Windows Server 2003 installation
------------------------------------------------------------------------------
Follow the instructions in this section to install the Silicon Image SiI 3124
SATALink controller into a system already running Windows 2000/XP or Windows
Server 2003.


1. Power off the system.  Insert the SiI 3124 SATALink controller into an
   available PCI slot.  Connect serial ATA cable(s) between the SiI 3124
   controller and the serial ATA device(s).  Power up the system.

2.  During OS boot up, Windows will display the 'Found New Hardware Wizard'.
    Click 'Next'.

3.  Select 'Search for a suitable driver for my device
    (Recommended)' and Click 'Next'.

4.  Under 'Optional search locations' insure that 'Floppy disk drives'
    is checked.

5.  Insert the diskette labeled 'Silicon Image SiI 3124 SATALink Driver
    Installation Disk' into A: and click 'Next'.

6.  When the wizard indicates that it found a driver for the device click
    'Next'.

7.  If the 'Digital Signature Not Found' dialog appears, click 'Yes' to
    continue installing the driver.

8.  The wizard will now copy the required files to the system and start the
    driver.  After starting the driver the wizard will display a completion
    dialog, click 'Finish' to exit the wizard.

9.  See instructions in section 4 to verify controller was installed
    correctly.



------------------------------------------------------------------------------
4) Verifying controller installation under Windows NT, Windows 2000/XP or
    Windows Server 2003
------------------------------------------------------------------------------
Follow the instructions in this section to verify that the controller was
installed correctly.

   For Windows 2000/XP and Windows Server 2003

      1. Right click on 'My Computer' icon, select 'Properties', left click
         on 'Hardware' tab, and then on 'Device Manager' button.

      2. Double click on 'SCSI and RAID Controllers', If there is no yellow
         '!' or '?' in front of 'Silicon Image SiI 3124 SATALink Controller'
         the driver has started correctly.  

      3. To view information about the devices attached to the controller,
         right click the 'Silicon Image SiI 3124 SATALink Controller' and
         select Properties from the context menu, then select the tab
         labeled 'Device Info'.

   For Windows NT 4.0

      1. Double click on 'My Computer' icon, select 'Control Panel', click
         on the 'SCSI Adapters' icon, 'Silicon Image SiI 3124 SATALink
         Controller' should be displayed under 'Device' and 'Driver' tab.

      2. To view information about the devices attached to the controller,
         double click on the 'Silicon Image ATA Controllers' control panel
         applet.  Select a controller from the list at the top of the
         dialog.  Then select a device from the 'Device Location' drop down
         list to view its information.



------------------------------------------------------------------------------
5) Update SiI 3124 driver on Windows NT 4.0
------------------------------------------------------------------------------

1.  After OS boots up, Click 'Start' 

2.  Under 'Settings', click 'Control Panel'.

3.  Select 'SCSI Adapters' from the Control Panel.

4.  Select the 'Drivers' tab and click 'Add'.

5.  Click 'Have Disk'.

6.  Insert the diskette labeled 'Silicon Image SiI 3124 SATALink Driver
    Installation Disk' into A: and press 'Enter'.

7.  Choose 'Silicon Image SiI 3124 SATALink Controller' and click 'OK'.

8.  Refer to instructions in section 4 to verify controller was installed
    correctly.



------------------------------------------------------------------------------
6) Update SiI 3124 driver on Windows 2000
------------------------------------------------------------------------------
With the Silicon Image SATALink controller already plugged in and the driver
already installed.  Follow the instructions below to update SiI 3124 SATALink
driver.


1.  Right click on 'My Computer' and select 'Properties'. Under the 'System
    Properties' section, click on 'Hardware' tab, and then on 'Device Manager'
    click 'SCSI and RAID Controllers' and right click 'Silicon Image SiI 3124
    SATALink Controller' then select 'Properties' from the context menu.

2.  Click 'Update Driver' button on the 'Driver' tab and select 'Display a list
    of the known drivers for this device so that I can choose a specific
    driver'.  Insert the diskette labeled 'Silicon Image SiI 3124 SATALink
    Driver Installation Disk' into the floppy drive. Click 'Next'.

3.  Click 'Have Disk'.  On the 'Install from Disk' dialog ensure that the
    correct floppy drive is specified and click 'OK'.

4.  Click 'Next' until the installation process begins.  If presented with a
    dialog warning about an unsigned driver click 'Yes' to accept it.

5.  If at the end of the installation process you are prompted to reboot the
    system click 'Yes'.

6.  See instructions in section 4 to verify controller was installed
    correctly.



------------------------------------------------------------------------------
7) Update SiI 3124 driver on Windows XP or Windows Server 2003
------------------------------------------------------------------------------
Follow the instructions in this section to update the driver for the SiI 3124
SATALink controller on Windows XP or Windows Server 2003.

1.  Right click on 'My Computer' and select 'Properties'. Under the 'System
    Properties' section, click on 'Hardware' tab, and then on 'Device Manager'
    click 'SCSI and RAID Controllers' and right click 'Silicon Image SiI 3124
    SATALink Controller' then select 'Properties' from the context menu.

2.  Select the 'Driver' tab, then click the 'Update Driver' button.

3.  Select 'Install from a list or specific location (Advanced)' and click
    'Next',

4.  Make sure 'Search for the best driver in these locations' and 'Search
    removable media (floppy, CD-ROM...)' are both selected and then click
    'Next'.

5.  As the installation process begins you may be presented with a dialog
    warning about a non-logo'd driver, click 'Continue Anyway' to continue
    the installation.

6.  If at the end of the installation process you are prompted to reboot the
    system click 'Yes'.

7.  See instructions in section 4 to verify controller was installed
    correctly.



