This page is not fully translated, yet. Please help completing the translation.
(remove this paragraph once the translation is finished)

# INDI Telescope interface

From the menu: Telescope

The configuration of the telescope driver is done from the menu Setup -> General -> Telescope

Click the “Connect button”, the light must change to green and the telescope coordinates are displayed.
In case of connection problem you can look at the message at the bottom of the window.

To free some space on the screen you can close the interface window by clicking the “Hide” button. Refer to the main menu Telescope to learn how to show the telescope position on the chart or to use the Goto facility if supported by your telescope.

Also if supported you can refine the local slewing precision by using “Sync current object” on a nearby star at any time.