Connect from GND ("-") to VCC ("+") wire by wire.
Special connection order for some batteries will be noted here when needed.

M37516/80AF
If you find double protection IC MM1373 (373E) on your battery PCB (for example DELL 1691P) you should connect cells as follow: GND ("-"), VCC ("+"), middle then any. 


