/*
=====================================================================
   PESpin v1.1 unpacker script for OllyScript plugin (by SHaG)
=====================================================================

    Script requires Windows XP.
    Script works good only with ASM and BC++ programs. Delphi
    and VC++ will not be properly fixed using OllyDump plugin.
    For those programs check my other scripts and read tutorial.
    Script will fix IAT redirection, code redirection and find
    stolen OEP code. This PESpin version uses CRYPT and CLEAR
    markers, which this script cannot decrypt. You'll have to
    decrypt code manually. However, two other scripts
    "PESpin - Code Fixer.txt"
    "PESpin - Find Markers.txt"
    will help you find encrypted sections and repir them.
    Before use, ignore ALL exceptions!

    [ haggar ]
=====================================================================
*/

var x
var A
var B
var C

msg "Script runs on Win XP only. Ignore ALL exceptions!"

//Break on GetTickCount
gpa "GetTickCount","kernel32.dll"
findop $RESULT,#C3#
bp $RESULT
esto
bc eip
rtu


//Find that code around timer call and just place bp.
mov A,eip
sub A,0E50
find A,#F?723F8D85F469271E2D8417E71DFFD0EB02#
add $RESULT,1
bp $RESULT

//Now find place where is IAT redirection jump.
mov A,eip
sub A,0F20
findop A,#FF6424FC#
bp $RESULT
esto
bc eip
mov A,$RESULT
//Find good call and NOP all bytes between.
find eip,#E8??????FFE803000000#
mov B,$RESULT
noping:
fill A,1,90
inc A
cmp A,B
jne noping
esto

//Timer place noping:
bc eip
fill eip,0F,90


//Go to byte before POPAD and NOP it.

mov A,eip
add A,221
fill A,1,90
add A,2
bp A
esto
bc eip
cmt eip,"Here starts stolen OEP."


//Code fixing:



var addr
var Redir
var buffer
var temp
var Value
mov addr,401000






search:
findop addr,#E???????FF#        //Find posible CALL/JMP to PEheader.
cmp $RESULT,0
je exit
mov addr,$RESULT
mov buffer,addr
add addr,1

mov Redir,[addr]                //Check does it realy jumps to PEheader.
add Redir,addr
and Redir,4FF000
cmp Redir,400000
jne search

mov Redir,[addr]                //Find that redirected address.
add Redir,addr
add Redir,4
mov Value,[Redir]               //Check is there JMP (E9) opcode.
and Value,0FF
cmp Value,0E9
je JumpsCalls                   //If not, just copy all bytes. If yes, goto Jumps fixing.

add Redir,1                     //Copy bytes, PUSH opcodes.
mov Value,[Redir]
sub addr,1
//cmt addr,"Fixed PUSH opcode."
fill addr,1,68
add addr,1
mov [addr],Value
mov addr,buffer
jmp search

JumpsCalls:                         //Fix jumps/calls.
sub addr,1
//cmt addr,"Fixed JMP or CALL opcode."
mov temp,[addr]
cmp temp,0E9
je Jump
fill addr,1,0E8
jmp Call
Jump:
fill addr,1,0E9
Call:
add Redir,1
add addr,1
mov Value,[Redir]
add Value,Redir
add Value,4
sub Value,addr
sub Value,4
mov [addr],Value
mov addr,buffer
jmp search


exit:
ret









