Home > Machine Settings > Menu Table (for LCD Models) > Settings Table

### Settings Table

Related Models:DocuPrint P268 d / DocuPrint P268 dw
Use these tables to understand the various menu and options that you will use to set your preferences on the machine.

Machine Info.

Level 1 | Level 2 | Description
Print Settings | - | Prints the Printer Settings page.
Print NetSetting | - | Prints the Network Configuration Report.
Print WLANReport (For wireless models) | - | Prints the result of wireless LAN connectivity diagnosis.
Test Print | - | Prints the test page.
Demo Print | - | Prints the demonstration sheet.
Print Font (DocuPrint P228 db/DocuPrint P268 b/DocuPrint P268 d/DocuPrint P268 dw) | - | Prints the font list.
Serial No. | - | Displays the machine's serial number.
Version | Main Version | Displays the main firmware version.
Sub1 Version (DocuPrint P268 d/DocuPrint P268 dw) | Displays the sub firmware version.
RAM Size | Displays the size of memory in this machine.
Page Count | - | Displays the total printed pages.
Parts Life | Toner Life | Displays the remaining life for toner cartridge.
Drum Life | Displays the remaining life for the drum unit.

Paper Tray

Level 1 | Description
Manual Feed | Select whether to print from the Manual Feed Slot.
2-sided (For automatic 2-sided printing models) | Select whether to print on both sides of the paper.
Tray1 Size | Select the size of paper you loaded in the standard paper tray.
Check Size | Select whether to display the message telling you to check that the size of the paper in the machine and the machine's Paper Size setting match.

General Setup

Level 1 | Level 2 | Description
Local Language | - | Select the LCD language for your country.
Resolution | - | Select a print resolution.
Density | - | Increases or Decreases the print density.
Ecology | Toner Save | Increases the page yield of the toner cartridge.
Sleep Time | Set the time to return to Power Saving Mode.
Quiet Mode | Decreases printing noise.
Auto Power Off | Sets the number of hours that the machine will remain in Deep Sleep Mode before going into Power Off Mode.
Panel Control | Button Repeat | Sets the time for the LCD message to change when holding or at intervals.
Message Scroll | Sets the time in seconds that an LCD message will scroll across the LCD. From Level 1=0.2 sec to Level 10=2.0 sec.
LCD Contrast | Adjusts the contrast of the LCD.
Auto Online | Sets the machine to return to Ready Mode after it has been idle for 30 seconds. If you select the setting to be Off, the machine cannot receive print jobs while it has been left in Menu Mode.
Setting Lock | - | Turns the lock panel settings by using the password.
Interface | Select | Select the interface to use. If you choose Auto, the machine automatically changes the interface to USB or Ethernet depending on which interface is receiving data.
Auto IF Time | You must set the time-out period for the auto interface selection.
Input Buffer | Increases or decreases the input buffer capacity.
Replace Toner | - | Sets the machine to continue printing after the LCD displays Replace Toner.

Print Menu

Level 1 | Level 2 | Description
Auto Continue | - | Select this setting if you want the machine to clear paper size errors.
Media Type (DocuPrint P228 db/DocuPrint P268 b/DocuPrint P268 d/DocuPrint P268 dw) | - | Sets the type of paper.
Paper (DocuPrint P228 db/DocuPrint P268 b/DocuPrint P268 d/DocuPrint P268 dw) | - | Sets the size of paper.
Copies (DocuPrint P228 db/DocuPrint P268 b/DocuPrint P268 d/DocuPrint P268 dw) | - | Sets the number of printed pages.
Orientation (DocuPrint P228 db/DocuPrint P268 b/DocuPrint P268 d/DocuPrint P268 dw) | - | This machine can print pages in portrait or landscape orientation.
Print Position | X Offset | Moves the print start position (at the top-left corner of pages) horizontally up to -500 (left) to +500 (right) dots in 300 dpi.
Y Offset | Moves the print start position (at the top-left corner of pages) vertically up to -500 (up) to +500 (down) dots in 300 dpi.
Auto FF (DocuPrint P228 db/DocuPrint P268 b/DocuPrint P268 d/DocuPrint P268 dw) | - | Allows the machine to print any remaining data automatically.
HP LaserJet (DocuPrint P228 db/DocuPrint P268 b/DocuPrint P268 d/DocuPrint P268 dw) | Font No. | Sets the font number.
Font Pitch | Sets the font pitch. The Font Pitch menu will appear when you choose I042 to I054 in Font No. setting.
Font Point | Sets the font size. The Font Point menu will appear when you choose I000 to I041 in Font No. setting.
Symbol Set | Sets the symbol set or the character set.
Table Print | Prints the code table.
Auto LF | ON: CR -> CR+LF, OFF: CR -> CR
Auto CR | ON: LF -> LF+CR, FF -> FF+CR, or VT -> VT+CR OFF: LF -> LF, FF -> FF, or VT -> VT
Auto WRAP | Chooses whether a line feed and carriage return will happen when the machine reaches the right margin.
Auto SKIP | Chooses whether a line feed and carriage return will happen when the carriage position reaches the bottom margin.
Left Margin | Sets the left margin at column 0 to 70 columns at 1 cpi.
Right Margin | Sets the right margin at column 10 to 80 columns at 1 cpi.
Top Margin | Sets the top margin at a distance from the top edge of the paper.
Bottom Margin | Sets the bottom margin at a distance from the bottom edge of the paper.
Lines | Sets the number of lines on each page.

Network DocuPrint P268 d

Level 1 | Level 2 | Description
TCP/IP | Boot Method | Chooses the IP method that best suits your needs.
IP Address | Enter the IP address.
Subnet Mask | Enter the Subnet mask.
Gateway | Enter the Gateway address.
IP Boot Tries | Specifies the number of attempts the machine will try to obtain an IP address when the Boot Method is set to any setting except Static.
APIPA | Automatically allocates the IP address from the link-local address range *1.
IPv6 | Enables or Disables the IPv6 protocol.
Ethernet | - | Chooses the Ethernet link mode.
Wired Status | - | Displays Ethernet link status.
MAC Address | - | Displays MAC address of the machine.
Network Reset | - | Restores all network settings of the internal print server to the factory settings.

*1
On connection to the network, if the machine's ‘Boot Method’ is ‘Auto’ the machine will attempt to set the IP address and Subnet Mask from a boot server such as DHCP. If a boot server cannot be found, an APIPA IP address will be allocated, such as 169. 254. [001-254]. [000-255]. If the ‘Boot Method’ of the machine is set to ‘Static’ you must manually enter an IP address from the machine's control panel.

Network DocuPrint P268 dw

Level 1 | Level 2 | Level 3 | Description
Wired LAN | TCP/IP | Boot Method | Chooses the IP method that best suits your needs.
IP Address | Enter the IP address.
Subnet Mask | Enter the Subnet mask.
Gateway | Enter the Gateway address.
IP Boot Tries | Specifies the number of attempts the machine will try to obtain an IP address when the Boot Method is set to any setting except Static.
APIPA | Automatically allocates the IP address from the link-local address range.
IPv6 | Enables or disables the IPv6 protocol.
Ethernet | - | Chooses the Ethernet link mode.
Wired Status | - | Displays Ethernet link status.
MAC Address | - | Displays MAC address of the machine.
Set to Default | - | Restores wired network settings of the internal print server to the factory settings.
Wired Enable | - | Turns the wired interface on or off.
WLAN | TCP/IP | Boot Method | Chooses the IP method that best suits your needs.
IP Address | Enter the IP address.
Subnet Mask | Enter the Subnet mask.
Gateway | Enter the Gateway address.
IP Boot Tries | Specifies the number of attempts the machine will try to obtain an IP address when the Boot Method is set to any setting except Static.
APIPA | Automatically allocates the IP address from the link-local address range *1.
IPv6 | Enables or Disables the IPv6 protocol.
WLAN Assistant | - | You can configure your wireless network settings using the Fuji Xerox CD-ROM.
Setup Wizard | - | Configures the wireless network settings using the setup wizard.
WPS/AOSS | - | Configures the wireless network settings using WPS or AOSS™ method.
WPS w/PIN Code | - | Configures the wireless network settings using WPS with a PIN code.
WLAN Status | Status | Displays wireless Ethernet link status.
Signal | Displays the signal condition.
Channel | Displays the channel in use when Status is Active.
Speed | Displays the connecting speed when Status is Active.
SSID | Displays SSID.
Comm. Mode | Displays the current Communication Mode.
MAC Address | - | Displays MAC address of the machine.
Set to Default | - | Restores wireless network settings of the internal print server to the factory settings.
WLAN Enable | - | Turns the wireless interface on or off.
Wi-Fi Direct | Push Button | - | You can easily configure your Wi-Fi Direct™ network settings using the one-button push method.
PIN Code | - | You can easily configure your Wi-Fi Direct™ network settings using WPS with a PIN code.
Manual | - | You can manually configure your Wi-Fi Direct™ network settings.
Group Owner | - | Sets your machine as the Group Owner.
Device Info. | Device Name | You can see the device name of your machine.
SSID | Displays SSID of Group Owner.
IP Address | Displays the IP Address of your machine.
Status Info. | Status | Displays the Wi-Fi Direct™ network status.
Signal | Displays the current Wi-Fi Direct™ network signal strength. When your machine acts as Group Owner, the LCD always displays strong.
Channel | Displays the channel in use when the Status is G/O Active or Client Active.
Speed | Displays the connecting speed when the Status is G/O Active or Client Active.
I/F Enable | - | Enables or disables the Wi-Fi Direct™ connection.
Network Reset | - | - | Restores all network settings of the internal print server to the factory settings.

*1
On connection to the network, if the machine's ‘Boot Method’ is ‘Auto’ the machine will attempt to set the IP address and Subnet Mask from a boot server such as DHCP. If a boot server cannot be found, an APIPA IP address will be allocated, such as 169. 254. [001-254]. [000-255]. If the ‘Boot Method’ of the machine is set to ‘Static’ you must manually enter an IP address from the machine's control panel.

Reset Menu

Level 1 | Description
Network | Restores all network settings of the internal print server to the factory settings.
Factory Reset | Resets the machine and restores the printer settings (including command settings) to the factory settings.

Related Information
  - Menu Table (for LCD Models)
  - General Specifications

Go to top of page