Home > Network > Additional Methods of Configuring Your Fuji Xerox Machine for a Wireless Network > Use Wi-Fi Direct™ > Configure Your Wi-Fi Direct Network > Configure Your Wi-Fi Direct Network Using the One-Push Method

### Configure Your Wi-Fi Direct Network Using the One-Push Method

Related Models:DocuPrint P268 dw
If your mobile device supports Wi-Fi Direct, follow these steps to configure a Wi-Fi Direct network:

1. Press or to select the Network option, and then press OK.
2. Press or to select the Wi-Fi Direct option, and then press OK.
3. Press or to select the Push Button option, and then press OK.
4. When Wi-Fi Direct On? appears, press to accept. To cancel, press .
5. Activate Wi-Fi Direct on your mobile device (see your mobile device's user's guide for instructions) when Activate Wi-Fi Direct on other device and press OK. appears on the machine's LCD. Press OK on your machine.
   This will start the Wi-Fi Direct setup. To cancel, press Back .
6. Do one of the following:
   - When your Fuji Xerox machine is the Group Owner (G/O), connect your mobile device to the machine directly.
   - When your Fuji Xerox machine is not the G/O, it will display available device names with which to configure a Wi-Fi Direct network. Press or to select the mobile device you want to connect to and press OK. Search for available devices again by pressing Rescan.
7. If your mobile device connects successfully, the machine's LCD displays Connected. You have completed the Wi-Fi Direct network setup.

Related Information
  - Configure Your Wi-Fi Direct Network
  - Step-by-step Guide for Wi-Fi Direct Network Configuration

Go to top of page