Home > Network > Additional Methods of Configuring Your Fuji Xerox Machine for a Wireless Network > Configure Your Machine for a Wireless Network Using the One Push Method of Wi-Fi Protected Setup™ (WPS) or AOSS™

### Configure Your Machine for a Wireless Network Using the One Push Method of Wi-Fi Protected Setup™ (WPS) or AOSS™

If your wireless access point/router supports either WPS (Push Button Configuration) or AOSS™, you can use WPS or AOSS™ from your machine's Wi-Fi/WPS button to configure your wireless network settings.

- Routers or access points that support WPS are marked with this symbol:
- Routers or access points that support AOSS™ are marked with this symbol:

Related Information
  - Additional Methods of Configuring Your Fuji Xerox Machine for a Wireless Network
  - How to Configure Your Wireless Network Using the One Push Method of WPS or AOSS™
  - Connected to a Computer with a Wireless LAN Access Point Router in the Network (Infrastructure Mode)

Go to top of page