;/*++
;
;Copyright (c) 2001-2009 Atheros Communications, Incorporated All Rights Reserved
;
;Module Name:
;
;    netathwx.inf
;
;Abstract:
;    INF file for installing Atheros AR5008 Wireless Network Adapter
;
;    Installs athw.sys (NDIS 5/5.1 driver) on NT platforms (2000, XP and greater)
;    Installs athwx.sys (NDIS 5 driver) on 9x platforms
;
;--*/

[Version]
Signature   = "$CHICAGO$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %ATHEROS%
Compatible  = 1
DriverVer   = 12/29/2009,7.7.0.456
Catalogfile.nt = netathwx.cat
;Catalogfile = netathwx.cat

[Manufacturer]
%ATHEROS%     = Atheros,NTamd64
%Gigabyte%    = Gigabyte,NTamd64

[ControlFlags]
;ExcludeFromSelect = \  ;for win95 and legacy support
;  PCI\VEN_168C&DEV_0013
ExcludeFromSelect = *

[Atheros]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
; Generic
%ATHER.DeviceDesc.0013%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013
%ATHER.DeviceDesc.0013%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0014
%ATHER.DeviceDesc.0013%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0015
%ATHER.DeviceDesc.0013%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0016
%ATHER.DeviceDesc.0013%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0017
%ATHER.DeviceDesc.0013%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0018
%ATHER.DeviceDesc.0013%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0019
%ATHER.DeviceDesc.001A%     = ATHER_DEV_001A.ndi,     PCI\VEN_168C&DEV_001A
%ATHER.DeviceDesc.001B%     = ATHER_DEV_001B.ndi,     PCI\VEN_168C&DEV_001B
%ATHER.DeviceDesc.001B%     = ATHER_DEV_001B.ndi,     PCI\VEN_168C&DEV_001C
%ATHER.DeviceDesc.001B%     = ATHER_DEV_001B.ndi,     PCI\VEN_168C&DEV_FF19
%ATHER.DeviceDesc.001D%     = ATHER_DEV_001D.ndi,     PCI\VEN_168C&DEV_001D
%ATHER.DeviceDesc.0023%     = ATHER_DEV_0023.ndi,     PCI\VEN_168C&DEV_0023
%ATHER.DeviceDesc.0023%     = ATHER_DEV_0023.ndi,     PCI\VEN_168C&DEV_0024
%ATHER.DeviceDesc.0023%     = ATHER_DEV_0023.ndi,     PCI\VEN_168C&DEV_FF1C
%ATHER.DeviceDesc.0023%     = ATHER_DEV_0023.ndi,     PCI\VEN_168C&DEV_FF1D
; Atheros
%ATHER.DeviceDesc.1025%     = ATHER_DEV_1025.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1025168C
%ATHER.DeviceDesc.2025%     = ATHER_DEV_2025.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2025168C
%ATHER.DeviceDesc.1026%     = ATHER_DEV_1026.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1026168C
%ATHER.DeviceDesc.2026%     = ATHER_DEV_2026.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2026168C
%ATHER.DeviceDesc.1027%     = ATHER_DEV_1027.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1027168C
%ATHER.DeviceDesc.2027%     = ATHER_DEV_2027.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2027168C
%ATHER.DeviceDesc.1030%     = ATHER_DEV_1030.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1030168C
%ATHER.DeviceDesc.2030%     = ATHER_DEV_2030.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2030168C
%ATHER.DeviceDesc.1031%     = ATHER_DEV_1031.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1031168C
%ATHER.DeviceDesc.2031%     = ATHER_DEV_2031.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2031168C
%ATHER.DeviceDesc.1041%     = ATHER_DEV_1041.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1041168C
%ATHER.DeviceDesc.2041%     = ATHER_DEV_2041.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2041168C
%ATHER.DeviceDesc.1042%     = ATHER_DEV_1042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1042168C
%ATHER.DeviceDesc.2042%     = ATHER_DEV_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2042168C
%ATHER.DeviceDesc.1051%     = ATHER_DEV_1051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1051168C
%ATHER.DeviceDesc.2051%     = ATHER_DEV_2051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2051168C
%ATHER.DeviceDesc.001A%     = ATHER_DEV_1052.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_1052168C
%ATHER.DeviceDesc.001A%     = ATHER_DEV_2052.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_2052168C
%ATHER.DeviceDesc.1053%     = ATHER_DEV_1053.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1053168C
%ATHER.DeviceDesc.2053%     = ATHER_DEV_2053.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2053168C
%ATHER.DeviceDesc.001A%     = ATHER_DEV_1054.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_1054168C
%ATHER.DeviceDesc.001A%     = ATHER_DEV_2054.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_2054168C
%ATHER.DeviceDesc.1062%     = ATHER_DEV_1062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1062168C
%ATHER.DeviceDesc.2062%     = ATHER_DEV_2062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2062168C
%ATHER.DeviceDesc.001B%     = ATHER_DEV_1063.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1063168C
%ATHER.DeviceDesc.001B%     = ATHER_DEV_2063.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2063168C
%ATHER.DeviceDesc.3062%     = ATHER_DEV_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3062168c
%ATHER.DeviceDesc.3063%     = ATHER_DEV_2063.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3063168c
%ATHER.DeviceDesc.3061%     = ATHER_DEV_2051.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3061168c
%ATHER.DeviceDesc.3065%     = ATHER_DEV_2052.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3065168c
%ATHER.DeviceDesc.2061%     = ATHER_DEV_2051.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2061168c
%ATHER.DeviceDesc.1061%     = ATHER_DEV_1051.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1061168c
%ATHER.DeviceDesc.2065%     = ATHER_DEV_2052.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2065168c
%ATHER.DeviceDesc.1065%     = ATHER_DEV_1052.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1065168c
%ATHER.DeviceDesc.3067%     = ATHER_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3067168C
%ATHER.DeviceDesc.3067%     = ATHER_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3064168C
%ATHER.DeviceDesc.2055%     = ATHER_DEV_2055.ndi,     PCI\VEN_168C&DEV_001D&SUBSYS_2055168c
%ATHER.DeviceDesc.1055%     = ATHER_DEV_1055.ndi,     PCI\VEN_168C&DEV_001D&SUBSYS_1055168c
; Others  
%ATHER.DeviceDesc.2026%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7005144F
%ATHER.DeviceDesc.2026%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7057144F
%ATHER.DeviceDesc.2026%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7058144F
%ATHER.DeviceDesc.2041%     = ATHER_DEV_2041.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7064144F
%ATHER.DeviceDesc.2042%     = ATHER_DEV_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7065144F
%ATHER.DeviceDesc.2051%     = ATHER_DEV_2051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7084144F
%ATHER.DeviceDesc.2051%     = ATHER_DEV_2051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7088144F
%ATHER.DeviceDesc.2062%     = ATHER_DEV_2062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_7092144F
%ATHER.DeviceDesc.001A%     = ATHER_DEV_2054.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_7094144F
%ATHER.DeviceDesc.2042%     = ATHER_DEV_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7005168C
%ATHER.DeviceDesc.3063%     = ATHER_DEV_2063.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7096144F
%ATHER.DeviceDesc.3065%     = ATHER_DEV_2052.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7106144F
%ATHER.DeviceDesc.3067%     = ATHER_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7128144f
%ATHER.DeviceDesc.0013%     = ATHER_DEV_F013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_123410CF
%ATHER.DeviceDesc.0013%     = ATHER_DEV_F013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_123510CF
%ATHER.DeviceDesc.10CF%     = ATHER_DEV_F013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_123610CF
%ATHER.DeviceDesc.001B%     = ATHER_DEV_F013.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_132910CF
%ATHER.DeviceDesc.10CF%     = ATHER_DEV_F013.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_134F10CF
%ATHER.DeviceDesc.3062%     = ATHER_DEV_F013C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_139C10CF
%ATHER.DeviceDesc.3067%     = ATHER_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_142E10CF
%ATHER.DeviceDesc.3062%     = ATHER_DEV_04221468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_04221468
%ATHER.DeviceDesc.001A%     = ATHER_DEV_04171468.ndi, PCI\VEN_168C&DEV_001A&SUBSYS_04171468
%ATHER.DeviceDesc.001A%     = ATHER_DEV_04171468.ndi, PCI\VEN_168C&DEV_001A&SUBSYS_04181468
%ATHER.DeviceDesc.001A%     = ATHER_DEV_04171468.ndi, PCI\VEN_168C&DEV_001A&SUBSYS_04201468
%ATHER.DeviceDesc.3067%     = ATHER_DEV_042A1468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_042A1468
%ATHER.DeviceDesc.E000%     = ATHER_DEV_E000105B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E000105B
%ATHER.DeviceDesc.E000%     = ATHER_DEV_E002105B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E002105B
%ATHER.DeviceDesc.0406%     = ATHER_DEV_04061468.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_04061468
%ATHER.DeviceDesc.0407%     = ATHER_DEV_04071468.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_04071468
%ATHER.DeviceDesc.E000%     = ATHER_DEV_04231468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_04231468
%ATHER.DeviceDesc.E000%     = ATHER_DEV_04231468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_0423168C
%ATHER.DeviceDesc.3063%     = ATHER_DEV_2063.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_04271468
%ATHER.DeviceDesc.3065%     = ATHER_DEV_2052.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_04251468
%ATHER.DeviceDesc.001A%     = ATHER_DEV_2052.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_04261468
%ATHER.DeviceDesc.3067%     = ATHER_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_042A1468
%ATHER.DeviceDesc.0055%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_123610CF
%ATHER.DeviceDesc.0055%     = ATHER_DEV_001B.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_134f10CF
%ATHER.DeviceDesc.3072%     = ATHER_DEV_7125144F.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_7125144F
%ATHER.DeviceDesc.3072%     = ATHER_DEV_7125144F.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_04291468
%ATHER.DeviceDesc.3072%     = ATHER_DEV_0023.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_04301468
%ATHER.DeviceDesc.3072%     = ATHER_DEV_05021A32.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_05021A32
%ATHER.DeviceDesc.3065%     = ATHER_DEV_01001A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01001A32
%ATHER.DeviceDesc.3063%     = ATHER_DEV_02001A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_02001A32
%ATHER.DeviceDesc.3067%     = ATHER_DEV_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01051A32
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3091168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3092168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3093168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3094168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3095168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3096168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3097168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3098168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3099168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309A168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309B168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309C168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309D168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309F168C
%ATHER.DeviceDesc.2091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2091168C
%ATHER.DeviceDesc.2091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2092168C
%ATHER.DeviceDesc.2091%     = ATHER_DEV_3091PB.ndi,   PCI\VEN_168C&DEV_0029&SUBSYS_2093168C
%ATHER.DeviceDesc.2091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2094168C
%ATHER.DeviceDesc.2091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2096168C
%ATHER.DeviceDesc.2091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2098168C
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30A1168C
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30A2168C
%ATHER.DeviceDesc.30AB%     = ATHER_DEV_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30AB168C
%ATHER.DeviceDesc.30AD%     = ATHER_DEV_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30AD168C
%ATHER.DeviceDesc.30AE%     = ATHER_DEV_30AA.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30AE168C
%ATHER.DeviceDesc.30AF%     = ATHER_DEV_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30AF168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_30A3168C
%ATHER.DeviceDesc.30A7%     = ATHER_DEV_001C.ndi,     PCI\VEN_168C&DEV_002C&SUBSYS_30A7168C
%ATHER.DeviceDesc.2099%     = ATHER_DEV_30A1.ndi,     PCI\VEN_168C&DEV_002D&SUBSYS_2099168C
%ATHER.DeviceDesc.30A4%     = ATHER_DEV_30A1.ndi,     PCI\VEN_168C&DEV_002E&SUBSYS_30A4168C
; NEC
%ATHER.DeviceDesc.3062%     = ATHER_DEV_N2062.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_102010E9
%ATHER.DeviceDesc.3062%     = ATHER_DEV_N2062.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_102510E9
%ATHER.DeviceDesc.3072%     = ATHER_DEV_N3072.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_102210E9
%ATHER.DeviceDesc.3072%     = ATHER_DEV_N3073.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_102610E9
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_03051A32.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_03051A32
; Foxconn
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_E023105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E023105B
%ATHER.DeviceDesc.30A7%     = ATHER_DEV_E029105B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_E029105B
%ATHER.DeviceDesc.30A7%     = ATHER_DEV_1029105B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_1029105B
%ATHER.DeviceDesc.30AB%     = ATHER_DEV_E033105Bw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_E033105B
; Apple
%ATHER.DeviceDesc.3072%     = ATHER_DEV_0023.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_00000000
%ATHER.DeviceDesc.3062%     = ATHER_DEV_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_0086106B
%ATHER.DeviceDesc.3072%     = ATHER_DEV_0023.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_0087106B
%ATHER.DeviceDesc.3091%     = ATHER_DEV_008F106B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_008F106B
; AMD
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091amd.ndi,  PCI\VEN_168C&DEV_002A&SUBSYS_1130168C
; Netgear
%ATHER.DeviceDesc.90001385% = ATHER_DEV_90001385.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_90001385
%ATHER.DeviceDesc.4B001385% = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_4B001385
%ATHER.DeviceDesc.4B001385% = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5B001385
%ATHER.DeviceDesc.5D001385% = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5D001385
%ATHER.DeviceDesc.4D001385% = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_4D001385
%ATHER.DeviceDesc.4F001385% = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_4F001385
%ATHER.DeviceDesc.5E001385% = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5E001385
%ATHER.DeviceDesc.4D001385% = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5A001385
;OQO
%ATHER.DeviceDesc.2062%     = ATHER_DEV_2062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1602196f
%ATHER.DeviceDesc.2062%     = ATHER_DEV_2062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1603196f
%ATHER.DeviceDesc.3062%     = ATHER_DEV_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_1604196f
; Lenovo Japan
%ATHER.DeviceDesc.5013%     = ATHER_DEV_5013.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_0034168c
%ATHER.DeviceDesc.6013%     = ATHER_DEV_6013.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_0035168c
%ATHER.DeviceDesc.3013%     = ATHER_DEV_3013.ndi,     PCI\VEN_168C&DEV_1014&SUBSYS_05891014
%ATHER.DeviceDesc.4013%     = ATHER_DEV_4013.ndi,     PCI\VEN_168C&DEV_1014&SUBSYS_058A1014
%ATHER.DeviceDesc.2013%     = ATHER_DEV_2013.ndi,     PCI\VEN_168C&DEV_1014&SUBSYS_057E1014
%ATHER.DeviceDesc.1013%     = ATHER_DEV_1013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_04081468
%ATHER.DeviceDesc.0032168c% = ATHER_DEV_0032168c.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_0032168c
%ATHER.DeviceDesc.0033168c% = ATHER_DEV_0033168c.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_0033168c
%ATHER.DeviceDesc.0036%     = ATHER_DEV_0036.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_0036168c
%ATHER.DeviceDesc.0037%     = ATHER_DEV_0037.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_0037168c
; Lenovo China
%ATHER.DeviceDesc.309917AA% = ATHER_DEV_309917AA.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_309917AA
%ATHER.DeviceDesc.3067%     = ATHER_DEV_316417AA.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_316417AA
%ATHER.DeviceDesc.3091%     = ATHER_DEV_309D17AA.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_309D17AA
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_30A117AA.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_30A117AA
; IBM
%ATHER.DeviceDesc.0033168c% = ATHER_DEV_03841014.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_03841014
; Samsung
%ATHER.DeviceDesc.001A%     = ATHER_DEV_S001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7101144F
%ATHER.DeviceDesc.001A%     = ATHER_DEV_S001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7114144F
%ATHER.DeviceDesc.001A%     = ATHER_DEV_S001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7115144F
%ATHER.DeviceDesc.3067%     = ATHER_DEV_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_7131144F
%ATHER.DeviceDesc.3067%     = ATHER_DEV_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_7130144F
%ATHER.DeviceDesc.001B%     = ATHER_DEV_S001B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7108144F
%ATHER.DeviceDesc.001B%     = ATHER_DEV_S001B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7116144F
%ATHER.DeviceDesc.3067%     = ATHER_DEV_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_E00B105B
%ATHER.DeviceDesc.3067%     = ATHER_DEV_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_E00C105B
%ATHER.DeviceDesc.001B%     = ATHER_DEV_S3067a.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_E00E105B
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091SF.ndi,   PCI\VEN_168C&DEV_002A&SUBSYS_E00F105B
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091SF.ndi,   PCI\VEN_168C&DEV_002A&SUBSYS_E010105B
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091SF.ndi,   PCI\VEN_168C&DEV_002A&SUBSYS_7161144F
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_30A1a.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_7167144F
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_30A1a.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E025105B
%ATHER.DeviceDesc.30AB%     = ATHER_DEV_30A1w.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E032105B
; Askey
%ATHER.DeviceDesc.7173144F% = ATHER_DEV_7173144Fw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_7173144F
; D-Link
%ATHER.DeviceDesc.DWA642%   = ATHER_DEV_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A6A1186
%ATHER.DeviceDesc.DWA645%   = ATHER_DEV_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A0907D1
%ATHER.DeviceDesc.DWA645%   = ATHER_DEV_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A761186
%ATHER.DeviceDesc.DWA645%   = ATHER_DEV_3A7B1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A791186
%ATHER.DeviceDesc.DWA542%   = ATHER_DEV_3A691186.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_3A691186
%ATHER.DeviceDesc.DWA547%   = ATHER_DEV_3A6D1186.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_3A6B1186
%ATHER.DeviceDesc.DWA547%   = ATHER_DEV_3A7A1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A781186
%ATHER.DeviceDesc.DWA652%   = ATHER_DEV_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A6E1186
%ATHER.DeviceDesc.DWA652%   = ATHER_DEV_3A7B1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A7B1186
%ATHER.DeviceDesc.DWA552%   = ATHER_DEV_3A6D1186.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_3A6D1186
%ATHER.DeviceDesc.DWA552%   = ATHER_DEV_3A7A1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A7A1186
%ATHER.DeviceDesc.DWA643%   = ATHER_DEV_3A6F1186.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_3A6F1186
%ATHER.DeviceDesc.DWA556%   = ATHER_DEV_3A701186.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_3A701186
%ATHER.DeviceDesc.DWA520%   = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A731186
%ATHER.DeviceDesc.DWA620%   = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A741186
%ATHER.DeviceDesc.WDA1320%  = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A1D1186
%ATHER.DeviceDesc.WDA2320%  = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A1B1186
%ATHER.DeviceDesc.WNA2330%  = ATHER_DEV_WNA2330.ndi,  PCI\VEN_168C&DEV_0013&SUBSYS_3A1A1186
%ATHER.DeviceDesc.WNA1330%  = ATHER_DEV_WNA1330.ndi,  PCI\VEN_168C&DEV_001A&SUBSYS_3A1C1186
; Alpha/ATKK
%ATIWC.DeviceDesc.ATICB%    = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_12041259
%ATIWC.DeviceDesc.ATIPC%    = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_12031259
; Motion Computing
%ATHER.DeviceDesc.3062%     = ATHER_DEV_7111144F.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_7111144F
; Azurewave
%ATHER.DeviceDesc.3067%     = ATHER_DEV_10261A3B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_10261A3B
%ATHER.DeviceDesc.3067%     = ATHER_DEV_10261A3B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_10601A3B
%ATHER.DeviceDesc.0024%     = ATHER_DEV_10241A3B.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_10241A3B
%ATHER.DeviceDesc.3091%     = ATHER_DEV_10671A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10671A3B
%ATHER.DeviceDesc.3091%     = ATHER_DEV_10711A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10711A3B
%ATHER.DeviceDesc.3091%     = ATHER_DEV_10711A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10811A3B
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_10891A3B
%ATHER.DeviceDesc.3091%     = ATHER_DEV_10671A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10901A3B
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_20371A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_11061A3B
%ATHER.DeviceDesc.3091%     = ATHER_DEV_1A671A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1A671A3B
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_1A891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_1A891A3B
%ATHER.DeviceDesc.30A7%     = ATHER_DEV_11121A3B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_11121A3B
%ATHER.DeviceDesc.30A7%     = ATHER_DEV_11121A3B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_1A121A3B
%ATHER.DeviceDesc.3067%     = ATHER_DEV_10261A3B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_10331A3B
%ATHER.DeviceDesc.30AB%     = ATHER_DEV_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_20361A3B
%ATHER.DeviceDesc.30AB%     = ATHER_DEV_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_2C371A3B
%ATHER.DeviceDesc.30A4%     = ATHER_DEV_11211A3B.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_11211A3B
%ATHER.DeviceDesc.30A4%     = ATHER_DEV_1A211A3B.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_1A211A3B
; Huawei
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A5003485
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A5013485
%ATHER.DeviceDesc.663111AD% = ATHER_DEV_663111AD.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A5023485
; Panasonic
%ATHER.DeviceDesc.3091%     = ATHER_DEV_1C711A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1C711A3B
; QMI                            
%ATHER.DeviceDesc.3091%     = ATHER_DEV_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_03011A32
%ATHER.DeviceDesc.3091%     = ATHER_DEV_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_05041A32
%ATHER.DeviceDesc.3067%     = ATHER_DEV_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_21081A32
%ATHER.DeviceDesc.3067%     = ATHER_DEV_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_2A97103C
%ATHER.DeviceDesc.3067%     = ATHER_DEV_01121A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01121A32
%ATHER.DeviceDesc.3091%     = ATHER_DEV_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_05071A32
%ATHER.DeviceDesc.30A4%     = ATHER_DEV_03091A32.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_03091A32
%ATHER.DeviceDesc.30AB%     = ATHER_DEV_03051A32w.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_23001A32
; Arcadyan
%ATHER.DeviceDesc.3067%     = ATHER_DEV_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_C6011113
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_03051A32.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_D8111113
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_03051A32.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_F6111113
%ATHER.DeviceDesc.3091%     = ATHER_DEV_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_C8221113
%ATHER.DeviceDesc.3091%     = ATHER_DEV_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_D8221113
; Askey/Compal
%ATHER.DeviceDesc.3091%     = ATHER_DEV_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7168144F
;LiteOn
%ATHER.DeviceDesc.3067%     = ATHER_DEV_6313.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_630311AD
%ATHER.DeviceDesc.3067%     = ATHER_DEV_6313.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_631311AD
%ATHER.DeviceDesc.3067%     = ATHER_DEV_6313.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_633311AD
%ATHER.DeviceDesc.2061%     = ATHER_DEV_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_530111AD
%ATHER.DeviceDesc.2062%     = ATHER_DEV_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_540111AD
%ATHER.DeviceDesc.30A4%     = ATHER_DEV_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_661311AD
%ATHER.DeviceDesc.30AB%     = ATHER_DEV_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_660311AD
; Siemens
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_662111AD.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_662111AD
%ATHER.DeviceDesc.3091%     = ATHER_DEV_662111AD.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_662211AD
; Acer
%ATHER.DeviceDesc.E006105B% = ATHER_DEV_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_660011AD
%ATHER.DeviceDesc.E006105B% = ATHER_DEV_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E006105B
%ATHER.DeviceDesc.E006105B% = ATHER_DEV_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_03031A32  
%ATHER.DeviceDesc.E01F105B% = ATHER_DEV_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E01F105B
%ATHER.DeviceDesc.E01F105B% = ATHER_DEV_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_663211AD
%ATHER.DeviceDesc.E01F105B% = ATHER_DEV_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_03061A32
%ATHER.DeviceDesc.3067%     = ATHER_DEV_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01081A32 
%ATHER.DeviceDesc.3067%     = ATHER_DEV_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_04281468
%ATHER.DeviceDesc.3067%     = ATHER_DEV_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E008105B 
%ATHER.DeviceDesc.3067%     = ATHER_DEV_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E00D105B
%ATHER.DeviceDesc.663111AD% = ATHER_DEV_E016105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_663111AD
%ATHER.DeviceDesc.3067%     = ATHER_DEV_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_635311AD
%ATHER.DeviceDesc.3067%     = ATHER_DEV_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_660311AD
%ATHER.DeviceDesc.663111AD% = ATHER_DEV_E016105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E016105B
%ATHER.DeviceDesc.663111AD% = ATHER_DEV_E016105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E022105B
%ATHER.DeviceDesc.E01F105B% = ATHER_DEV_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_309D185F
%ATHER.DeviceDesc.30AB%     = ATHER_DEV_E031105Bw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_E031105B
%ATHER.DeviceDesc.660311AD% = ATHER_DEV_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_660311AD
%ATHER.DeviceDesc.660311AD% = ATHER_DEV_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_23091A32
%ATHER.DeviceDesc.660311AD% = ATHER_DEV_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_E034105B
%ATHER.DeviceDesc.663111AD% = ATHER_DEV_E016105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_23051A32
%ATHER.DeviceDesc.663111AD% = ATHER_DEV_E035105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E035105B
%ATHER.DeviceDesc.663111AD% = ATHER_DEV_E035105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_664111AD
%ATHER.DeviceDesc.663111AD% = ATHER_DEV_E035105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_63051A32
%ATHER.DeviceDesc.E01F105B% = ATHER_DEV_664211AD.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_664211AD
; Toshiba
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E004105B
%ATHER.DeviceDesc.7141144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E009105B
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7136144F
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7154144F
%ATHER.DeviceDesc.7141144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7141144F
%ATHER.DeviceDesc.3067%     = ATHER_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_41051A32
%ATHER.DeviceDesc.7141144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_43011A32
%ATHER.DeviceDesc.7141144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_43031A32
%ATHER.DeviceDesc.7141144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E012105B
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E013105B
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E015105B
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E014105B
%ATHER.DeviceDesc.7141144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7158144F
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7156144F
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7157144F
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_7159144F
%ATHER.DeviceDesc.3067%     = ATHER_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_632311AD
%ATHER.DeviceDesc.7141144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_662011AD
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_650211AD
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_653211AD
%ATHER.DeviceDesc.7141144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_661011AD
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_651211AD
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_652211AD
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_661111AD
%ATHER.DeviceDesc.7163144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_661211AD
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_660111AD
%ATHER.DeviceDesc.7163144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7163144F
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_7164144F
%ATHER.DeviceDesc.7163144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E019105B
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E01A105B
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_43051A32
%ATHER.DeviceDesc.7163144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_43061A32
%ATHER.DeviceDesc.3067%     = ATHER_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_A6011113
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E6111113
%ATHER.DeviceDesc.7141144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E6221113
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_D6221113
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E8111113
%ATHER.DeviceDesc.7163144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_F8221113
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_A8221113
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_B8221113
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_45071A32
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_65071A32
; Sony 11n
%ATHER.DeviceDesc.3091%     = ATHER_DEV_E007105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E007105B
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_S30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E017105B
%ATHER.DeviceDesc.30A4%     = ATHER_DEV_SS30A1.ndi,   PCI\VEN_168C&DEV_002E&SUBSYS_E030105B
; HP Desktop
%ATHER.DeviceDesc.2A5F103C% = ATHER_DEV_2A5F103C.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_2A5F103C
%ATHER.DeviceDesc.500011AD% = ATHER_DEV_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_500011AD
%ATHER.DeviceDesc.500111AD% = ATHER_DEV_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_500111AD
%ATHER.DeviceDesc.1000168c% = ATHER_DEV_1000168C.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1000168C
%ATHER.DeviceDesc.1000168c% = ATHER_DEV_1001168C.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1001168C
; Asus 11n
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7137144F
; Sharp(Mitac) 11n
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7138144F
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7139144F
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7140144F 
; Fujitsu 11n   
%ATHER.DeviceDesc.3072%     = ATHER_DEV_13C010CF.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_13C010CF
%ATHER.DeviceDesc.3091%     = ATHER_DEV_147C10CF.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_147C10CF
%ATHER.DeviceDesc.3091%     = ATHER_DEV_147D10CF.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_147D10CF
%ATHER.DeviceDesc.0023%     = ATHER_DEV_13C010CF.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_147E10CF
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_153710CF.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_153710CF
%ATHER.DeviceDesc.7163144F% = ATHER_DEV_147D10CF.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_153610CF
%ATHER.DeviceDesc.30A4%     = ATHER_DEV_153710CF.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_158F10CF
; WNC
%ATHER.DeviceDesc.CM9%	    = ATHER_DEV_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1012185F
%ATHER.DeviceDesc.CM9%	    = ATHER_DEV_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1012185E
%ATHER.DeviceDesc.30AB%     = ATHER_DEV_03051A32w.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_30AE185F
; TPLINK
%ATHER.DeviceDesc.1ACE%     = ATHER_DEV_T3091.ndi,    PCI\VEN_168C&DEV_0029&SUBSYS_92231ACE
; Pegatron
%ATHER.DeviceDesc.00341B0A% = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_00341B0A
; I-O DATA
%ATHER.DeviceDesc.D05B10FC% = ATHER_DEV_D05B10FC.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_D05B10FC
; SEMCO
%ATHER.DeviceDesc.30AB%     = ATHER_DEV_BA91167D.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_BA91167D
[Gigabyte]
%GIGA.DeviceDesc.E801%      = GIGA_DEV_E801.ndi,      PCI\VEN_168C&DEV_0013&SUBSYS_E8011458
%GIGA.DeviceDesc.E811%      = GIGA_DEV_E811.ndi,      PCI\VEN_168C&DEV_0013&SUBSYS_E8111458
%GIGA.DeviceDesc.E814%      = GIGA_DEV_E814.ndi,      PCI\VEN_168C&DEV_0013&SUBSYS_E8141458
%GIGA.DeviceDesc.0013%      = GIGA_DEV_0013.ndi,      PCI\VEN_168C&DEV_0013&SUBSYS_E9011458
%GIGA.DeviceDesc.E901%      = GIGA_DEV_E901.ndi,      PCI\VEN_168C&DEV_001B&SUBSYS_E9011458
%GIGA.DeviceDesc.E911%      = GIGA_DEV_E911.ndi,      PCI\VEN_168C&DEV_0013&SUBSYS_E9111458
%GIGA.DeviceDesc.E912%      = GIGA_DEV_E912.ndi,      PCI\VEN_168C&DEV_0013&SUBSYS_E9121458
%GIGA.DeviceDesc.E913%      = GIGA_DEV_E913.ndi,      PCI\VEN_168C&DEV_001C&SUBSYS_E9131458
%GIGA.DeviceDesc.E917%      = GIGA_DEV_E917.ndi,      PCI\VEN_168C&DEV_001C&SUBSYS_E9171458
%GIGA.DeviceDesc.E815%      = GIGA_DEV_E914.ndi,      PCI\VEN_168C&DEV_0024&SUBSYS_E8151458
%GIGA.DeviceDesc.E914%      = GIGA_DEV_E914.ndi,      PCI\VEN_168C&DEV_0023&SUBSYS_E9141458
%GIGA.DeviceDesc.E915%      = GIGA_DEV_E914.ndi,      PCI\VEN_168C&DEV_0024&SUBSYS_E9151458
%GIGA.DeviceDesc.E916%      = GIGA_DEV_E916.ndi,      PCI\VEN_168C&DEV_0024&SUBSYS_E9161458
%GIGA.DeviceDesc.E918%      = GIGA_DEV_E918.ndi,      PCI\VEN_168C&DEV_001C&SUBSYS_E9181458
%GIGA.DeviceDesc.E9191458% = ATHER_DEV_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E9191458 

[Atheros.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
; Generic
%ATHER.DeviceDesc.0013%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013
%ATHER.DeviceDesc.0013%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0014
%ATHER.DeviceDesc.0013%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0015
%ATHER.DeviceDesc.0013%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0016
%ATHER.DeviceDesc.0013%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0017
%ATHER.DeviceDesc.0013%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0018
%ATHER.DeviceDesc.0013%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0019
%ATHER.DeviceDesc.001A%     = ATHER_DEV_001A.ndi,     PCI\VEN_168C&DEV_001A
%ATHER.DeviceDesc.001B%     = ATHER_DEV_001B.ndi,     PCI\VEN_168C&DEV_001B
%ATHER.DeviceDesc.001B%     = ATHER_DEV_001B.ndi,     PCI\VEN_168C&DEV_001C
%ATHER.DeviceDesc.001B%     = ATHER_DEV_001B.ndi,     PCI\VEN_168C&DEV_FF19
%ATHER.DeviceDesc.001D%     = ATHER_DEV_001D.ndi,     PCI\VEN_168C&DEV_001D
%ATHER.DeviceDesc.0023%     = ATHER_DEV_0023.ndi,     PCI\VEN_168C&DEV_0023
%ATHER.DeviceDesc.0023%     = ATHER_DEV_0023.ndi,     PCI\VEN_168C&DEV_0024
%ATHER.DeviceDesc.0023%     = ATHER_DEV_0023.ndi,     PCI\VEN_168C&DEV_FF1C
%ATHER.DeviceDesc.0023%     = ATHER_DEV_0023.ndi,     PCI\VEN_168C&DEV_FF1D
; Atheros
%ATHER.DeviceDesc.1025%     = ATHER_DEV_1025.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1025168C
%ATHER.DeviceDesc.2025%     = ATHER_DEV_2025.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2025168C
%ATHER.DeviceDesc.1026%     = ATHER_DEV_1026.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1026168C
%ATHER.DeviceDesc.2026%     = ATHER_DEV_2026.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2026168C
%ATHER.DeviceDesc.1027%     = ATHER_DEV_1027.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1027168C
%ATHER.DeviceDesc.2027%     = ATHER_DEV_2027.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2027168C
%ATHER.DeviceDesc.1030%     = ATHER_DEV_1030.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1030168C
%ATHER.DeviceDesc.2030%     = ATHER_DEV_2030.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2030168C
%ATHER.DeviceDesc.1031%     = ATHER_DEV_1031.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1031168C
%ATHER.DeviceDesc.2031%     = ATHER_DEV_2031.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2031168C
%ATHER.DeviceDesc.1041%     = ATHER_DEV_1041.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1041168C
%ATHER.DeviceDesc.2041%     = ATHER_DEV_2041.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2041168C
%ATHER.DeviceDesc.1042%     = ATHER_DEV_1042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1042168C
%ATHER.DeviceDesc.2042%     = ATHER_DEV_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2042168C
%ATHER.DeviceDesc.1051%     = ATHER_DEV_1051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1051168C
%ATHER.DeviceDesc.2051%     = ATHER_DEV_2051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2051168C
%ATHER.DeviceDesc.001A%     = ATHER_DEV_1052.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_1052168C
%ATHER.DeviceDesc.001A%     = ATHER_DEV_2052.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_2052168C
%ATHER.DeviceDesc.1053%     = ATHER_DEV_1053.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1053168C
%ATHER.DeviceDesc.2053%     = ATHER_DEV_2053.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2053168C
%ATHER.DeviceDesc.001A%     = ATHER_DEV_1054.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_1054168C
%ATHER.DeviceDesc.001A%     = ATHER_DEV_2054.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_2054168C
%ATHER.DeviceDesc.1062%     = ATHER_DEV_1062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1062168C
%ATHER.DeviceDesc.2062%     = ATHER_DEV_2062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2062168C
%ATHER.DeviceDesc.001B%     = ATHER_DEV_1063.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1063168C
%ATHER.DeviceDesc.001B%     = ATHER_DEV_2063.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2063168C
%ATHER.DeviceDesc.3062%     = ATHER_DEV_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3062168c
%ATHER.DeviceDesc.3063%     = ATHER_DEV_2063.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3063168c
%ATHER.DeviceDesc.3061%     = ATHER_DEV_2051.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3061168c
%ATHER.DeviceDesc.3065%     = ATHER_DEV_2052.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3065168c
%ATHER.DeviceDesc.2061%     = ATHER_DEV_2051.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2061168c
%ATHER.DeviceDesc.1061%     = ATHER_DEV_1051.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1061168c
%ATHER.DeviceDesc.2065%     = ATHER_DEV_2052.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2065168c
%ATHER.DeviceDesc.1065%     = ATHER_DEV_1052.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1065168c
%ATHER.DeviceDesc.3067%     = ATHER_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3067168C
%ATHER.DeviceDesc.3067%     = ATHER_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3064168C
%ATHER.DeviceDesc.2055%     = ATHER_DEV_2055.ndi,     PCI\VEN_168C&DEV_001D&SUBSYS_2055168c
%ATHER.DeviceDesc.1055%     = ATHER_DEV_1055.ndi,     PCI\VEN_168C&DEV_001D&SUBSYS_1055168c
; Others  
%ATHER.DeviceDesc.2026%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7005144F
%ATHER.DeviceDesc.2026%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7057144F
%ATHER.DeviceDesc.2026%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7058144F
%ATHER.DeviceDesc.2041%     = ATHER_DEV_2041.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7064144F
%ATHER.DeviceDesc.2042%     = ATHER_DEV_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7065144F
%ATHER.DeviceDesc.2051%     = ATHER_DEV_2051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7084144F
%ATHER.DeviceDesc.2051%     = ATHER_DEV_2051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7088144F
%ATHER.DeviceDesc.2062%     = ATHER_DEV_2062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_7092144F
%ATHER.DeviceDesc.001A%     = ATHER_DEV_2054.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_7094144F
%ATHER.DeviceDesc.2042%     = ATHER_DEV_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7005168C
%ATHER.DeviceDesc.3063%     = ATHER_DEV_2063.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7096144F
%ATHER.DeviceDesc.3065%     = ATHER_DEV_2052.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7106144F
%ATHER.DeviceDesc.3067%     = ATHER_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7128144f
%ATHER.DeviceDesc.0013%     = ATHER_DEV_F013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_123410CF
%ATHER.DeviceDesc.0013%     = ATHER_DEV_F013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_123510CF
%ATHER.DeviceDesc.10CF%     = ATHER_DEV_F013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_123610CF
%ATHER.DeviceDesc.001B%     = ATHER_DEV_F013.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_132910CF
%ATHER.DeviceDesc.10CF%     = ATHER_DEV_F013.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_134F10CF
%ATHER.DeviceDesc.3062%     = ATHER_DEV_F013C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_139C10CF
%ATHER.DeviceDesc.3067%     = ATHER_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_142E10CF
%ATHER.DeviceDesc.3062%     = ATHER_DEV_04221468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_04221468
%ATHER.DeviceDesc.001A%     = ATHER_DEV_04171468.ndi, PCI\VEN_168C&DEV_001A&SUBSYS_04171468
%ATHER.DeviceDesc.001A%     = ATHER_DEV_04171468.ndi, PCI\VEN_168C&DEV_001A&SUBSYS_04181468
%ATHER.DeviceDesc.001A%     = ATHER_DEV_04171468.ndi, PCI\VEN_168C&DEV_001A&SUBSYS_04201468
%ATHER.DeviceDesc.3067%     = ATHER_DEV_042A1468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_042A1468
%ATHER.DeviceDesc.E000%     = ATHER_DEV_E000105B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E000105B
%ATHER.DeviceDesc.E000%     = ATHER_DEV_E002105B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E002105B
%ATHER.DeviceDesc.0406%     = ATHER_DEV_04061468.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_04061468
%ATHER.DeviceDesc.0407%     = ATHER_DEV_04071468.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_04071468
%ATHER.DeviceDesc.E000%     = ATHER_DEV_04231468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_04231468
%ATHER.DeviceDesc.E000%     = ATHER_DEV_04231468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_0423168C
%ATHER.DeviceDesc.3063%     = ATHER_DEV_2063.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_04271468
%ATHER.DeviceDesc.3065%     = ATHER_DEV_2052.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_04251468
%ATHER.DeviceDesc.001A%     = ATHER_DEV_2052.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_04261468
%ATHER.DeviceDesc.3067%     = ATHER_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_042A1468
%ATHER.DeviceDesc.0055%     = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_123610CF
%ATHER.DeviceDesc.0055%     = ATHER_DEV_001B.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_134f10CF
%ATHER.DeviceDesc.3072%     = ATHER_DEV_7125144F.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_7125144F
%ATHER.DeviceDesc.3072%     = ATHER_DEV_7125144F.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_04291468
%ATHER.DeviceDesc.3072%     = ATHER_DEV_0023.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_04301468
%ATHER.DeviceDesc.3072%     = ATHER_DEV_05021A32.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_05021A32
%ATHER.DeviceDesc.3065%     = ATHER_DEV_01001A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01001A32
%ATHER.DeviceDesc.3063%     = ATHER_DEV_02001A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_02001A32
%ATHER.DeviceDesc.3067%     = ATHER_DEV_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01051A32
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3091168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3092168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3093168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3094168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3095168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3096168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3097168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3098168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3099168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309A168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309B168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309C168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309D168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309F168C
%ATHER.DeviceDesc.2091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2091168C
%ATHER.DeviceDesc.2091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2092168C
%ATHER.DeviceDesc.2091%     = ATHER_DEV_3091PB.ndi,   PCI\VEN_168C&DEV_0029&SUBSYS_2093168C
%ATHER.DeviceDesc.2091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2094168C
%ATHER.DeviceDesc.2091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2096168C
%ATHER.DeviceDesc.2091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2098168C
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30A1168C
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30A2168C
%ATHER.DeviceDesc.30AB%     = ATHER_DEV_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30AB168C
%ATHER.DeviceDesc.30AD%     = ATHER_DEV_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30AD168C
%ATHER.DeviceDesc.30AE%     = ATHER_DEV_30AA.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30AE168C
%ATHER.DeviceDesc.30AF%     = ATHER_DEV_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30AF168C
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_30A3168C
%ATHER.DeviceDesc.30A7%     = ATHER_DEV_001C.ndi,     PCI\VEN_168C&DEV_002C&SUBSYS_30A7168C
%ATHER.DeviceDesc.2099%     = ATHER_DEV_30A1.ndi,     PCI\VEN_168C&DEV_002D&SUBSYS_2099168C
%ATHER.DeviceDesc.30A4%     = ATHER_DEV_30A1.ndi,     PCI\VEN_168C&DEV_002E&SUBSYS_30A4168C
; NEC
%ATHER.DeviceDesc.3062%     = ATHER_DEV_N2062.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_102010E9
%ATHER.DeviceDesc.3062%     = ATHER_DEV_N2062.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_102510E9
%ATHER.DeviceDesc.3072%     = ATHER_DEV_N3072.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_102210E9
%ATHER.DeviceDesc.3072%     = ATHER_DEV_N3073.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_102610E9
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_03051A32.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_03051A32
; Foxconn
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_E023105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E023105B
%ATHER.DeviceDesc.30A7%     = ATHER_DEV_E029105B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_E029105B
%ATHER.DeviceDesc.30A7%     = ATHER_DEV_1029105B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_1029105B
%ATHER.DeviceDesc.30AB%     = ATHER_DEV_E033105Bw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_E033105B
; Apple
%ATHER.DeviceDesc.3072%     = ATHER_DEV_0023.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_00000000
%ATHER.DeviceDesc.3062%     = ATHER_DEV_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_0086106B
%ATHER.DeviceDesc.3072%     = ATHER_DEV_0023.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_0087106B
%ATHER.DeviceDesc.3091%     = ATHER_DEV_008F106B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_008F106B
; AMD
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091amd.ndi,  PCI\VEN_168C&DEV_002A&SUBSYS_1130168C
; Netgear
%ATHER.DeviceDesc.90001385% = ATHER_DEV_90001385.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_90001385
%ATHER.DeviceDesc.4B001385% = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_4B001385
%ATHER.DeviceDesc.4B001385% = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5B001385
%ATHER.DeviceDesc.5D001385% = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5D001385
%ATHER.DeviceDesc.4D001385% = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_4D001385
%ATHER.DeviceDesc.4F001385% = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_4F001385
%ATHER.DeviceDesc.5E001385% = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5E001385
%ATHER.DeviceDesc.4D001385% = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5A001385
;OQO
%ATHER.DeviceDesc.2062%     = ATHER_DEV_2062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1602196f
%ATHER.DeviceDesc.2062%     = ATHER_DEV_2062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1603196f
%ATHER.DeviceDesc.3062%     = ATHER_DEV_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_1604196f
; Lenovo Japan
%ATHER.DeviceDesc.5013%     = ATHER_DEV_5013.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_0034168c
%ATHER.DeviceDesc.6013%     = ATHER_DEV_6013.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_0035168c
%ATHER.DeviceDesc.3013%     = ATHER_DEV_3013.ndi,     PCI\VEN_168C&DEV_1014&SUBSYS_05891014
%ATHER.DeviceDesc.4013%     = ATHER_DEV_4013.ndi,     PCI\VEN_168C&DEV_1014&SUBSYS_058A1014
%ATHER.DeviceDesc.2013%     = ATHER_DEV_2013.ndi,     PCI\VEN_168C&DEV_1014&SUBSYS_057E1014
%ATHER.DeviceDesc.1013%     = ATHER_DEV_1013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_04081468
%ATHER.DeviceDesc.0032168c% = ATHER_DEV_0032168c.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_0032168c
%ATHER.DeviceDesc.0033168c% = ATHER_DEV_0033168c.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_0033168c
%ATHER.DeviceDesc.0036%     = ATHER_DEV_0036.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_0036168c
%ATHER.DeviceDesc.0037%     = ATHER_DEV_0037.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_0037168c
; Lenovo China
%ATHER.DeviceDesc.309917AA% = ATHER_DEV_309917AA.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_309917AA
%ATHER.DeviceDesc.3067%     = ATHER_DEV_316417AA.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_316417AA
%ATHER.DeviceDesc.3091%     = ATHER_DEV_309D17AA.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_309D17AA
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_30A117AA.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_30A117AA
; IBM
%ATHER.DeviceDesc.0033168c% = ATHER_DEV_03841014.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_03841014
; Samsung
%ATHER.DeviceDesc.001A%     = ATHER_DEV_S001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7101144F
%ATHER.DeviceDesc.001A%     = ATHER_DEV_S001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7114144F
%ATHER.DeviceDesc.001A%     = ATHER_DEV_S001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7115144F
%ATHER.DeviceDesc.3067%     = ATHER_DEV_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_7131144F
%ATHER.DeviceDesc.3067%     = ATHER_DEV_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_7130144F
%ATHER.DeviceDesc.001B%     = ATHER_DEV_S001B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7108144F
%ATHER.DeviceDesc.001B%     = ATHER_DEV_S001B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7116144F
%ATHER.DeviceDesc.3067%     = ATHER_DEV_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_E00B105B
%ATHER.DeviceDesc.3067%     = ATHER_DEV_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_E00C105B
%ATHER.DeviceDesc.001B%     = ATHER_DEV_S3067a.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_E00E105B
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091SF.ndi,   PCI\VEN_168C&DEV_002A&SUBSYS_E00F105B
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091SF.ndi,   PCI\VEN_168C&DEV_002A&SUBSYS_E010105B
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091SF.ndi,   PCI\VEN_168C&DEV_002A&SUBSYS_7161144F
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_30A1a.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_7167144F
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_30A1a.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E025105B
%ATHER.DeviceDesc.30AB%     = ATHER_DEV_30A1w.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E032105B
; Askey
%ATHER.DeviceDesc.7173144F% = ATHER_DEV_7173144Fw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_7173144F
; D-Link
%ATHER.DeviceDesc.DWA642%   = ATHER_DEV_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A6A1186
%ATHER.DeviceDesc.DWA645%   = ATHER_DEV_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A0907D1
%ATHER.DeviceDesc.DWA645%   = ATHER_DEV_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A761186
%ATHER.DeviceDesc.DWA645%   = ATHER_DEV_3A7B1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A791186
%ATHER.DeviceDesc.DWA542%   = ATHER_DEV_3A691186.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_3A691186
%ATHER.DeviceDesc.DWA547%   = ATHER_DEV_3A6D1186.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_3A6B1186
%ATHER.DeviceDesc.DWA547%   = ATHER_DEV_3A7A1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A781186
%ATHER.DeviceDesc.DWA652%   = ATHER_DEV_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A6E1186
%ATHER.DeviceDesc.DWA652%   = ATHER_DEV_3A7B1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A7B1186
%ATHER.DeviceDesc.DWA552%   = ATHER_DEV_3A6D1186.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_3A6D1186
%ATHER.DeviceDesc.DWA552%   = ATHER_DEV_3A7A1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A7A1186
%ATHER.DeviceDesc.DWA643%   = ATHER_DEV_3A6F1186.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_3A6F1186
%ATHER.DeviceDesc.DWA556%   = ATHER_DEV_3A701186.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_3A701186
%ATHER.DeviceDesc.DWA520%   = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A731186
%ATHER.DeviceDesc.DWA620%   = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A741186
%ATHER.DeviceDesc.WDA1320%  = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A1D1186
%ATHER.DeviceDesc.WDA2320%  = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A1B1186
%ATHER.DeviceDesc.WNA2330%  = ATHER_DEV_WNA2330.ndi,  PCI\VEN_168C&DEV_0013&SUBSYS_3A1A1186
%ATHER.DeviceDesc.WNA1330%  = ATHER_DEV_WNA1330.ndi,  PCI\VEN_168C&DEV_001A&SUBSYS_3A1C1186
; Alpha/ATKK
%ATIWC.DeviceDesc.ATICB%    = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_12041259
%ATIWC.DeviceDesc.ATIPC%    = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_12031259
; Motion Computing
%ATHER.DeviceDesc.3062%     = ATHER_DEV_7111144F.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_7111144F
; Azurewave
%ATHER.DeviceDesc.3067%     = ATHER_DEV_10261A3B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_10261A3B
%ATHER.DeviceDesc.3067%     = ATHER_DEV_10261A3B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_10601A3B
%ATHER.DeviceDesc.0024%     = ATHER_DEV_10241A3B.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_10241A3B
%ATHER.DeviceDesc.3091%     = ATHER_DEV_10671A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10671A3B
%ATHER.DeviceDesc.3091%     = ATHER_DEV_10711A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10711A3B
%ATHER.DeviceDesc.3091%     = ATHER_DEV_10711A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10811A3B
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_10891A3B
%ATHER.DeviceDesc.3091%     = ATHER_DEV_10671A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10901A3B
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_20371A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_11061A3B
%ATHER.DeviceDesc.3091%     = ATHER_DEV_1A671A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1A671A3B
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_1A891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_1A891A3B
%ATHER.DeviceDesc.30A7%     = ATHER_DEV_11121A3B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_11121A3B
%ATHER.DeviceDesc.30A7%     = ATHER_DEV_11121A3B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_1A121A3B
%ATHER.DeviceDesc.3067%     = ATHER_DEV_10261A3B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_10331A3B
%ATHER.DeviceDesc.30AB%     = ATHER_DEV_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_20361A3B
%ATHER.DeviceDesc.30AB%     = ATHER_DEV_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_2C371A3B
%ATHER.DeviceDesc.30A4%     = ATHER_DEV_11211A3B.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_11211A3B
%ATHER.DeviceDesc.30A4%     = ATHER_DEV_1A211A3B.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_1A211A3B
;Huawei
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A5003485
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A5013485
%ATHER.DeviceDesc.663111AD% = ATHER_DEV_663111AD.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A5023485
; Panasonic
%ATHER.DeviceDesc.3091%     = ATHER_DEV_1C711A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1C711A3B
; QMI                            
%ATHER.DeviceDesc.3091%     = ATHER_DEV_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_03011A32
%ATHER.DeviceDesc.3091%     = ATHER_DEV_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_05041A32
%ATHER.DeviceDesc.3067%     = ATHER_DEV_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_21081A32
%ATHER.DeviceDesc.3067%     = ATHER_DEV_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_2A97103C
%ATHER.DeviceDesc.3067%     = ATHER_DEV_01121A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01121A32
%ATHER.DeviceDesc.3091%     = ATHER_DEV_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_05071A32
%ATHER.DeviceDesc.30A4%     = ATHER_DEV_03091A32.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_03091A32
%ATHER.DeviceDesc.30AB%     = ATHER_DEV_03051A32w.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_23001A32
; Arcadyan
%ATHER.DeviceDesc.3067%     = ATHER_DEV_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_C6011113
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_03051A32.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_D8111113
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_03051A32.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_F6111113
%ATHER.DeviceDesc.3091%     = ATHER_DEV_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_C8221113
%ATHER.DeviceDesc.3091%     = ATHER_DEV_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_D8221113
; Askey/Compal
%ATHER.DeviceDesc.3091%     = ATHER_DEV_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7168144F
;LiteOn
%ATHER.DeviceDesc.3067%     = ATHER_DEV_6313.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_630311AD
%ATHER.DeviceDesc.3067%     = ATHER_DEV_6313.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_631311AD
%ATHER.DeviceDesc.3067%     = ATHER_DEV_6313.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_633311AD
%ATHER.DeviceDesc.2061%     = ATHER_DEV_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_530111AD
%ATHER.DeviceDesc.2062%     = ATHER_DEV_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_540111AD
%ATHER.DeviceDesc.30A4%     = ATHER_DEV_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_661311AD
%ATHER.DeviceDesc.30AB%     = ATHER_DEV_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_660311AD
; Siemens
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_662111AD.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_662111AD
%ATHER.DeviceDesc.3091%     = ATHER_DEV_662111AD.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_662211AD
; Acer
%ATHER.DeviceDesc.E006105B% = ATHER_DEV_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_660011AD
%ATHER.DeviceDesc.E006105B% = ATHER_DEV_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E006105B
%ATHER.DeviceDesc.E006105B% = ATHER_DEV_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_03031A32  
%ATHER.DeviceDesc.E01F105B% = ATHER_DEV_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E01F105B
%ATHER.DeviceDesc.E01F105B% = ATHER_DEV_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_663211AD
%ATHER.DeviceDesc.E01F105B% = ATHER_DEV_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_03061A32
%ATHER.DeviceDesc.3067%     = ATHER_DEV_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01081A32 
%ATHER.DeviceDesc.3067%     = ATHER_DEV_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_04281468
%ATHER.DeviceDesc.3067%     = ATHER_DEV_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E008105B 
%ATHER.DeviceDesc.3067%     = ATHER_DEV_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E00D105B
%ATHER.DeviceDesc.663111AD% = ATHER_DEV_E016105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_663111AD
%ATHER.DeviceDesc.3067%     = ATHER_DEV_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_635311AD
%ATHER.DeviceDesc.3067%     = ATHER_DEV_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_660311AD
%ATHER.DeviceDesc.663111AD% = ATHER_DEV_E016105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E016105B
%ATHER.DeviceDesc.663111AD% = ATHER_DEV_E016105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E022105B
%ATHER.DeviceDesc.E01F105B% = ATHER_DEV_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_309D185F
%ATHER.DeviceDesc.30AB%     = ATHER_DEV_E031105Bw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_E031105B
%ATHER.DeviceDesc.660311AD% = ATHER_DEV_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_660311AD
%ATHER.DeviceDesc.660311AD% = ATHER_DEV_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_23091A32
%ATHER.DeviceDesc.660311AD% = ATHER_DEV_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_E034105B
%ATHER.DeviceDesc.663111AD% = ATHER_DEV_E016105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_23051A32
%ATHER.DeviceDesc.663111AD% = ATHER_DEV_E035105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E035105B
%ATHER.DeviceDesc.663111AD% = ATHER_DEV_E035105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_664111AD
%ATHER.DeviceDesc.663111AD% = ATHER_DEV_E035105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_63051A32
%ATHER.DeviceDesc.E01F105B% = ATHER_DEV_664211AD.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_664211AD
; Toshiba
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E004105B
%ATHER.DeviceDesc.7141144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E009105B
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7136144F
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7154144F
%ATHER.DeviceDesc.7141144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7141144F
%ATHER.DeviceDesc.3067%     = ATHER_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_41051A32
%ATHER.DeviceDesc.7141144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_43011A32
%ATHER.DeviceDesc.7141144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_43031A32
%ATHER.DeviceDesc.7141144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E012105B
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E013105B
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E015105B
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E014105B
%ATHER.DeviceDesc.7141144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7158144F
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7156144F
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7157144F
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_7159144F
%ATHER.DeviceDesc.3067%     = ATHER_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_632311AD
%ATHER.DeviceDesc.7141144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_662011AD
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_650211AD
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_653211AD
%ATHER.DeviceDesc.7141144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_661011AD
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_651211AD
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_652211AD
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_661111AD
%ATHER.DeviceDesc.7163144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_661211AD
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_660111AD
%ATHER.DeviceDesc.7163144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7163144F
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_7164144F
%ATHER.DeviceDesc.7163144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E019105B
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E01A105B
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_43051A32
%ATHER.DeviceDesc.7163144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_43061A32
%ATHER.DeviceDesc.3067%     = ATHER_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_A6011113
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E6111113
%ATHER.DeviceDesc.7141144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E6221113
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_D6221113
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E8111113
%ATHER.DeviceDesc.7163144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_F8221113
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_A8221113
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_B8221113
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_45071A32
%ATHER.DeviceDesc.7136144F% = ATHER_DEV_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_65071A32
; Sony 11n
%ATHER.DeviceDesc.3091%     = ATHER_DEV_E007105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E007105B
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_S30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E017105B
%ATHER.DeviceDesc.30A4%     = ATHER_DEV_SS30A1.ndi,   PCI\VEN_168C&DEV_002E&SUBSYS_E030105B
; HP Desktop
%ATHER.DeviceDesc.2A5F103C% = ATHER_DEV_2A5F103C.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_2A5F103C
%ATHER.DeviceDesc.500011AD% = ATHER_DEV_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_500011AD
%ATHER.DeviceDesc.500111AD% = ATHER_DEV_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_500111AD
%ATHER.DeviceDesc.1000168c% = ATHER_DEV_1000168C.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1000168C
%ATHER.DeviceDesc.1000168c% = ATHER_DEV_1001168C.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1001168C
; Asus 11n
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7137144F
; Sharp(Mitac) 11n
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7138144F
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7139144F
%ATHER.DeviceDesc.3091%     = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7140144F 
; Fujitsu 11n   
%ATHER.DeviceDesc.3072%     = ATHER_DEV_13C010CF.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_13C010CF
%ATHER.DeviceDesc.3091%     = ATHER_DEV_147C10CF.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_147C10CF
%ATHER.DeviceDesc.3091%     = ATHER_DEV_147D10CF.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_147D10CF
%ATHER.DeviceDesc.0023%     = ATHER_DEV_13C010CF.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_147E10CF
%ATHER.DeviceDesc.30A1%     = ATHER_DEV_153710CF.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_153710CF
%ATHER.DeviceDesc.7163144F% = ATHER_DEV_147D10CF.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_153610CF
%ATHER.DeviceDesc.30A4%     = ATHER_DEV_153710CF.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_158F10CF
; WNC
%ATHER.DeviceDesc.CM9%	    = ATHER_DEV_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1012185F
%ATHER.DeviceDesc.CM9%	    = ATHER_DEV_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1012185E
%ATHER.DeviceDesc.30AB%     = ATHER_DEV_03051A32w.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_30AE185F
; TPLINK
%ATHER.DeviceDesc.1ACE%     = ATHER_DEV_T3091.ndi,    PCI\VEN_168C&DEV_0029&SUBSYS_92231ACE
; Pegatron
%ATHER.DeviceDesc.00341B0A% = ATHER_DEV_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_00341B0A
; I-O DATA
%ATHER.DeviceDesc.D05B10FC% = ATHER_DEV_D05B10FC.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_D05B10FC
; SEMCO
%ATHER.DeviceDesc.30AB%     = ATHER_DEV_BA91167D.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_BA91167D
[Gigabyte.NTamd64]
%GIGA.DeviceDesc.E801%      = GIGA_DEV_E801.ndi,      PCI\VEN_168C&DEV_0013&SUBSYS_E8011458
%GIGA.DeviceDesc.E811%      = GIGA_DEV_E811.ndi,      PCI\VEN_168C&DEV_0013&SUBSYS_E8111458
%GIGA.DeviceDesc.E814%      = GIGA_DEV_E814.ndi,      PCI\VEN_168C&DEV_0013&SUBSYS_E8141458
%GIGA.DeviceDesc.0013%      = GIGA_DEV_0013.ndi,      PCI\VEN_168C&DEV_0013&SUBSYS_E9011458
%GIGA.DeviceDesc.E901%      = GIGA_DEV_E901.ndi,      PCI\VEN_168C&DEV_001B&SUBSYS_E9011458
%GIGA.DeviceDesc.E911%      = GIGA_DEV_E911.ndi,      PCI\VEN_168C&DEV_0013&SUBSYS_E9111458
%GIGA.DeviceDesc.E912%      = GIGA_DEV_E912.ndi,      PCI\VEN_168C&DEV_0013&SUBSYS_E9121458
%GIGA.DeviceDesc.E913%      = GIGA_DEV_E913.ndi,      PCI\VEN_168C&DEV_001C&SUBSYS_E9131458
%GIGA.DeviceDesc.E917%      = GIGA_DEV_E917.ndi,      PCI\VEN_168C&DEV_001C&SUBSYS_E9171458
%GIGA.DeviceDesc.E815%      = GIGA_DEV_E914.ndi,      PCI\VEN_168C&DEV_0024&SUBSYS_E8151458
%GIGA.DeviceDesc.E914%      = GIGA_DEV_E914.ndi,      PCI\VEN_168C&DEV_0023&SUBSYS_E9141458
%GIGA.DeviceDesc.E915%      = GIGA_DEV_E914.ndi,      PCI\VEN_168C&DEV_0024&SUBSYS_E9151458
%GIGA.DeviceDesc.E916%      = GIGA_DEV_E916.ndi,      PCI\VEN_168C&DEV_0024&SUBSYS_E9161458
%GIGA.DeviceDesc.E918%      = GIGA_DEV_E918.ndi,      PCI\VEN_168C&DEV_001C&SUBSYS_E9181458
%GIGA.DeviceDesc.E9191458%  = ATHER_DEV_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E9191458 

; Windows NT specific entries

[ATHER_DEV_0013.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_001A.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_001B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1025.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2025.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1026.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2026.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1027.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2027.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1030.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2030.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1031.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2031.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1041.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2041.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1051.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2051.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1042.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2042.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1052.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2052.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_001C.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E023105B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func1_1.reg, overrideAC.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E033105Bw.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func1_1.reg, overrideAC.reg, janusda.reg, triggerlevelkiteonly.reg, c3war.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E029105B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg, cemspecled_func1_1.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1029105B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg, cemspecled_func1_1.reg, overrideAC.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_11121A3B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg, cemspecled_func1_1.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_6313.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg, cemspecled_func1_3.reg, d3hot.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1053.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2053.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1054.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2054.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1062.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2062.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_7111144F.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, Customer14.led.reg, 5212.abgmp.reg, uapsd.reg, expresscardaspmoff.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_04221468.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgmp.reg, customer3.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_04171468.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, customer3.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_04281468.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgmp.reg, customer3e.reg, uapsd.reg, d3hot.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_01001A32.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, customer10.LED3.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_02001A32.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgmp.reg, customer10.LED3.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_01051A32.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgmp.reg, customer3a.reg, uapsd.reg, d3hot.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_01121A32.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgmp.reg, customer3a.reg, uapsd.reg, d3hot.reg, customer3d.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_042A1468.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, customer9.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E000105B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, customer4b.reg, customer4_basic.reg, customer4a_ASPM.reg, uapsd.reg, d3hot.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E002105B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, customer4b.reg, customer4_basic.reg, customer4a_ASPM.reg, uapsd.reg, d3hot.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_04061468.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, customer4a.reg,customer4_basic.reg, customer4a_ASPM.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_04071468.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, COMMON_AG.reg, customer4a.reg,customer4_basic.reg, customer4a_ASPM.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_04231468.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, customer4a.reg,customer4_basic.reg, customer4a_ASPM.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E007105B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, customer4a.reg, sys.TcpParams.reg, customer4c.reg, uapsd.reg, customer4adhoc.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_S30A1.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, customer4adhoc.reg, customer4a.reg, triggerlevelkiteonly.reg, c3war.reg, cmdRegister.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_SS30A1.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, customer4adhoc.reg, customer4as.reg, triggerlevelkiteonly.reg, c3war.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_10261A3B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, 10261a3b.reg, uapsd.reg, d3hot.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1063.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2063.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_F013.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgcb.reg, customer1ani.reg, bandselect.reg, uapsd.reg, customer1roam.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_F013C.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgcb.reg, customer1ani.reg, bandselect.reg, uapsd.reg, customer1roam.reg, minpower.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_001D.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1055.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg, gpioled.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2055.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1013.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, customer0.PS1.reg, customer0.LED.reg, customer0.5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3013.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, customer0.PS1.reg, customer0.LED1.reg, customer0.5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2013.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, customer0.PS1.reg, customer0.LED.reg, customer0.5213.abg.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_4013.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, customer0.PS1.reg, customer0.LED1.reg, customer0.5213.abg.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_5013.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, customer0.PS1.reg, customer0.LED2.reg, customer0.5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_6013.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, customer0.PS1.reg, customer0.LED2.reg, customer0.5212.bgmp.reg, uapsd.reg, d3hot.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_0036.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, sys.TcpParams.reg, customer0.PS1.reg, customer0.LED1.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_0037.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, sys.TcpParams.reg, customer0.PS1.reg, customer0.LED1_HB95.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_0023.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgncb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_90001385.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgncb.reg, sys.TcpParams.reg, uapsd.reg, expresscardaspmoff.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_05021A32.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgncb.reg, sys.TcpParams.reg, customer10.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_0033168c.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgnxb.reg, sys.TcpParams.reg, customer0.reg, 5416.antennacontrols.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_0032168c.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, customer0.reg, 5416.antennacontrols.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_13C010CF.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgnxb.reg, sys.TcpParams.reg, 5416.antennacontrols.reg, uapsd.reg, customer1roam.reg, htAdhocdisable.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_147C10CF.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgnxb.reg, sys.TcpParams.reg, uapsd.reg, customer1roam.reg, htAdhocdisable.reg, smpsDynamic.reg, customer1fullreset.reg, merlinshiftdelay.reg, d3forcel1disable.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_147D10CF.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, customer1roam.reg, htAdhocdisable.reg, customer1fullreset.reg, merlinshiftdelay.reg, d3forcel1disable.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_153710CF.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, customer1roam.reg, htAdhocdisable.reg, customer1fullreset.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_7125144F.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgncb.reg, sys.TcpParams.reg, 5416.antennacontrols.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2A5F103C.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, customer2.11n.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_11AD.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, customer2.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_03841014.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgncb.reg, sys.TcpParams.reg, 5416.antennacontrols.reg, xb72.via.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E801.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led0.reg, 5211.reg, ATHER.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E811.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led0.reg, 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E814.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led0.reg, 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_0013.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led0.reg, 5211.reg, ATHER.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E901.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led0.reg, 5211.reg, ATHER.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E911.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led0.reg, 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E912.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led0.reg, 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E913.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led1.reg, 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E917.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led1.reg, 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E918.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led2.reg, 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E914.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, customer12Led0.reg, 5416.abgncb.reg, sys.TcpParams.reg, 5416.antennacontrols.reg, customer12.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E916.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, customer12Led1.reg, 5416.abgncb.reg, sys.TcpParams.reg, 5416.antennacontrols.reg, customer12.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_N2062.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer11.reg, customer11_legacywmode.reg, cemspecled_func1_1.reg, customer11Ant.reg, ATHER.reg, customer11ACStatus.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_N3072.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = customer11.reg, customer11_11nwmode.reg, cemspecled_func1_1.reg, ATHER.reg, sys.TcpParams.reg, customer11ACStatus.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_N3073.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = customer11.reg, customer11_11n40wmode.reg, cemspecled_func1_1.reg, ATHER.reg, sys.TcpParams.reg, customer11ACStatus.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1186.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, customer5.11nLED.reg, customer5.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3A691186.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, customer5.11nLED.reg, pcibusconfig.reg, customer5.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3A6D1186.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, customer5.11nLED.reg, pcibusconfig.reg, customer5.3x3.reg, customer5.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3A6F1186.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, customer5.PCIe11nLed.reg, customer5.reg, uapsd.reg, expresscardaspmoff.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3A701186.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, customer5.PCIe11nLed.reg, customer5.3x3.reg, customer5.reg, uapsd.reg, expresscardaspmoff.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3A7A1186.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = ATHER.reg, 5416.reg, 5416.bgnxb.reg, sys.TcpParams.reg, customer5.11nLED.reg, pcibusconfig.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3A7B1186.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = ATHER.reg, 5416.reg, 5416.bgnxb.reg, sys.TcpParams.reg, customer5.11nLED.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_WNA2330.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, wnaled.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_WNA1330.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, wnaled.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3091.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3091amd.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg, cemspecled_func1_1.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_008F106B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg, wowenable.reg, merlinshiftdelay.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_7136144F.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg, merlinshiftdelay.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_T3091.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, uapsd.reg, smpsDynamic.reg, pcibusconfig.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_309917AA.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgnxb.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func1_1.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1000168C.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgnxb.reg, sys.TcpParams.reg, uapsd.reg, customer2merlin.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1001168C.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgnxb.reg, sys.TcpParams.reg, uapsd.reg, customer2.11n.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3091PB.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, pushbutton.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_30A1.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_T30A1.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_660311AD.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, customer3f.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_03091A32.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, cemspecled_func1_8.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_30AA.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, triggerlevelkiteonly.reg, Customer15a.led.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_30AB.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, janusda.reg, triggerlevelkiteonly.reg, Customer15a.led.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_BA91167D.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, janusda.reg, cemspecled_func1_1.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_7173144Fw.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, janusda.reg, triggerlevelkiteonly.reg, c3war.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_30A1a.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, customer_Samsung.reg, uapsd.reg, htAdhoc.reg, scanasync.reg, cmdRegister.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_30A1w.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, customer_Samsung.reg, uapsd.reg, htAdhoc.reg, janusda.reg, scanasync.reg, cmdRegister.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_309D17AA.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, Customer15a.led.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_30A117AA.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, Customer15a.led.reg, triggerlevelkiteonly.reg, c3war.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_316417AA.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, uapsd.reg, Customer15b.led.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_662111AD.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func1_1.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_03051A32.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func1_1.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_03051A32w.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func1_1.reg, htAdhoc.reg, janusda.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_10891A3B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func1_1.reg, htWepTkipOpt.reg, htAdhoc.reg, wirelessmodeselectkite.reg, triggerlevelkiteonly.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_11211A3B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func2_8.reg, htWepTkipOpt.reg, htAdhoc.reg, wirelessmodeselectkite.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1A211A3B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5212.bgmp.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func2_8.reg, htWepTkipOpt.reg, htAdhoc.reg, wirelessmodeselectkite.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_20371A3B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func1_1.reg, htEnableWepTkip.reg, htAdhoc.reg, wirelessmodeselectkite.reg, triggerlevelkiteonly.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1A891A3B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5212.bgmp.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func1_1.reg, triggerlevelkiteonly.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3091SF.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, customer_Samsung.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg, scanasync.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_03011A32.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, cemspecled_func1_1.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_10671A3B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg,cemspecled_func1_1.reg, uapsd.reg, smpsDynamic.reg, htWepTkipOpt.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1A671A3B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5212.bgmp.reg, sys.TcpParams.reg,cemspecled_func1_1.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_10711A3B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgnxb.reg, sys.TcpParams.reg, cemspecled_func1_1.reg, uapsd.reg, smpsDynamic.reg, htEnableWepTkip.reg, htAdhoc.reg, d3forcel1disable.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1C711A3B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgnxb.reg, sys.TcpParams.reg, cemspecled_func1_1.reg, uapsd.reg, smpsDynamic.reg, htEnableWepTkip.reg, htAdhoc.reg, d3forcel1disable.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E006105B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParamslan.reg, customer3c.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg, serializing.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E01F105B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParamslan.reg, customer3c.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg, serializing.reg, d3forcel1disable1.reg, cmdRegister.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_664211AD.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParamslan.reg, customer3c.reg, uapsd.reg, smpsDynamic.reg, serializing.reg, d3forcel1disable1.reg, cmdRegister.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_663111AD.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParamslan.reg, customer3c.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg, serializing.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E016105B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParamslan.reg, customer3c.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg, serializing.reg, triggerlevelkiteonly.reg, c3war.reg, cmdRegister.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E035105B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParamslan.reg, customer3c.reg, uapsd.reg, smpsDynamic.reg, serializing.reg, cmdRegister.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E031105Bw.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParamslan.reg, customer3c.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg, serializing.reg, janusda.reg, triggerlevelkiteonly.reg, c3war.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_S001A.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_S001B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_S3067a.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, customer_Samsung.reg, rssiAdjust.reg, uapsd.reg, scanasync.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_S3067b.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, customer_Samsung.reg, rssiAdjust.reg, uapsd.reg, cmdRegister.reg, scanasync.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_10241A3B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, customer1a3b.reg, uapsd.reg, htEnableWepTkip.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_D05B10FC.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = customer_IODATA.reg, ATHER.reg, sys.TcpParams.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_05021A32.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_0013.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_001A.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_001B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1025.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2025.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1026.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2026.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1027.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2027.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1030.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2030.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1031.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2031.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1041.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2041.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1042.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2042.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1051.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2051.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1052.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2052.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_001C.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E023105B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E033105Bw.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E029105B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1029105B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_11121A3B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_6313.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1053.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2053.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1054.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2054.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1062.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2062.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_7111144F.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_04221468.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_04171468.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1063.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_F013.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_F013C.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_001D.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1055.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2055.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1013.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3013.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2013.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_4013.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_5013.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_6013.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_0036.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_0037.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_0023.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_90001385.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_0033168c.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_0032168c.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_13C010CF.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_147C10CF.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_147D10CF.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_153710CF.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_7125144F.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2A5F103C.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_11AD.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_03841014.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_04281468.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_01051A32.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_01121A32.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_042A1468.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E000105B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E002105B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_04061468.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_04071468.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_04231468.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E007105B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_S30A1.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_660311AD.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_03091A32.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_SS30A1.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2063.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_10261A3B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_01001A32.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_02001A32.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_N2062.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_N3072.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_N3073.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E801.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E811.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E814.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_0013.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E901.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E911.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E912.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E913.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E917.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E918.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E914.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E916.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1186.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3A691186.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3A6D1186.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3A6F1186.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3A701186.NDI.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3A7A1186.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3A7B1186.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_WNA2330.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_WNA1330.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3091.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3091amd.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_008F106B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_7136144F.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_T3091.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_309917AA.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1000168C.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1001168C.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3091PB.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_30A1.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_T30A1.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_30AA.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_30AB.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_BA91167D.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_7173144Fw.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_30A1a.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_30A1w.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_309D17AA.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_30A117AA.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_316417AA.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_662111AD.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_03051A32.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_03051A32w.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_10891A3B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_11211A3B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1A211A3B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_20371A3B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1A891A3B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3091SF.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_03011A32.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_10671A3B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1A671A3B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_10711A3B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1C711A3B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E006105B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E01F105B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_664211AD.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_663111AD.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E016105B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E035105B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E031105Bw.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_S001A.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_S001B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_S3067a.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_S3067b.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_10241A3B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_D05B10FC.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

;AMD 64
; Windows AMD64 specific entries

[ATHER_DEV_0013.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_001A.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_001B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1025.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2025.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1026.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgcb.reg, uapsd.reg, d3hot.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2026.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1027.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2027.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1030.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2030.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1031.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2031.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1041.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2041.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1051.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2051.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1042.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2042.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1052.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2052.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_001C.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E023105B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func1_1.reg, overrideAC.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E033105Bw.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func1_1.reg, overrideAC.reg, janusda.reg, triggerlevelkiteonly.reg, c3war.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E029105B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg, cemspecled_func1_1.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1029105B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg, cemspecled_func1_1.reg, overrideAC.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_11121A3B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg, cemspecled_func1_1.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_6313.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, cemspecled_func1_3.reg, d3hot.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1053.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2053.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1054.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2054.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1062.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2062.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_7111144F.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgmp.reg, Customer14.led.reg, uapsd.reg, expresscardaspmoff.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_04221468.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgmp.reg, customer3.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_04171468.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, customer3.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1063.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2063.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_F013.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgcb.reg, customer1ani.reg, bandselect.reg, uapsd.reg, customer1roam.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_F013C.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgcb.reg, customer1ani.reg, bandselect.reg, uapsd.reg, customer1roam.reg, minpower.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_001D.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1055.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg, gpioled.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2055.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1013.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, customer0.PS1.reg, customer0.LED.reg, customer0.5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3013.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, customer0.PS1.reg, customer0.LED1.reg, customer0.5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2013.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, customer0.PS1.reg, customer0.LED.reg, customer0.5213.abg.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_4013.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, customer0.PS1.reg, customer0.LED1.reg, customer0.5213.abg.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_5013.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, customer0.PS1.reg, customer0.LED2.reg, customer0.5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_6013.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, customer0.PS1.reg, customer0.LED2.reg, customer0.5212.bgmp.reg, d3hot.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_0036.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, sys.TcpParams.reg, customer0.PS1.reg, customer0.LED1.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_0037.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, sys.TcpParams.reg, customer0.PS1.reg, customer0.LED1_HB95.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_0023.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgncb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_90001385.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgncb.reg, sys.TcpParams.reg, uapsd.reg, expresscardaspmoff.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_05021A32.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgncb.reg, sys.TcpParams.reg, customer10.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_05021A32.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_0033168c.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgnxb.reg, sys.TcpParams.reg, customer0.reg, 5416.antennacontrols.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_0032168c.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, customer0.reg, 5416.antennacontrols.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_13C010CF.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgnxb.reg, sys.TcpParams.reg, 5416.antennacontrols.reg, uapsd.reg, customer1roam.reg, htAdhocdisable.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_147C10CF.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgnxb.reg, sys.TcpParams.reg, uapsd.reg, customer1roam.reg, htAdhocdisable.reg, smpsDynamic.reg, customer1fullreset.reg, merlinshiftdelay.reg, d3forcel1disable.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_147D10CF.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, customer1roam.reg, htAdhocdisable.reg, customer1fullreset.reg, merlinshiftdelay.reg, d3forcel1disable.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_153710CF.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, customer1roam.reg, htAdhocdisable.reg, customer1fullreset.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_7125144F.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgncb.reg, sys.TcpParams.reg, 5416.antennacontrols.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2A5F103C.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, customer2.11n.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_11AD.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, customer2.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_03841014.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgncb.reg, sys.TcpParams.reg, 5416.antennacontrols.reg, xb72.via.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_04281468.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgmp.reg, customer3e.reg, uapsd.reg, d3hot.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_01001A32.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, customer10.LED3.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_02001A32.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgmp.reg, customer10.LED3.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_01051A32.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgmp.reg, customer3a.reg, uapsd.reg, d3hot.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_01121A32.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgmp.reg, customer3a.reg, uapsd.reg, d3hot.reg, customer3d.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_042A1468.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, customer9.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E000105B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, customer4b.reg, customer4_basic.reg, customer4a_ASPM.reg, uapsd.reg, d3hot.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E002105B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, customer4b.reg, customer4_basic.reg, customer4a_ASPM.reg, uapsd.reg, d3hot.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_04061468.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, customer4a.reg,customer4_basic.reg, customer4a_ASPM.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_04071468.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, COMMON_AG.reg, customer4a.reg,customer4_basic.reg, customer4a_ASPM.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_04231468.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, customer4a.reg,customer4_basic.reg, customer4a_ASPM.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E007105B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, customer4a.reg, sys.TcpParams.reg, customer4c.reg, customer4adhoc.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_S30A1.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, customer4adhoc.reg, customer4a.reg, triggerlevelkiteonly.reg, c3war.reg, cmdRegister.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_SS30A1.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, customer4adhoc.reg, customer4as.reg, triggerlevelkiteonly.reg, c3war.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_10261A3B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, 10261a3b.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2052.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E801.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led0.reg, 5211.reg, ATHER.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E811.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led0.reg, 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E814.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led0.reg, 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_0013.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led0.reg, 5211.reg, ATHER.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E901.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led0.reg, 5211.reg, ATHER.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E911.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led0.reg, 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E912.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led0.reg, 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E913.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led1.reg, 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E917.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led1.reg, 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E918.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led2.reg, 5211.reg, ATHER.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E914.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, customer12Led0.reg, 5416.abgncb.reg, sys.TcpParams.reg, 5416.antennacontrols.reg, customer12.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E916.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, customer12Led1.reg, 5416.abgncb.reg, sys.TcpParams.reg, 5416.antennacontrols.reg, customer12.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_N2062.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer11.reg, customer11_legacywmode.reg, cemspecled_func1_1.reg, customer11Ant.reg, ATHER.reg, customer11ACStatus.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_N3072.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = customer11.reg, customer11_11nwmode.reg, cemspecled_func1_1.reg, ATHER.reg, sys.TcpParams.reg, customer11ACStatus.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_N3073.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = customer11.reg, customer11_11n40wmode.reg, cemspecled_func1_1.reg, ATHER.reg, sys.TcpParams.reg, customer11ACStatus.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1186.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, customer5.11nLED.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3A691186.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, customer5.11nLED.reg, pcibusconfig.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3A6D1186.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, customer5.11nLED.reg, pcibusconfig.reg, customer5.3x3.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3A6F1186.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, customer5.PCIe11nLed.reg, uapsd.reg, expresscardaspmoff.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3A701186.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, customer5.PCIe11nLed.reg, customer5.3x3.reg, uapsd.reg, expresscardaspmoff.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3A7A1186.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = ATHER.reg, 5416.reg, 5416.bgnxb.reg, sys.TcpParams.reg, customer5.11nLED.reg, pcibusconfig.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3A7B1186.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = ATHER.reg, 5416.reg, 5416.bgnxb.reg, sys.TcpParams.reg, customer5.11nLED.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_WNA2330.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, wnaled.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_WNA1330.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, wnaled.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3091.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3091amd.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg, cemspecled_func1_1.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_008F106B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg, wowenable.reg, merlinshiftdelay.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_7136144F.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg, merlinshiftdelay.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_T3091.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, uapsd.reg, smpsDynamic.reg, pcibusconfig.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_309917AA.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgnxb.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func1_1.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1000168C.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgnxb.reg, sys.TcpParams.reg, uapsd.reg, customer2merlin.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1001168C.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgnxb.reg, sys.TcpParams.reg, uapsd.reg, customer2.11n.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3091PB.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, pushbutton.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_30A1.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_T30A1.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_660311AD.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, customer3f.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_03091A32.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, cemspecled_func1_8.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_30AA.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, triggerlevelkiteonly.reg, Customer15a.led.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_30AB.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, janusda.reg, triggerlevelkiteonly.reg, Customer15a.led.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_BA91167D.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, janusda.reg, cemspecled_func1_1.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_7173144Fw.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, janusda.reg, triggerlevelkiteonly.reg, c3war.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_30A1a.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, customer_Samsung.reg, uapsd.reg, htAdhoc.reg, scanasync.reg, cmdRegister.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_30A1w.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, customer_Samsung.reg, uapsd.reg, htAdhoc.reg, janusda.reg, scanasync.reg, cmdRegister.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_309D17AA.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, Customer15a.led.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_30A117AA.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, uapsd.reg, htAdhoc.reg, Customer15a.led.reg, triggerlevelkiteonly.reg, c3war.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_316417AA.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, uapsd.reg, Customer15b.led.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_662111AD.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func1_1.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_03051A32.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func1_1.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_03051A32w.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func1_1.reg, htAdhoc.reg, janusda.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_10891A3B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func1_1.reg, htWepTkipOpt.reg, htAdhoc.reg, wirelessmodeselectkite.reg, triggerlevelkiteonly.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_11211A3B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func2_8.reg, htWepTkipOpt.reg, htAdhoc.reg, wirelessmodeselectkite.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1A211A3B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5212.bgmp.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func2_8.reg, htWepTkipOpt.reg, htAdhoc.reg, wirelessmodeselectkite.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_20371A3B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func1_1.reg, htEnableWepTkip.reg, htAdhoc.reg, wirelessmodeselectkite.reg, triggerlevelkiteonly.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1A891A3B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5212.bgmp.reg, sys.TcpParams.reg, uapsd.reg, cemspecled_func1_1.reg, triggerlevelkiteonly.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3091SF.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, customer_Samsung.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg, scanasync.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_S001A.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_S001B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_S3067a.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, customer_Samsung.reg, rssiAdjust.reg, uapsd.reg, scanasync.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_S3067b.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5212.bgmp.reg, customer_Samsung.reg, rssiAdjust.reg, uapsd.reg, cmdRegister.reg, scanasync.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_10241A3B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, customer1a3b.reg, uapsd.reg, htEnableWepTkip.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_03011A32.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, cemspecled_func1_1.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_10671A3B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.bgnxb.reg, sys.TcpParams.reg,cemspecled_func1_1.reg, uapsd.reg, htWepTkipOpt.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_10711A3B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgnxb.reg, sys.TcpParams.reg,cemspecled_func1_1.reg, uapsd.reg, htEnableWepTkip.reg, smpsDynamic.reg, htAdhoc.reg, d3forcel1disable.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1C711A3B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.abgnxb.reg, sys.TcpParams.reg, cemspecled_func1_1.reg, uapsd.reg, smpsDynamic.reg, htEnableWepTkip.reg, htAdhoc.reg, d3forcel1disable.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E006105B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, customer3c.reg, uapsd.reg, uapsd.reg, htAdhoc.reg, smpsDynamic.reg, serializing.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E01F105B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, customer3c.reg, uapsd.reg, uapsd.reg, htAdhoc.reg, smpsDynamic.reg, serializing.reg, d3forcel1disable1.reg, cmdRegister.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_664211AD.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, customer3c.reg, uapsd.reg, smpsDynamic.reg, serializing.reg, d3forcel1disable1.reg, cmdRegister.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_663111AD.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParams.reg, customer3c.reg, uapsd.reg, uapsd.reg, htAdhoc.reg, smpsDynamic.reg, serializing.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E016105B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParamslan.reg, customer3c.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg, serializing.reg, triggerlevelkiteonly.reg, c3war.reg, cmdRegister.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E035105B.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParamslan.reg, customer3c.reg, uapsd.reg, smpsDynamic.reg, serializing.reg, cmdRegister.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E031105Bw.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, sys.TcpParamslan.reg, customer3c.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg, serializing.reg, janusda.reg, triggerlevelkiteonly.reg, c3war.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_D05B10FC.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = customer_IODATA.reg, ATHER.reg, sys.TcpParams.reg, uapsd.reg, smpsDynamic.reg, htAdhoc.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_0013.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_001A.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_001B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1025.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2025.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1026.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2026.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1027.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2027.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1030.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2030.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1031.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2031.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1041.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2041.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1042.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2042.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1051.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2051.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1052.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2052.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_001C.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E023105B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E033105Bw.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E029105B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1029105B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_11121A3B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_6313.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1053.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2053.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1054.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2054.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1062.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2062.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_04221468.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_7111144F.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_04171468.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1063.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2063.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_F013.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_F013C.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_001D.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1055.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2055.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1013.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3013.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2013.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_4013.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_5013.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_6013.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_0036.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_0037.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_0023.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_90001385.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog


[ATHER_DEV_0033168c.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_0032168c.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_13C010CF.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_147C10CF.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_147D10CF.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_153710CF.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_7125144F.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2A5F103C.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_11AD.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_03841014.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_04281468.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_01051A32.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_01121A32.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_042A1468.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E000105B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E002105B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_04061468.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_04071468.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_04231468.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E007105B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_S30A1.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_SS30A1.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_10261A3B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_01001A32.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_02001A32.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E801.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E811.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E814.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_0013.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E901.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E911.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E912.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E913.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E917.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E918.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E914.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E916.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_N2062.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_N3072.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_N3073.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1186.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3A691186.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3A6D1186.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3A6F1186.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3A701186.NDI.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3A7A1186.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3A7B1186.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_WNA2330.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_WNA1330.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3091.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3091amd.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_008F106B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_7136144F.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_T3091.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog
  
[ATHER_DEV_309917AA.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1000168C.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1001168C.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3091PB.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_30A1.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_T30A1.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_660311AD.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_03091A32.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_309D17AA.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_30A117AA.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_316417AA.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_30AA.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_30AB.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_BA91167D.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_7173144Fw.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_30A1a.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_30A1w.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_662111AD.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_03051A32.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_03051A32w.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_10891A3B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_11211A3B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1A211A3B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_20371A3B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1A891A3B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3091SF.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_S001A.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_S001B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_S3067a.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_S3067b.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_10241A3B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_03011A32.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_10671A3B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_10711A3B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1C711A3B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E006105B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E01F105B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_664211AD.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_663111AD.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E016105B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E035105B.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E031105Bw.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_D05B10FC.ndi.NTamd64.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

;End of AMD 64
;
; 5211 Enumerated Types
;

[5212.abgcb.reg]
HKR, ,                                  NetBand,                        0x00002,  "1823"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1
HKR, ,					pciCacheLineSize,		0x00002,  1

[5212.abgmp.reg]
HKR, ,                                  NetBand,                        0x00002,  "1823"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  2
HKR, ,					pciCacheLineSize,		0x00002,  1

[5212.bgcb.reg]
HKR, ,                                  NetBand,                        0x00002,  "28"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1
HKR, ,					pciCacheLineSize,		0x00002,  1

[5212.bgmp.reg]
HKR, ,                                  NetBand,                        0x00002,  "28"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  2
HKR, ,					pciCacheLineSize,		0x00002,  1

[5416.abgncb.reg]
HKR, ,                                  NetBand,                        0x00002,  "61455"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1
HKR, ,                                  rmEnable,                       0x00002,  "1"
HKR, ,                                  abolt,                          0x00002,  "0"
HKR, ,                                  rateCtrlEnable,                 0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"
HKR, ,					pciCacheLineSize,		0x00002,  1

[5416.bgnxb.reg]
HKR, ,                                  NetBand,                        0x00002,  "40972"
HKR, ,                                  wModeSelect,                    0x00002,  "40972"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1
HKR, ,                                  abolt,                          0x00002,  "0"
HKR, ,                                  rateCtrlEnable,                 0x00002,  "1"
HKR, ,                                  rmEnable,                       0x00002,  "1"
HKR, ,					pciCacheLineSize,		0x00002,  1

[5416.abgnxb.reg]
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1
HKR, ,                                  abolt,                          0x00002,  "0"
HKR, ,                                  rateCtrlEnable,                 0x00002,  "1"
HKR, ,                                  rmEnable,                       0x00002,  "1"
HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "61455"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "61455",                        0,  %WirelessModeAuto%
HKR, Ndi\params\NetBand\enum,           "20481",                        0,  %WirelessMode5GHzOnly%
HKR, Ndi\params\NetBand\enum,           "40972",                        0,  %WirelessMode2GHzOnly%
HKR, ,					pciCacheLineSize,		0x00002,  1

[5416.antennacontrols.reg] 
HKR, ,                                  rxChainSelect,                 	0x00002,  "7"
;HKR, ,                                  txChainSelectLegacy,            0x00002,  "5"
HKR, ,                                  rxChainSelectLegacy,           	0x00002,  "7"
HKR, ,                                  forceBias,           	        0x00002,  "2"
HKR, ,                                  rxChainDetect,                  0x00002,  "1"
HKR, ,                                  rxChainDetectRef,               0x00002,  "0"
HKR, ,                                  rxChainDetectThreshA,           0x00002,  "0"
HKR, ,                                  rxChainDetectThreshG,           0x00002,  "0"
HKR, ,                                  rxChainDetectDeltaA,            0x00002,  "20"
HKR, ,                                  rxChainDetectDeltaG,            0x00002,  "20"

[pushbutton.reg]
HKR, ,                                  wpsButtonGpio,                  0x00002,  "9"

[smpsDynamic.reg]
HKR, Ndi\params\smpsDynamic,            ParamDesc,                      0,        %smpsDynamic%
HKR, Ndi\params\smpsDynamic,            Base,                           0,        "10"
HKR, Ndi\params\smpsDynamic,            default,                        0,        "0"
HKR, Ndi\params\smpsDynamic,            type,                           0,        "enum"
HKR, Ndi\params\smpsDynamic\enum,       "1",                            0,        %smpsDynamicEnable%
HKR, Ndi\params\smpsDynamic\enum,       "0",                            0,        %smpsDynamicDisable% 

[bandselect.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,        %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,        "10"
HKR, Ndi\params\NetBand,                default,                        0,        "1823"
HKR, Ndi\params\NetBand,                type,                           0,        "enum"
HKR, Ndi\params\NetBand\enum,           "1823",                         0,        %WirelessModeAuto%
HKR, Ndi\params\NetBand\enum,           "1795",                         0,        %WirelessMode5GHzOnly%
HKR, Ndi\params\NetBand\enum,           "28",                           0,        %WirelessMode2GHzOnly%

[wirelessmodeselectkite.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "40972"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "40972",                        0,  %WirelessModeAuto%
HKR, Ndi\params\NetBand\enum,           "12",                           0,  %WirelessMode11bgOnly%

[pcibusconfig.reg]
HKR, ,                                  serializeRegMode,               0x00002,  "2"
HKR, ,                                  BusConfig,                 	0x00002,  "0"

[serializing.reg]
HKR, ,                                  serializeRegMode,               0x00002,  "1"

[d3hot.reg]
HKR, ,                                  pciePowerReset,                 0x00002,  "0"
HKR, ,                                  pcieRestore,                 	0x00002,  "1"

[expresscardaspmoff.reg]
HKR, ,                                  pciDetectEnable,                0x00002,  "2"
HKR, ,                                  pciePowerSaveEnable,            0x00002,  "1"
HKR, ,                                  pcieAspm,                       0x00002,  "0"

[gpioled.reg]
HKR,,                                   linkLEDFunc,                    0,        "49"
HKR,,                                   activityLEDFunc,                0,        "51"
HKR,,                                   connectionLEDFunc,              0,        "55"

[scanasync.reg]
HKR, ,                                  scanAsc,                        0x00002,  "1"

; Allow non admin uses to switch profiles
;[5211.reg.security]
;"D:ARAI(A;;GA;;;BA)(A;;GA;;;SY)(A;CI;GA;;;IU)"

;-----------------------------------------------------------------------------
;
; 5211 common
;
[5211.DelReg]
HKR,,NetBand
HKR,,ssid
HKR,,ssid2
HKR,,ssid3
HKR,,prefBssid1
HKR,,prefBssid2
HKR,,prefBssid3
HKR,,prefBssid4
HKR,Ndi\Params\tpc
HKR,,tpc
HKR,Ndi\Params\authTypeUseOnly
HKR,,authTypeUseOnly
HKR,,AdHocBand
HKR,,AwakeTimePerf
HKR,,beaconInterval
HKR,,bkScanEnable
HKR,,bssType
HKR,,ccode
HKR,,clist
HKR,,defaultKey
HKR,,EncryptionAlg
HKR,,FragThreshold
HKR,,HwTxRetries
HKR,,privacyInvoked
HKR,,QoS
HKR,,rateCtrlEnable
HKR,,RTSThreshold
HKR,,scanType
HKR,,SwTxRetryScale
HKR,,SmeEnable
HKR,,aifs
HKR,,cwmin
HKR,,pcieClockReq
HKR,,overrideACstatus
HKR,Ndi\params\sleepMode
HKR,Ndi\params\sleepMode\enum
HKR, Ndi\params\ExtendedChannel
HKR, NDI\params\Mode11dSwitch
HKR, Ndi\params\MapRegisters
HKR, CustomParams\Configurations\Cfg0
HKR, Ndi\params\NetBand
HKR,,pciePowerSaveEnable
HKR,,pcieAspm
HKR, Ndi\params\smpsDynamic
HKR,,d3forcel1disable.reg
HKR,,d3forcel1disablekite.reg
HKR,,d3forcel1disablekite1.reg
HKR,,pcieWaen
HKR,,halPcieDetach
HKR,,PcieDetach

[5211.reg]
HKR, Ndi\params\MapRegisters,           ParamDesc,                      0,  %MapRegisters%
HKR, Ndi\params\MapRegisters,           default,                        0,  "256"
HKR, Ndi\params\MapRegisters,           min,                            0,  "32"
HKR, Ndi\params\MapRegisters,           max,                            0,  "512"
HKR, Ndi\params\MapRegisters,           step,                           0,  "8"
HKR, Ndi\params\MapRegisters,           base,                           0,  "10"
HKR, Ndi\params\MapRegisters,           type,                           0,  "int"

HKR, Ndi\params\NetworkAddress,         ParamDesc,                      0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,         default,                        0,  ""
HKR, Ndi\params\NetworkAddress,         LimitText,                      0,  "12"
HKR, Ndi\params\NetworkAddress,         UpperCase,                      0,  "1"
HKR, Ndi\params\NetworkAddress,         optional,                       0,  "1"
HKR, Ndi\params\NetworkAddress,         type,                           0,  "edit"

HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "2"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  "1"
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%

HKR, Ndi\params\radioEnable,            ParamDesc,                      0,  %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,  "10"
HKR, Ndi\params\radioEnable,            default,                        0,  "1"
HKR, Ndi\params\radioEnable,            type,                           0,  "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,  %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,  %radioEnableOff%

HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"

HKR, Ndi\params\ccx5FeatureEnable,      ParamDesc,                      0,  %ccx5FeatureEnable%
HKR, Ndi\params\ccx5FeatureEnable,      Base,                           0,  "10"
HKR, Ndi\params\ccx5FeatureEnable,      default,                        0,  "0"
HKR, Ndi\params\ccx5FeatureEnable,      type,                           0,  "enum"
HKR, Ndi\params\ccx5FeatureEnable\enum, "1",                            0,  %ccx5FeatureEnableMfpEnable%
HKR, Ndi\params\ccx5FeatureEnable\enum, "0",                            0,  %ccx5FeatureEnableMfpDisable%

HKR, CustomParams\Configurations,       MajorVersion,                   0x10003,  2
HKR, CustomParams\Configurations,       MinorVersion,                   0x10003,  0

HKR, CustomParams\Configurations,       SelectedConfigurationIndex,     0x10003,  0
HKR, CustomParams\Configurations,       SelectedConfigurationName,      0x00002,  "Default"

[uapsd.reg]
HKR, Ndi\params\uapsdEnabledBE,            ParamDesc,                      0,  %uapsdEnabledBE%
HKR, Ndi\params\uapsdEnabledBE,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledBE,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledBE,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledBE\enum,       "1",                            0,  %uapsdEnabledBEOn%
HKR, Ndi\params\uapsdEnabledBE\enum,       "0",                            0,  %uapsdEnabledBEOff%

HKR, Ndi\params\uapsdEnabledBK,            ParamDesc,                      0,  %uapsdEnabledBK%
HKR, Ndi\params\uapsdEnabledBK,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledBK,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledBK,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledBK\enum,       "1",                            0,  %uapsdEnabledBKOn%
HKR, Ndi\params\uapsdEnabledBK\enum,       "0",                            0,  %uapsdEnabledBKOff%

HKR, Ndi\params\uapsdEnabledVI,            ParamDesc,                      0,  %uapsdEnabledVI%
HKR, Ndi\params\uapsdEnabledVI,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledVI,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledVI,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledVI\enum,       "1",                            0,  %uapsdEnabledVIOn%
HKR, Ndi\params\uapsdEnabledVI\enum,       "0",                            0,  %uapsdEnabledVIOff%

HKR, Ndi\params\uapsdEnabledVO,            ParamDesc,                      0,  %uapsdEnabledVO%
HKR, Ndi\params\uapsdEnabledVO,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledVO,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledVO,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledVO\enum,       "1",                            0,  %uapsdEnabledVOOn%
HKR, Ndi\params\uapsdEnabledVO\enum,       "0",                            0,  %uapsdEnabledVOOff%

HKR, Ndi\params\psPollEnable,            ParamDesc,                      0,  %psPoll%
HKR, Ndi\params\psPollEnable,            Base,                           0,  "10"
HKR, Ndi\params\psPollEnable,            default,                        0,  "0"
HKR, Ndi\params\psPollEnable,            type,                           0,  "enum"
HKR, Ndi\params\psPollEnable\enum,       "1",                            0,  %psPollEnable%
HKR, Ndi\params\psPollEnable\enum,       "0",                            0,  %psPollDisable%

;-----------------------------------------------------------------------------
;
; 5416 common
;
[5416.DelReg]
HKR,,NetBand
HKR,,ssid
HKR,,ssid2
HKR,,ssid3
HKR,,prefBssid1
HKR,,prefBssid2
HKR,,prefBssid3
HKR,,prefBssid4
HKR,Ndi\Params\tpc
HKR,,tpc
HKR,Ndi\Params\authTypeUseOnly
HKR,,authTypeUseOnly
HKR,,AdHocBand
HKR,,AwakeTimePerf
HKR,,beaconInterval
HKR,,bkScanEnable
HKR,,bssType
HKR,,ccode
HKR,,clist
HKR,,defaultKey
HKR,,EncryptionAlg
HKR,,FragThreshold
HKR,,HwTxRetries
HKR,,privacyInvoked
HKR,,QoS
HKR,,rateCtrlEnable
HKR,,RTSThreshold
HKR,,scanType
HKR,,SwTxRetryScale
HKR,,SmeEnable
HKR,,aifs
HKR,,cwmin
HKR,,pcieClockReq
HKR,,rmEnable
HKR,,overrideACstatus
HKR, Ndi\params\NetBand
HKR,,rxChainSelect
HKR,,txChainSelectLegacy
HKR,,rxChainSelectLegacy
HKR,,rxChainDetect
HKR,,rxChainDetectRef
HKR,,rxChainDetectThreshA
HKR,,rxChainDetectThreshG
HKR,,rxChainDetectDeltaA
HKR,,rxChainDetectDeltaG
HKR,,pciePowerSaveEnable
HKR,,pcieAspm
HKR, Ndi\params\smpsDynamic
HKR,,d3forcel1disable.reg
HKR,,d3forcel1disablekite.reg
HKR,,d3forcel1disablekite1.reg
HKR,,pcieWaen
HKR,,halPcieDetach
HKR,,PcieDetach

[5416.reg]
HKR, Ndi\params\MapRegisters,           ParamDesc,                      0,  %MapRegisters%
HKR, Ndi\params\MapRegisters,           default,                        0,  "256"
HKR, Ndi\params\MapRegisters,           min,                            0,  "32"
HKR, Ndi\params\MapRegisters,           max,                            0,  "512"
HKR, Ndi\params\MapRegisters,           step,                           0,  "8"
HKR, Ndi\params\MapRegisters,           base,                           0,  "10"
HKR, Ndi\params\MapRegisters,           type,                           0,  "int"

HKR, Ndi\params\NetworkAddress,         ParamDesc,                      0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,         default,                        0,  ""
HKR, Ndi\params\NetworkAddress,         LimitText,                      0,  "12"
HKR, Ndi\params\NetworkAddress,         UpperCase,                      0,  "1"
HKR, Ndi\params\NetworkAddress,         optional,                       0,  "1"
HKR, Ndi\params\NetworkAddress,         type,                           0,  "edit"

HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "2"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  "1"
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%

HKR, Ndi\params\radioEnable,            ParamDesc,                      0,  %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,  "10"
HKR, Ndi\params\radioEnable,            default,                        0,  "1"
HKR, Ndi\params\radioEnable,            type,                           0,  "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,  %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,  %radioEnableOff%

HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"

HKR, Ndi\params\ccx5FeatureEnable,      ParamDesc,                      0,  %ccx5FeatureEnable%
HKR, Ndi\params\ccx5FeatureEnable,      Base,                           0,  "10"
HKR, Ndi\params\ccx5FeatureEnable,      default,                        0,  "0"
HKR, Ndi\params\ccx5FeatureEnable,      type,                           0,  "enum"
HKR, Ndi\params\ccx5FeatureEnable\enum, "1",                            0,  %ccx5FeatureEnableMfpEnable%
HKR, Ndi\params\ccx5FeatureEnable\enum, "0",                            0,  %ccx5FeatureEnableMfpDisable%

HKR, CustomParams\Configurations,       MajorVersion,                   0x10003,  2
HKR, CustomParams\Configurations,       MinorVersion,                   0x10003,  0

HKR, CustomParams\Configurations,       SelectedConfigurationIndex,     0x10003,  0
HKR, CustomParams\Configurations,       SelectedConfigurationName,      0x00002,  "Default"

;-----------------------------------------------------------------------------
;;Customized Section

[customer0.reg]
;PCIe Related
HKR, ,                                  pcieAspm,                 	0x00002,  "2"
HKR, ,                                  pciePowerSaveEnable,            0x00002,  "1"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  forceWake,                 	0x00002,  "0"
HKR, ,                                  antennaSwitchSwap,              0x00002,  "1"
;LED Related
HKR, ,                                  gpioPinFunc1,                  0x00002,  "1"
;General Customer0
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR,NDI\params\ignore11dBeacon,ParamDesc,,	%Mode11d%
HKR,NDI\params\ignore11dBeacon,type,,		"enum"
HKR,NDI\params\ignore11dBeacon,Default,,	"1"
HKR,NDI\params\ignore11dBeacon\enum,0,,		%Mode11dEnable%
HKR,NDI\params\ignore11dBeacon\enum,1,,		%Mode11dDisable%

HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,  %roamRssiA%
HKR, Ndi\params\roamRssiA,              default,                        0,  "15"
HKR, Ndi\params\roamRssiA,              min,                            0,  "1"
HKR, Ndi\params\roamRssiA,              max,                            0,  "95"
HKR, Ndi\params\roamRssiA,           	step,                           0,  "1"
HKR, Ndi\params\roamRssiA,           	base,                           0,  "10"
HKR, Ndi\params\roamRssiA,           	type,                           0,  "int"

HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "1"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"

[customer0.5212.bgmp.reg]
HKR, ,                                  NetBand,                        0x00002,  "1823"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  2

HKR,NDI\params\TransmitRate11g,ParamDesc,,	%TxRate11g%
HKR,NDI\params\TransmitRate11g,type,,		"enum"
HKR,NDI\params\TransmitRate11g,Default,,	"11"

HKR,NDI\params\TransmitRate11g\enum,0,,		%TxRate11g1M%
HKR,NDI\params\TransmitRate11g\enum,1,,		%TxRate11g2M%
HKR,NDI\params\TransmitRate11g\enum,2,,		%TxRate11g5M%
HKR,NDI\params\TransmitRate11g\enum,3,,		%TxRate11g11M%
HKR,NDI\params\TransmitRate11g\enum,4,,		%TxRate11g6M%
HKR,NDI\params\TransmitRate11g\enum,5,,		%TxRate11g9M%
HKR,NDI\params\TransmitRate11g\enum,6,,		%TxRate11g12M%
HKR,NDI\params\TransmitRate11g\enum,7,,		%TxRate11g18M%
HKR,NDI\params\TransmitRate11g\enum,8,,		%TxRate11g24M%
HKR,NDI\params\TransmitRate11g\enum,9,,		%TxRate11g36M%
HKR,NDI\params\TransmitRate11g\enum,10,,	%TxRate11g48M%
HKR,NDI\params\TransmitRate11g\enum,11,,	%TxRate11g54M%

[customer0.5213.abg.reg]
HKR, ,                                  NetBand,                        0x00002,  "1823"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1

HKR,NDI\params\TransmitRate11g,ParamDesc,,	%TxRate11g%
HKR,NDI\params\TransmitRate11g,type,,		"enum"
HKR,NDI\params\TransmitRate11g,Default,,	"11"

HKR,NDI\params\TransmitRate11g\enum,0,,		%TxRate11g1M%
HKR,NDI\params\TransmitRate11g\enum,1,,		%TxRate11g2M%
HKR,NDI\params\TransmitRate11g\enum,2,,		%TxRate11g5M%
HKR,NDI\params\TransmitRate11g\enum,3,,		%TxRate11g11M%
HKR,NDI\params\TransmitRate11g\enum,4,,		%TxRate11g6M%
HKR,NDI\params\TransmitRate11g\enum,5,,		%TxRate11g9M%
HKR,NDI\params\TransmitRate11g\enum,6,,		%TxRate11g12M%
HKR,NDI\params\TransmitRate11g\enum,7,,		%TxRate11g18M%
HKR,NDI\params\TransmitRate11g\enum,8,,		%TxRate11g24M%
HKR,NDI\params\TransmitRate11g\enum,9,,		%TxRate11g36M%
HKR,NDI\params\TransmitRate11g\enum,10,,	%TxRate11g48M%
HKR,NDI\params\TransmitRate11g\enum,11,,	%TxRate11g54M%

HKR,NDI\params\TransmitRate11a,ParamDesc,,	%TxRate11a%
HKR,NDI\params\TransmitRate11a,type,,		"enum"
HKR,NDI\params\TransmitRate11a,Default,,	"7"

HKR,NDI\params\TransmitRate11a\enum,0,,		%TxRate11a6M%
HKR,NDI\params\TransmitRate11a\enum,1,,		%TxRate11a9M%
HKR,NDI\params\TransmitRate11a\enum,2,,		%TxRate11a12M%
HKR,NDI\params\TransmitRate11a\enum,3,,		%TxRate11a18M%
HKR,NDI\params\TransmitRate11a\enum,4,,		%TxRate11a24M%
HKR,NDI\params\TransmitRate11a\enum,5,,		%TxRate11a36M%
HKR,NDI\params\TransmitRate11a\enum,6,,		%TxRate11a48M%
HKR,NDI\params\TransmitRate11a\enum,7,,		%TxRate11a54M%

HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "1823"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "1823",                         0,  %WirelessModeAuto%
HKR, Ndi\params\NetBand\enum,           "1795",                         0,  %WirelessMode5GHzOnly%
HKR, Ndi\params\NetBand\enum,           "28",                           0,  %WirelessMode2GHzOnly%

[customer0.5211.reg]
HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTimeValidcust%
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          default,                        0,  "45000"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "enum"
HKR, Ndi\params\scanTimeValid\enum,     "120000",                       0,  %scanTimeValidcust120%
HKR, Ndi\params\scanTimeValid\enum,     "60000",                        0,  %scanTimeValidcust60%
HKR, Ndi\params\scanTimeValid\enum,     "45000",                        0,  %scanTimeValidcust45%
HKR, Ndi\params\scanTimeValid\enum,     "30000",                        0,  %scanTimeValidcust30%
HKR, Ndi\params\scanTimeValid\enum,     "20000",                        0,  %scanTimeValidcust20%
HKR, Ndi\params\scanTimeValid\enum,     "10000",                        0,  %scanTimeValidcust10%
HKR, Ndi\params\scanTimeValid\enum,     "5000",                         0,  %scanTimeValidcust5%

HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,  %roamRssiA%
HKR, Ndi\params\roamRssiA,              default,                        0,  "15"
HKR, Ndi\params\roamRssiA,              min,                            0,  "1"
HKR, Ndi\params\roamRssiA,              max,                            0,  "95"
HKR, Ndi\params\roamRssiA,           	step,                           0,  "1"
HKR, Ndi\params\roamRssiA,           	base,                           0,  "10"
HKR, Ndi\params\roamRssiA,           	type,                           0,  "int"

HKR, Ndi\params\NetworkAddress,         ParamDesc,                      0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,         default,                        0,  ""
HKR, Ndi\params\NetworkAddress,         LimitText,                      0,  "12"
HKR, Ndi\params\NetworkAddress,         UpperCase,                      0,  "1"
HKR, Ndi\params\NetworkAddress,         optional,                       0,  "1"
HKR, Ndi\params\NetworkAddress,         type,                           0,  "edit"

HKR, Ndi\params\tpc,                    ParamDesc,                      0,  %tpc%
HKR, Ndi\params\tpc,                    Base,                           0,  "10"
HKR, Ndi\params\tpc,                    default,                        0,  "0"
HKR, Ndi\params\tpc,                    type,                           0,  "enum"
HKR, Ndi\params\tpc\enum,               "0",                            0,  %tpc100%
HKR, Ndi\params\tpc\enum,               "1",                            0,  %tpc50%
HKR, Ndi\params\tpc\enum,               "2",                            0,  %tpc25%
HKR, Ndi\params\tpc\enum,               "3",                            0,  %tpc12%
HKR, Ndi\params\tpc\enum,               "4",                            0,  %tpcLowest%

HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  "1"
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%

;Following Entry made to Enable/Disable rate Auto Rate control.
HKR,NDI\params\rateCtrlEnable,ParamDesc,,	%RateCtrl%
HKR,NDI\params\rateCtrlEnable,type,,		"enum"
HKR,NDI\params\rateCtrlEnable,Default,,		"1"
HKR,NDI\params\rateCtrlEnable\enum,0,,		%RateCtrlDisable%
HKR,NDI\params\rateCtrlEnable\enum,1,,		%RateCtrlEnable%

;Following Entry made to 11d mode switch 
HKR,NDI\params\ignore11dBeacon,ParamDesc,,	%Mode11d%
HKR,NDI\params\ignore11dBeacon,type,,		"enum"
HKR,NDI\params\ignore11dBeacon,Default,,	"1"
HKR,NDI\params\ignore11dBeacon\enum,0,,		%Mode11dEnable%
HKR,NDI\params\ignore11dBeacon\enum,1,,		%Mode11dDisable%

HKR,NDI\params\TransmitRate11b,ParamDesc,,	%TxRate11b%
HKR,NDI\params\TransmitRate11b,type,,		"enum"
HKR,NDI\params\TransmitRate11b,Default,,	"3"

HKR,NDI\params\TransmitRate11b\enum,0,,		%TxRate11b1M%
HKR,NDI\params\TransmitRate11b\enum,1,,		%TxRate11b2M%
HKR,NDI\params\TransmitRate11b\enum,2,,		%TxRate11b5M%
HKR,NDI\params\TransmitRate11b\enum,3,,		%TxRate11b11M%

HKR, Ndi\params\radioEnable,            ParamDesc,                      0,  %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,  "10"
HKR, Ndi\params\radioEnable,            default,                        0,  "1"
HKR, Ndi\params\radioEnable,            type,                           0,  "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,  %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,  %radioEnableOff%

HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR, ,					scanTimePreSleep,               0x00002,  "60" 
HKR, ,					capLinkSp,               	0x00002,  "1" 
HKR, ,                                  abolt,                          0x00002,  "191"

HKR, CustomParams\Configurations,       MajorVersion,                   0x10003,  2
HKR, CustomParams\Configurations,       MinorVersion,                   0x10003,  0

HKR, CustomParams\Configurations,       SelectedConfigurationIndex,     0x10003,  0
HKR, CustomParams\Configurations,       SelectedConfigurationName,      0x00002,  "Default"

[customer0.PS1.reg]
;HKR, CustomParams\Configurations\Cfg0,  PowerManagement,                0x10003,  1 ;Set power Mgmt mode to Max.
HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "1"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

;[customer0.PS2.reg]
;HKR, CustomParams\Configurations\Cfg0,  PowerManagement,                0x10003,  2 ;Set power Mgmt mode to Normal.
;HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
;HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
;HKR, Ndi\params\sleepMode,              default,                        0,  "1"
;HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
;HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
;HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
;HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

[customer0.LED.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "0"

[customer0.LED1.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  pcieClockReq,                   0x00002,  "0"
HKR, ,                                  pciePowerSaveEnable,            0x00002,  "1"
HKR, ,                                  pcieAspm,                       0x00002,  "2"

[customer0.LED1_HB95.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  overrideACstatus,               0x00002,  "1"

[customer0.LED2.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  pcieClockReq,                   0x00002,  "0"
HKR, ,                                  pciePowerSaveEnable,            0x00002,  "1"
HKR, ,                                  pcieAspm,                       0x00002,  "2"

[wnaled.reg]
HKR, ,                                  softLEDEnable,                  0x00002,  "1"
HKR, ,                                  swapDefaultLED,                 0x00002,  "1"

[customer1ani.reg]
HKR, Ndi\params\rssiThrHigh,            ParamDesc,                      0,        %rssiThrHigh%
HKR, Ndi\params\rssiThrHigh,            Base,                           0,        "10"
HKR, Ndi\params\rssiThrHigh,            default,                        0,        "40"
HKR, Ndi\params\rssiThrHigh,            type,                           0,        "enum"
HKR, Ndi\params\rssiThrHigh\enum,       "40",                           0,        %rssiThrHighNormal%
HKR, Ndi\params\rssiThrHigh\enum,       "32",                           0,        %rssiThrHighMin%

[customer1roam.reg]
HKR, Ndi\params\roamPolicy,             ParamDesc,                      0,        %roamPolicy%
HKR, Ndi\params\roamPolicy,             Base,                           0,        "10"
HKR, Ndi\params\roamPolicy,             default,                        0,        "3"
HKR, Ndi\params\roamPolicy,             type,                           0,        "enum"
HKR, Ndi\params\roamPolicy\enum,        "1",                            0,        %roamPolicyVeryLow%
HKR, Ndi\params\roamPolicy\enum,        "2",                            0,        %roamPolicyLow%
HKR, Ndi\params\roamPolicy\enum,        "3",                            0,        %roamPolicyNormal%
HKR, Ndi\params\roamPolicy\enum,        "4",                            0,        %roamPolicyHigh%
HKR, Ndi\params\roamPolicy\enum,        "5",                            0,        %roamPolicyVeryHigh%

[customer1fullreset.reg]
HKR, Ndi\params\halFullResetWarEnable,  ParamDesc,                      0,        %FullReset%
HKR, Ndi\params\halFullResetWarEnable,  Base,                           0,        "10"
HKR, Ndi\params\halFullResetWarEnable,  default,                        0,        "1"
HKR, Ndi\params\halFullResetWarEnable,  type,                           0,        "enum"
HKR, Ndi\params\halFullResetWarEnable\enum,   "1",                      0,        %Enable%
HKR, Ndi\params\halFullResetWarEnable\enum,   "0",                      0,        %Disable%

[customer2.reg]
HKR,,                                   linkLEDFunc,                    0,        "53"
HKR,,                                   activityLEDFunc,                0,        "51"
HKR,,                                   connectionLEDFunc,              0,        "55"

[customer2.11n.reg]
HKR, ,					gpioPinFunc0,        		0x00002,  "1"

[customer2merlin.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "1"

[customer3.reg]
HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "1"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%
HKR, ,                                  scanTimePreSleep,		0x00002,  "60"
HKR, ,                                  SleepTimePerf,			0x00002,  "500"
HKR, ,                                  LinkLEDFunc,			0x00002,  "19"
HKR, ,                                  ActivityLEDFunc,		0x00002,  "21"

[customer3a.reg]
HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "1"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  pcieClockReq,                   0x00002,  "0"
HKR, ,                                  abolt,                          0x00002,  "0"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "0"

[customer3c.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[customer3d.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "0"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "0"

[customer3e.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[customer3f.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "8"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[customer1a3b.reg]
HKR, ,                                  NetBand,                        0x00002,  "61455"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1
HKR, ,                                  rmEnable,                       0x00002,  "1"
HKR, ,                                  abolt,                          0x00002,  "0"
HKR, ,                                  rateCtrlEnable,                 0x00002,  "1"
HKR, ,                          	gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[customer4a.reg]
HKR, ,					gpioPinFunc0,        		0x00002,  "1"
HKR, ,					gpioFunc0ActHi,      		0x00002,  "0"
HKR, ,					PcieClockReq,     		0x00002,  "0"

[customer4as.reg]
HKR, ,					gpioPinFunc0,        		0x00002,  "8"
HKR, ,					gpioFunc0ActHi,      		0x00002,  "0"
HKR, ,					PcieClockReq,     		0x00002,  "0"

[customer4adhoc.reg]
HKR, ,					adhocChannel,        	        0x00002,  "2462"

[customer4b.reg]
HKR, ,					gpioPinFunc0,        		0x00002,  "3"
HKR, ,					gpioFunc0ActHi,      		0x00002,  "0"
HKR, ,					PcieClockReq,     		0x00002,  "0"

[customer4_basic.reg]
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"
HKR, ,                                  abolt,                          0x00002,  "0"
HKR, ,                                  sleepMode,                      0x00002, %sleepMode_DEFAULT%
HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  %sleepMode_DEFAULT%
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%
HKR, ,                                  shortPreamble,                  0x00002, %shortPreamble_DEFAULT%
HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  %shortPreamble_DEFAULT%
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%
HKR, Ndi\params\authTypeUseOnly,        ParamDesc,                      0,  %authTypeUseOnly%
HKR, Ndi\params\authTypeUseOnly,        Base,                           0,  "10"
HKR, Ndi\params\authTypeUseOnly,        default,                        0,  "0"
HKR, Ndi\params\authTypeUseOnly,        type,                           0,  "enum"
HKR, Ndi\params\authTypeUseOnly\enum,   "0",                            0,  %authAuto%
HKR, Ndi\params\authTypeUseOnly\enum,   "1",                            0,  %authOpen%
HKR, Ndi\params\authTypeUseOnly\enum,   "2",                            0,  %authShared%
HKR, ,                                  beaconInterval,                 0x00002,  "100"
HKR, ,                                  bkScanEnable,                   0x00002,  "1"
HKR, ,                                  bssType,                        0x00002,  "1"
HKR, ,                                  ccode,                          0x00002,  "US"
HKR, ,                                  clist,                          0x00002,  ""
HKR, ,                                  defaultKey,                     0x00002,  "0"
HKR, ,                                  EncryptionAlg,                  0x00002,  "2"
HKR, ,                                  FragThreshold,                  0x00002,  "2346"
HKR, ,                                  HwTxRetries,                    0x00002,  "4"
HKR, ,                                  privacyInvoked,                 0x00002,  "0"
HKR, ,                                  QoS,                            0x00002,  "0"
HKR, ,                                  rateCtrlEnable,                 0x00002,  "1"
HKR, ,                                  RTSThreshold,                   0x00002,  "2346"
HKR, ,                                  scanType,                       0x00002,  "2"
HKR, ,                                  SwTxRetryScale,                 0x00002,  "6"
HKR, ,                                  SmeEnable,                      0x00002,  "1"
HKR, ,                                  adhocChannel,                   0x00002,  "2462"
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  capLinkSp,                      0x00002,  "2"
HKR, ,                                  pcieAspm,                       0x00002,  "0"
HKR, ,                                  LanExpress,                     0,         "AS00"
HKR, ,                                  DynamicConfig,                  0,         "0"

[customer4c.reg]
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"
HKR, ,                                  abolt,                          0x00002,  "0"
HKR, ,                                  sleepMode,                      0x00002,  "1"
HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  %sleepMode_DEFAULT%
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%
HKR, ,                                  shortPreamble,                  0x00002, %shortPreamble_DEFAULT%
HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  %shortPreamble_DEFAULT%
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%
HKR, Ndi\params\authTypeUseOnly,        ParamDesc,                      0,  %authTypeUseOnly%
HKR, Ndi\params\authTypeUseOnly,        Base,                           0,  "10"
HKR, Ndi\params\authTypeUseOnly,        default,                        0,  "0"
HKR, Ndi\params\authTypeUseOnly,        type,                           0,  "enum"
HKR, Ndi\params\authTypeUseOnly\enum,   "0",                            0,  %authAuto%
HKR, Ndi\params\authTypeUseOnly\enum,   "1",                            0,  %authOpen%
HKR, Ndi\params\authTypeUseOnly\enum,   "2",                            0,  %authShared%
HKR, ,                                  beaconInterval,                 0x00002,  "100"
HKR, ,                                  bkScanEnable,                   0x00002,  "1"
HKR, ,                                  bssType,                        0x00002,  "1"
HKR, ,                                  ccode,                          0x00002,  "US"
HKR, ,                                  clist,                          0x00002,  ""
HKR, ,                                  defaultKey,                     0x00002,  "0"
HKR, ,                                  EncryptionAlg,                  0x00002,  "2"
HKR, ,                                  FragThreshold,                  0x00002,  "2346"
HKR, ,                                  HwTxRetries,                    0x00002,  "4"
HKR, ,                                  privacyInvoked,                 0x00002,  "0"
HKR, ,                                  QoS,                            0x00002,  "0"
HKR, ,                                  rateCtrlEnable,                 0x00002,  "1"
HKR, ,                                  RTSThreshold,                   0x00002,  "2346"
HKR, ,                                  scanType,                       0x00002,  "2"
HKR, ,                                  SwTxRetryScale,                 0x00002,  "6"
HKR, ,                                  SmeEnable,                      0x00002,  "1"
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  LanExpress,                     0,         "AS00"
HKR, ,                                  DynamicConfig,                  0,         "0"

[customer4a_ASPM.reg]
HKR, ,                                  pcieAspm,                       0x00002,  "0"

[customer5.reg]
HKR, ,                                  forceBias,                      0x00002,  "2"
HKR, ,                                  enable2GHzHt40Cap,                    0,  "1"

[customer5.11nLED.reg]
HKR, ,                                  gpioLedCustom,                  0x00002,  "1"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "2"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "1"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "0"

[customer5.3x3.reg]
HKR, ,                                  txChainSelect,                 	0x00002,  "7"
HKR, ,                                  RxChainSelect,                 	0x00002,  "7"

[customer5.PCIe11nLed.reg]
HKR, ,                                  gpioLedCustom,                  0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"

[customer9.reg]
HKR, Ndi\params\MapRegisters,           ParamDesc,                      0,  %MapRegisters%
HKR, Ndi\params\MapRegisters,           default,                        0,  "256"
HKR, Ndi\params\MapRegisters,           min,                            0,  "32"
HKR, Ndi\params\MapRegisters,           max,                            0,  "512"
HKR, Ndi\params\MapRegisters,           step,                           0,  "8"
HKR, Ndi\params\MapRegisters,           base,                           0,  "10"
HKR, Ndi\params\MapRegisters,           type,                           0,  "int"
HKR, Ndi\params\NetworkAddress,         ParamDesc,                      0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,         default,                        0,  ""
HKR, Ndi\params\NetworkAddress,         LimitText,                      0,  "12"
HKR, Ndi\params\NetworkAddress,         UpperCase,                      0,  "1"
HKR, Ndi\params\NetworkAddress,         optional,                       0,  "1"
HKR, Ndi\params\NetworkAddress,         type,                           0,  "edit"
HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "2"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%
HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  "1"
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%
HKR, Ndi\params\radioEnable,            ParamDesc,                      0,  %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,  "10"
HKR, Ndi\params\radioEnable,            default,                        0,  "1"
HKR, Ndi\params\radioEnable,            type,                           0,  "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,  %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,  %radioEnableOff%
HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"
HKR, Ndi\params\ccx5FeatureEnable,      ParamDesc,                      0,  %ccx5FeatureEnable%
HKR, Ndi\params\ccx5FeatureEnable,      Base,                           0,  "10"
HKR, Ndi\params\ccx5FeatureEnable,      default,                        0,  "0"
HKR, Ndi\params\ccx5FeatureEnable,      type,                           0,  "enum"
HKR, Ndi\params\ccx5FeatureEnable\enum, "1",                            0,  %ccx5FeatureEnableMfpEnable%
HKR, Ndi\params\ccx5FeatureEnable\enum, "0",                            0,  %ccx5FeatureEnableMfpDisable%
HKR, CustomParams\Configurations,       MajorVersion,                   0x10003,  2
HKR, CustomParams\Configurations,       MinorVersion,                   0x10003,  0
HKR, CustomParams\Configurations,       SelectedConfigurationIndex,     0x10003,  0
HKR, CustomParams\Configurations,       SelectedConfigurationName,      0x00002,  "Default"
HKR, ,                                  AwakeTimePerf,                  0,  "1000"                  
HKR, ,                                  abolt,                          0x00002,  "0"
HKR, ,                                  pcieAspm,                       0x00002,  "0"

[COMMON_AG.reg]
HKR, ,                                  NetBand,                        0x00002,  %NetBand_DEF_STR_AG%
HKR, ,                                  AdHocBand,                      0x00002,  %AdhocBand_DEF_STR_AG%
HKR, CustomParams\Configurations,       NicType,                        0x10003,  2

[10261a3b.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,									OemLinkLED,			    		0x00002,  "1"

[customer10.LED3.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"

[customer10.reg]
HKR, ,                                  gpioPinFunc1,                  0x00002,  "1"

[customer11.reg]
HKR, Ndi\params\MapRegisters,           ParamDesc,                      0,  %MapRegisters%
HKR, Ndi\params\MapRegisters,           default,                        0,  "256"
HKR, Ndi\params\MapRegisters,           min,                            0,  "32"
HKR, Ndi\params\MapRegisters,           max,                            0,  "512"
HKR, Ndi\params\MapRegisters,           step,                           0,  "8"
HKR, Ndi\params\MapRegisters,           base,                           0,  "10"
HKR, Ndi\params\MapRegisters,           type,                           0,  "int"

HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "2"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  "1"
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%

HKR, Ndi\params\radioEnable,            ParamDesc,                      0,  %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,  "10"
HKR, Ndi\params\radioEnable,            default,                        0,  "1"
HKR, Ndi\params\radioEnable,            type,                           0,  "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,  %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,  %radioEnableOff%

HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"

HKR, Ndi\params\ccx5FeatureEnable,      ParamDesc,                      0,  %ccx5FeatureEnable%
HKR, Ndi\params\ccx5FeatureEnable,      Base,                           0,  "10"
HKR, Ndi\params\ccx5FeatureEnable,      default,                        0,  "0"
HKR, Ndi\params\ccx5FeatureEnable,      type,                           0,  "enum"
HKR, Ndi\params\ccx5FeatureEnable\enum, "1",                            0,  %ccx5FeatureEnableMfpEnable%
HKR, Ndi\params\ccx5FeatureEnable\enum, "0",                            0,  %ccx5FeatureEnableMfpDisable%

HKR, CustomParams\Configurations,       MajorVersion,                   0x10003,  2
HKR, CustomParams\Configurations,       MinorVersion,                   0x10003,  0

HKR, CustomParams\Configurations,       SelectedConfigurationIndex,     0x10003,  0
HKR, CustomParams\Configurations,       SelectedConfigurationName,      0x00002,  "Default"

HKR, CustomParams\Configurations,       NicType,                        0x10003,  1

HKR, Ndi\params\bkScanEnable,           ParamDesc,                      0,        %bkScanEnable%
HKR, Ndi\params\bkScanEnable,           Base,                           0,        "10"
HKR, Ndi\params\bkScanEnable,           default,                        0,        "1"
HKR, Ndi\params\bkScanEnable,           type,                           0,        "enum"
HKR, Ndi\params\bkScanEnable\enum,      "1",                            0,        %bkScanEnableOn%
HKR, Ndi\params\bkScanEnable\enum,      "0",                            0,        %bkScanEnableOff%

HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,        %roamRssi11A%
HKR, Ndi\params\roamRssiA,              default,                        0,        "15"
HKR, Ndi\params\roamRssiA,              min,                            0,        "1"
HKR, Ndi\params\roamRssiA,              max,                            0,        "95"
HKR, Ndi\params\roamRssiA,              step,                           0,        "1"
HKR, Ndi\params\roamRssiA,              base,                           0,        "10"
HKR, Ndi\params\roamRssiA,              type,                           0,        "int"

HKR, Ndi\params\roamRssiBOnly,          ParamDesc,                      0,        %roamRssi11BOnly%
HKR, Ndi\params\roamRssiBOnly,          default,                        0,        "8"
HKR, Ndi\params\roamRssiBOnly,          min,                            0,        "0"
HKR, Ndi\params\roamRssiBOnly,          max,                            0,        "95"
HKR, Ndi\params\roamRssiBOnly,          step,                           0,        "1"
HKR, Ndi\params\roamRssiBOnly,          base,                           0,        "10"
HKR, Ndi\params\roamRssiBOnly,          type,                           0,        "int"

HKR, Ndi\params\roamRssiB,              ParamDesc,                      0,        %roamRssi11B%
HKR, Ndi\params\roamRssiB,              default,                        0,        "24"
HKR, Ndi\params\roamRssiB,              min,                            0,        "0"
HKR, Ndi\params\roamRssiB,              max,                            0,        "95"
HKR, Ndi\params\roamRssiB,              step,                           0,        "1"
HKR, Ndi\params\roamRssiB,              base,                           0,        "10"
HKR, Ndi\params\roamRssiB,              type,                           0,        "int"

HKR, Ndi\params\roamRateA,              ParamDesc,                      0,        %roamRateA%
HKR, Ndi\params\roamRateA,              Base,                           0,        "10"
HKR, Ndi\params\roamRateA,              default,                        0,        "24000"
HKR, Ndi\params\roamRateA,              type,                           0,        "enum"
HKR, Ndi\params\roamRateA\enum,         "6000",                         0,        %roamRateA6M%
HKR, Ndi\params\roamRateA\enum,         "9000",                         0,        %roamRateA9M%
HKR, Ndi\params\roamRateA\enum,         "12000",                        0,        %roamRateA12M%
HKR, Ndi\params\roamRateA\enum,         "18000",                        0,        %roamRateA18M%
HKR, Ndi\params\roamRateA\enum,         "24000",                        0,        %roamRateA24M%
HKR, Ndi\params\roamRateA\enum,         "36000",                        0,        %roamRateA36M%
HKR, Ndi\params\roamRateA\enum,         "48000",                        0,        %roamRateA48M%
HKR, Ndi\params\roamRateA\enum,         "54000",                        0,        %roamRateA54M%

HKR, Ndi\params\roamRateBOnly,          ParamDesc,                      0,        %roamRateBOnly%
HKR, Ndi\params\roamRateBOnly,          Base,                           0,        "10"
HKR, Ndi\params\roamRateBOnly,          default,                        0,        "5000"
HKR, Ndi\params\roamRateBOnly,          type,                           0,        "enum"
HKR, Ndi\params\roamRateBOnly\enum,     "1000",                         0,        %roamRateBOnly1M%
HKR, Ndi\params\roamRateBOnly\enum,     "2000",                         0,        %roamRateBOnly2M%
HKR, Ndi\params\roamRateBOnly\enum,     "5000",                         0,        %roamRateBOnly5M%
HKR, Ndi\params\roamRateBOnly\enum,     "11000",                        0,        %roamRateBOnly11M%

HKR, Ndi\params\roamRateB,              ParamDesc,                      0,        %roamRateB%
HKR, Ndi\params\roamRateB,              Base,                           0,        "10"
HKR, Ndi\params\roamRateB,              default,                        0,        "9000"
HKR, Ndi\params\roamRateB,              type,                           0,        "enum"
HKR, Ndi\params\roamRateB\enum,         "1000",                         0,        %roamRateB1M%
HKR, Ndi\params\roamRateB\enum,         "2000",                         0,        %roamRateB2M%
HKR, Ndi\params\roamRateB\enum,         "5000",                         0,        %roamRateB5M%
HKR, Ndi\params\roamRateB\enum,         "6000",                         0,        %roamRateB6M%
HKR, Ndi\params\roamRateB\enum,         "9000",                         0,        %roamRateB9M%
HKR, Ndi\params\roamRateB\enum,         "11000",                        0,        %roamRateB11M%

HKR, Ndi\params\pcieAspm,               ParamDesc,                      0,        %pcieAspm%
HKR, Ndi\params\pcieAspm,               Base,                           0,        "10"
HKR, Ndi\params\pcieAspm,               default,                        0,        "0"
HKR, Ndi\params\pcieAspm,               type,                           0,        "enum"
HKR, Ndi\params\pcieAspm\enum,          "0",                            0,        %pcieAspmOff%
HKR, Ndi\params\pcieAspm\enum,          "2",                            0,        %pcieAspmL1On%

[customer11_11n40wmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "61467"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "40964",                        0,        %wModeSelect11bonly%
HKR, Ndi\params\wModeSelect\enum,       "20483",                        0,        %wModeSelect11na%
HKR, Ndi\params\wModeSelect\enum,       "40988",                        0,        %wModeSelect11nbg%
HKR, Ndi\params\wModeSelect\enum,       "61467",                        0,        %wModeSelect11abgn%

[customer11_11nwmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "49719"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "32772",                        0,        %wModeSelect11bonly%
HKR, Ndi\params\wModeSelect\enum,       "16387",                        0,        %wModeSelect11na%
HKR, Ndi\params\wModeSelect\enum,       "32796",                        0,        %wModeSelect11nbg%
HKR, Ndi\params\wModeSelect\enum,       "49719",                        0,        %wModeSelect11abgn%

[customer11_legacywmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "2079"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "4",                            0,        %wModeLegacy11bonly%
HKR, Ndi\params\wModeSelect\enum,       "3",                            0,        %wModeLegacy11a%
HKR, Ndi\params\wModeSelect\enum,       "28",                           0,        %wModeLegacy11bg%
HKR, Ndi\params\wModeSelect\enum,       "2079",                         0,        %wModeLegacy11abg%

[customer11Ant.reg]
HKR, Ndi\params\antennaSwitch,          ParamDesc,                      0,        %antennaSwitch%
HKR, Ndi\params\antennaSwitch,          Base,                           0,        "10"
HKR, Ndi\params\antennaSwitch,          default,                        0,        "0"
HKR, Ndi\params\antennaSwitch,          type,                           0,        "enum"
HKR, Ndi\params\antennaSwitch\enum,     "1",                            0,        %antennaSwitchA%
HKR, Ndi\params\antennaSwitch\enum,     "2",                            0,        %antennaSwitchB%
HKR, Ndi\params\antennaSwitch\enum,     "0",                            0,        %antennaSwitchAuto%

[customer11ACStatus.reg]
HKR, ,                                  overrideACstatus,               0x00002,  "2"

[customer12.reg]
HKR, ,                                  txChainSelect,                 	0x00002,  "5"

[customer12Led0.reg]
HKR, ,                  		LinkLedFunc,       		0, "19"
HKR, ,                  	        ActivityLedFunc,       	        0, "21" 

[customer12Led1.reg]
HKR, ,                  		LinkLedFunc,       		0, "03"
HKR, ,                  		ActivityLedFunc,       		0, "05"

[customer12led2.reg]
HKR, ,                  		LinkLedFunc,       		0, "07"
HKR, ,                  		ActivityLedFunc,       		0, "05"

[Customer14.led.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[Customer15a.led.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[Customer15b.led.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[customer_Samsung.reg]
HKR,NDI\params\ignore11dBeacon,ParamDesc,,	%Mode11d%
HKR,NDI\params\ignore11dBeacon,type,,		"enum"
HKR,NDI\params\ignore11dBeacon,Default,,	"1"
HKR,NDI\params\ignore11dBeacon\enum,0,,		%Mode11dEnable%
HKR,NDI\params\ignore11dBeacon\enum,1,,		%Mode11dDisable% 

[customer_IODATA.reg]
HKR, Ndi\params\bssAgingPeriod,         ParamDesc,                      0,  %bssAgingPeriod%
HKR, Ndi\params\bssAgingPeriod,         default,                        0,  "10"
HKR, Ndi\params\bssAgingPeriod,         min,                            0,  "0"
HKR, Ndi\params\bssAgingPeriod,         max,                            0,  "256"
HKR, Ndi\params\bssAgingPeriod,         step,                           0,  "10"
HKR, Ndi\params\bssAgingPeriod,         base,                           0,  "10"
HKR, Ndi\params\bssAgingPeriod,         type,                           0,  "int"

HKR, Ndi\params\MapRegisters,           ParamDesc,                      0,  %MapRegisters%
HKR, Ndi\params\MapRegisters,           default,                        0,  "256"
HKR, Ndi\params\MapRegisters,           min,                            0,  "32"
HKR, Ndi\params\MapRegisters,           max,                            0,  "512"
HKR, Ndi\params\MapRegisters,           step,                           0,  "8"
HKR, Ndi\params\MapRegisters,           base,                           0,  "10"
HKR, Ndi\params\MapRegisters,           type,                           0,  "int"

HKR, Ndi\params\NetworkAddress,         ParamDesc,                      0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,         default,                        0,  ""
HKR, Ndi\params\NetworkAddress,         LimitText,                      0,  "12"
HKR, Ndi\params\NetworkAddress,         UpperCase,                      0,  "1"
HKR, Ndi\params\NetworkAddress,         optional,                       0,  "1"
HKR, Ndi\params\NetworkAddress,         type,                           0,  "edit"

HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "2"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  "1"
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%

HKR, Ndi\params\radioEnable,            ParamDesc,                      0,  %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,  "10"
HKR, Ndi\params\radioEnable,            default,                        0,  "1"
HKR, Ndi\params\radioEnable,            type,                           0,  "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,  %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,  %radioEnableOff%

HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"

HKR, Ndi\params\ccx5FeatureEnable,      ParamDesc,                      0,  %ccx5FeatureEnable%
HKR, Ndi\params\ccx5FeatureEnable,      Base,                           0,  "10"
HKR, Ndi\params\ccx5FeatureEnable,      default,                        0,  "1"
HKR, Ndi\params\ccx5FeatureEnable,      type,                           0,  "enum"
HKR, Ndi\params\ccx5FeatureEnable\enum, "1",                            0,  %ccx5FeatureEnableMfpEnable%
HKR, Ndi\params\ccx5FeatureEnable\enum, "0",                            0,  %ccx5FeatureEnableMfpDisable%

HKR, CustomParams\Configurations,       MajorVersion,                   0x10003,  2
HKR, CustomParams\Configurations,       MinorVersion,                   0x10003,  0

HKR, CustomParams\Configurations,       SelectedConfigurationIndex,     0x10003,  0
HKR, CustomParams\Configurations,       SelectedConfigurationName,      0x00002,  "Default"

HKR, ,                  		LinkLedFunc,       		0, "49"
HKR, ,                  		ActivityLedFunc,       		0, "51"

[cemspecled_func1_1.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[cemspecled_func1_3.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[cemspecled_func1_8.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "8"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[cemspecled_func2_8.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "8"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[rssiAdjust.reg]
HKR, ,                                  rssiAdjust,                     0x00002,  "7"

[cmdRegister.reg]
HKR, ,                                  cmdRegister,                    0x00002,  "838"

[htAdhocdisable.reg]
HKR, ,                                  htAdhocEnable,                  0x00002,  "0"

[xb72.via.reg]
HKLM, SYSTEM\CurrentControlSet\Services\pci\Parameters,168c0024,0x00000001, 00,00,00,20,00,00,00,00

[htAdhoc.reg]
HKR, Ndi\params\htAdhocEnable,          ParamDesc,                      0,  %AdHoc11n%
HKR, NDI\params\htAdhocEnable,type,,    "enum"
HKR, NDI\params\htAdhocEnable,Default,,	"0"
HKR, NDI\params\htAdhocEnable\enum,0,,	%Disable%
HKR, NDI\params\htAdhocEnable\enum,1,,	%Enable%

[htWepTkipOpt.reg]
HKR, Ndi\params\htEnableWepTkip,          ParamDesc,                      0,  %WepTkip11n%
HKR, NDI\params\htEnableWepTkip,type,,	  "enum"
HKR, NDI\params\htEnableWepTkip,Default,, "1"
HKR, NDI\params\htEnableWepTkip\enum,0,,  %Disable%
HKR, NDI\params\htEnableWepTkip\enum,1,,  %Enable%

[htEnableWepTkip.reg]
HKR, ,                                  htEnableWepTkip,                  0x00002,  "1"

[d3forcel1disable.reg]
HKR, ,                                  pcieWaen,                         0x00002,  "4212539"

[d3forcel1disable1.reg]
HKR, ,                                  pcieWaen,                         0x00002,  "4212539"
HKR, ,                                  halPcieDetach,                    0x00002,  "1"

[janusda.reg]
HKR, ,                                  btCoexEnable,                     0x00002,  "4"
HKR, ,                                  btCoexAgent,                      0x00002,  "1"

[merlinshiftdelay.reg]
HKR, ,                                  analogShiftRegDelay,            0x00002,  "10"

[minpower.reg]
HKR, ,                                  legacyMinTxPowerLimit,            0x00002,  "10"

[wowenable.reg]
HKR, ,                                  wowEnable,                      0x00002,  "1"

[overrideAC.reg]
HKR, ,                                  overrideACstatus,               0x00002,  "1"

[triggerlevelkiteonly.reg]
HKR, ,                                  txTrigLevelMax ,                0x00002,  "32"

[c3war.reg]
HKR, ,                                  c3WarTimerPeriod,               0x00002,  "130"

;-----------------------------------------------------------------------------
; ATHER NT specific
;

[ATHER.reg]
HKR, Ndi,             Service,      0, "AR5416"
HKR, Ndi\Interfaces,  UpperRange,   0, "ndis5"
HKR, Ndi\Interfaces,  LowerRange,   0, "ethernet"

[ATHER.Service]
DisplayName     = %ATHER.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\athwx.sys
LoadOrderGroup  = NDIS

;-----------------------------------------------------------------------------
; ATHER NT/XP common
;
[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, ,                  EventMessageFile,   0x00020000,   "%%SystemRoot%%\System32\netevent.dll"
HKR, ,                  TypesSupported,     0x00010001,   7

;----------------------------------------------------------------------------
; System TCPIP parameter changes
;
[sys.TcpParams.reg]
HKLM, SYSTEM\CurrentControlSet\Services\Tcpip\Parameters, Tcp1323Opts, 0x00010001, 0x00000003
HKLM, SYSTEM\CurrentControlSet\Services\Tcpip\Parameters, TcpWindowSize, 0x00010001, 0x00040000

[sys.TcpParamslan.reg]
HKLM, SYSTEM\CurrentControlSet\Services\Tcpip\Parameters, Tcp1323Opts, 0x00010001, 0x00000001
HKLM, SYSTEM\CurrentControlSet\Services\Tcpip\Parameters, TcpWindowSize, 0x00010001, 0x00040000

;----------------------------------------------------------------------------
; NT Files to Copy
[ATHER.CopyFiles.nt]
athwx.sys,,,2

[ATHER.DelIniFiles]
Athnic.ini,,,1

[SourceDisksNames]
;
; diskid = description[, [tagfile] [, <unused>, subdir]]
;
1 = %Atheros_Disk%,,,

;----------------------------------------------------------------------------
; Source Files
[SourceDisksFiles]
ar54169x.sys                 = 1,, ; on distribution disk 1
athwx.sys                   = 1,, ; on distribution disk 1


[DestinationDirs]
ATHER.CopyFiles.nt           = 12
;ATHER.win.CopyFiles          = 10,system32\drivers ; %SystemRoot%\system32\drivers
ATHER.DelIniFiles            = 10,system32\drivers ; %SystemRoot%\system32\drivers
DefaultDestDir               = 11

[DEFAULTDESTDIRS]
;


[Strings]
Atheros                      = "Atheros"
Gigabyte                     = "Gigabyte Technology Corp."			 
MapRegisters                 = "Map Registers"
NetworkAddress               = "Network Address"
sleepMode                    = "Power Save Mode"
scanTimeValid                = "Scan Valid Interval"
scanTime                     = "Roam Time (sec)"
roamRssiA                    = "Roam Time Threshold (db)"
sleepModeOff                 = "Off"
sleepModeNormal              = "Normal"
sleepModeMax                 = "Maximum"
tpc                          = "Transmit Power"
tpcLowest                    = "Lowest"
tpc12                        = "12.5%"
tpc25                        = "25%"
tpc50                        = "50%"
tpc100                       = "100%"
shortPreamble                = "802.11b Preamble"
shortPreambleEnable          = "Long and Short"
shortPreambleDisable         = "Long only"
radioEnable                  = "Radio On/Off"
radioEnableOn                = "On"
radioEnableOff               = "Off"
WirelessMode                 = "Wireless Mode Selection"
WirelessModeAuto             = "Auto"
WirelessMode5GHzOnly         = "5 GHz Only"
WirelessMode2GHzOnly         = "2.4 GHz Only"
WirelessMode11bgOnly         = "802.11b/g"
rssiThrHigh                  = "RSSI Threshold"
rssiThrHighNormal            = "Normal"
rssiThrHighMin               = "Min"
roamPolicy                   = "Roaming Policy"
roamPolicyVeryLow            = "Very Low"
roamPolicyLow                = "Low"
roamPolicyNormal             = "Normal"
roamPolicyHigh               = "High"
roamPolicyVeryHigh           = "Very High"
scanTimeValidcust            = "Roam Time (sec)"
scanTimeValidcust120         = "120"
scanTimeValidcust60          = "60"
scanTimeValidcust45          = "45"
scanTimeValidcust30          = "30"
scanTimeValidcust20          = "20"
scanTimeValidcust10          = "10"
scanTimeValidcust5           = "5"
sleepMode_DEFAULT            = "2"  
NetBand_DEF_STR_A            = "3"                       ; (A/T) 
NetBand_DEF_STR_AB           = "7"                       ; (A/T/B)   
NetBand_DEF_STR_G            = "12"                      ; (B/G)     
NetBand_DEF_STR_AG           = "15"                      ; (A/T/B/G)
AdhocBand_DEF_STR_A          = "1"                       ; (A)
AdhocBand_DEF_STR_AB         = "1"                       ; (A)
AdhocBand_DEF_STR_G          = "0"                       ; (B)
AdhocBand_DEF_STR_AG         = "0"                       ; (B)
shortPreamble_DEFAULT        = "1"
authTypeUseOnly              = "802.11 Authentication Type"
authAuto                     = "Auto"
authOpen                     = "Open"
authShared                   = "Shared"
bkScanEnable                 = "BackgroundScan On/Off"
bkScanEnableOn               = "On"
bkScanEnableOff              = "Off"
roamRssi11A                  = "roamRssiA"
roamRssi11B                  = "roamRssiB"
roamRssi11BOnly              = "roamRssiBOnly"
roamRateA                    = "roamRateA"
roamRateA6M                  = " 6Mbps"
roamRateA9M                  = " 9Mbps"
roamRateA12M                 = "12Mbps"
roamRateA18M                 = "18Mbps"
roamRateA24M                 = "24Mbps"
roamRateA36M                 = "36Mbps"
roamRateA48M                 = "48Mbps"
roamRateA54M                 = "54Mbps"
roamRateBOnly                = "roamRateBOnly"
roamRateBOnly1M              = " 1Mbps"
roamRateBOnly2M              = " 2Mbps"
roamRateBOnly5M              = " 5Mbps"
roamRateBOnly11M             = "11Mbps"
roamRateB                    = "roamRateB"
roamRateB1M                  = " 1Mbps"
roamRateB2M                  = " 2Mbps"
roamRateB5M                  = " 5Mbps"
roamRateB6M                  = " 6Mbps"
roamRateB9M                  = " 9Mbps"
roamRateB11M                 = "11Mbps"
pcieAspm                     = "pcieAspm"
pcieAspmOff                  = "L0s Off, L1 Off"
pcieAspmL1On                 = "L0s Off, L1 On"
wModeSelect                  = "Wireless Mode"
wModeSelect11bonly           = "11b only"
wModeSelect11nbg             = "11n(2.4GHz) and g and b"
wModeSelect11na              = "11n(5GHz) and a"
wModeSelect11abgn            = "11abgn"
wModeLegacy11a               = "11a only"
wModeLegacy11bonly           = "11b only"
wModeLegacy11bg              = "11g and 11b"
wModeLegacy11abg             = "11abg"
antennaSwitch                = "AntennaSwitch"
antennaSwitchAuto            = "Auto"
antennaSwitchA               = "Antenna A"
antennaSwitchB               = "Antenna B"
uapsdEnabledBE               = "Power Save Policy (Best Effort)"
uapsdEnabledBEOn             = "WMM Power Save (UAPSD)"
uapsdEnabledBEOff            = "Legacy Power Save"
uapsdEnabledBK               = "Power Save Policy (Background)"
uapsdEnabledBKOn             = "WMM Power Save (UAPSD)"
uapsdEnabledBKOff            = "Legacy Power Save"
uapsdEnabledVO               = "Power Save Policy (Voice)"
uapsdEnabledVOOn             = "WMM Power Save (UAPSD)"
uapsdEnabledVOOff            = "Legacy Power Save"
uapsdEnabledVI               = "Power Save Policy (Video)"
uapsdEnabledVIOn             = "WMM Power Save (UAPSD)"
uapsdEnabledVIOff            = "Legacy Power Save"
psPoll                       = "Power Save Legacy Algorithm"
psPollEnable                 = "PS Poll"
psPollDisable                = "PS non Poll"
smpsDynamic                  = "Dynamic MIMO Power Save"
smpsDynamicEnable            = "Enable"
smpsDynamicDisable           = "Disable"
AdHoc11n                     = "AdHoc 11n"
Enable			     = "Enable"
Disable                      = "Disable"
WepTkip11n                   = "WepTKIP 11n"
ccx5FeatureEnable            = "MFP"
ccx5FeatureEnableMfpEnable   = "Enable"
ccx5FeatureEnableMfpDisable  = "Disable"
Mode11d                      = "11d Mode Switch"
Mode11dEnable                = "Enable"
Mode11dDisable               = "Disable"
RateCtrl                     = "Auto Transmit Rate"
RateCtrlEnable               = "Enable"
RateCtrlDisable              = "Disable"
TxRate11b                    = "11b Transmit Rates"
TxRate11b1M                  = "1 Mbps"
TxRate11b2M                  = "2 Mbps"
TxRate11b5M                  = "5.5 Mbps"
TxRate11b11M                 = "11 Mbps"
TxRate11g                    = "11g Transmit Rates"
TxRate11g1M                  = "1 Mbps"
TxRate11g2M                  = "2 Mbps"
TxRate11g5M                  = "5.5 Mbps"
TxRate11g11M                 = "11 Mbps"
TxRate11g6M                  = "6 Mbps"
TxRate11g9M                  = "9 Mbps"
TxRate11g12M                 = "12 Mbps"
TxRate11g18M                 = "18 Mbps"
TxRate11g24M                 = "24 Mbps"
TxRate11g36M                 = "36 Mbps"
TxRate11g48M                 = "48 Mbps"
TxRate11g54M                 = "54 Mbps"
TxRate11a                    = "11a Transmit Rates"
TxRate11a6M                  = "6 Mbps"
TxRate11a9M                  = "9 Mbps"
TxRate11a12M                 = "12 Mbps"
TxRate11a18M                 = "18 Mbps"
TxRate11a24M                 = "24 Mbps"
TxRate11a36M                 = "36 Mbps"
TxRate11a48M                 = "48 Mbps"
TxRate11a54M                 = "54 Mbps"
FullReset                    = "Full Reset"
bssAgingPeriod               = "Scanlist Aging"

Atheros_Disk                 = "Atheros Driver Disk 1"
ATHER.Service.DispName       = "Atheros AR5008 Wireless Network Adapter Service"
ATHER.DeviceDesc.0013        = "Atheros Wireless Network Adapter"
ATHER.DeviceDesc.001A        = "Atheros AR5005G Wireless Network Adapter"
ATHER.DeviceDesc.001B        = "Atheros AR5006X Wireless Network Adapter"
ATHER.DeviceDesc.1025        = "Atheros AR5001X+ Wireless Network Adapter"
ATHER.DeviceDesc.2025        = "Atheros AR5001X+ Wireless Network Adapter"
ATHER.DeviceDesc.1026        = "Atheros AR5001X+ Wireless Network Adapter"
ATHER.DeviceDesc.2026        = "Atheros AR5001X+ Wireless Network Adapter"
ATHER.DeviceDesc.1027        = "Atheros AR5001X+ Wireless Network Adapter"
ATHER.DeviceDesc.2027        = "Atheros AR5001X+ Wireless Network Adapter"
ATHER.DeviceDesc.1030        = "Atheros AR5002G Wireless Network Adapter"
ATHER.DeviceDesc.2030        = "Atheros AR5002G Wireless Network Adapter"
ATHER.DeviceDesc.1031        = "Atheros AR5002X Wireless Network Adapter"
ATHER.DeviceDesc.2031        = "Atheros AR5002X Wireless Network Adapter"
ATHER.DeviceDesc.1041        = "Atheros AR5004G Wireless Network Adapter"
ATHER.DeviceDesc.2041        = "Atheros AR5004G Wireless Network Adapter"
ATHER.DeviceDesc.1042        = "Atheros AR5004X Wireless Network Adapter"
ATHER.DeviceDesc.2042        = "Atheros AR5004X Wireless Network Adapter"
ATHER.DeviceDesc.1051        = "Atheros AR5005GS Wireless Network Adapter"
ATHER.DeviceDesc.2051        = "Atheros AR5005GS Wireless Network Adapter"
ATHER.DeviceDesc.1053        = "Atheros AR5005GS Wireless Network Adapter"
ATHER.DeviceDesc.2053        = "Atheros AR5005GS Wireless Network Adapter"
ATHER.DeviceDesc.1062        = "Atheros AR5006XS Wireless Network Adapter"
ATHER.DeviceDesc.2062        = "Atheros AR5006XS Wireless Network Adapter"
ATHER.DeviceDesc.3062        = "Atheros AR5006EXS Wireless Network Adapter"
ATHER.DeviceDesc.3063        = "Atheros AR5006EX Wireless Network Adapter"
ATHER.DeviceDesc.3061        = "Atheros AR5006EGS Wireless Network Adapter"
ATHER.DeviceDesc.3065        = "Atheros AR5006EG Wireless Network Adapter"
ATHER.DeviceDesc.2061        = "Atheros AR5006GS Wireless Network Adapter"
ATHER.DeviceDesc.1061        = "Atheros AR5006GS Wireless Network Adapter"
ATHER.DeviceDesc.2065        = "Atheros AR5006G Wireless Network Adapter"
ATHER.DeviceDesc.1065        = "Atheros AR5006G Wireless Network Adapter"
ATHER.DeviceDesc.0055        = "IEEE 802.11a/g Wireless LAN Adapter (A)"
ATHER.DeviceDesc.10CF        = "IEEE 802.11a/g Wireless LAN Adapter (A)"
ATHER.DeviceDesc.3067        = "Atheros AR5007EG Wireless Network Adapter"
ATHER.DeviceDesc.001D        = "Atheros AR5007G Wireless Network Adapter"
ATHER.DeviceDesc.1055        = "Atheros AR5007G Wireless Network Adapter"
ATHER.DeviceDesc.2055        = "Atheros AR5007G Wireless Network Adapter"
ATHER.DeviceDesc.3013        = "11b/g Wireless LAN Mini PCI Express Adapter"
ATHER.DeviceDesc.4013        = "11a/b/g Wireless LAN Mini PCI Express Adapter" 
ATHER.DeviceDesc.1013        = "11b/g Wireless LAN Mini PCI Adapter"
ATHER.DeviceDesc.2013        = "11a/b/g Wireless LAN Mini PCI Adapter II" 
ATHER.DeviceDesc.5013        = "11b/g Wireless LAN Mini PCI Express Adapter II"  
ATHER.DeviceDesc.6013        = "11b/g Wireless LAN Mini PCI Express Adapter III"  
ATHER.DeviceDesc.0023        = "Atheros AR5008 Wireless Network Adapter"
ATHER.DeviceDesc.0032168c    = "11b/g/n Wireless LAN Mini-PCI Express Adapter"
ATHER.DeviceDesc.0033168c    = "11a/b/g/n Wireless LAN Mini-PCI Express Adapter"
ATHER.DeviceDesc.309917AA    = "11a/b/g/n Wireless LAN Adapter"
ATHER.DeviceDesc.0036        = "11b/g/n Wireless LAN Mini-PCI Express Adapter II"
ATHER.DeviceDesc.0037        = "11b/g/n Wireless LAN Mini-PCI Express Adapter III"
ATHER.DeviceDesc.90001385    = "NETGEAR WN711 RangeMax Wireless-N Expresscard Adapter"
ATHER.DeviceDesc.4B001385    = "NETGEAR 108 Mbps Wireless PC Card WG511T"
ATHER.DeviceDesc.5D001385    = "NETGEAR RangeMax(TM) Wireless PC Card WPN511"
ATHER.DeviceDesc.4D001385    = "NETGEAR 108 Mbps Wireless PCI Adapter WG311T"
ATHER.DeviceDesc.4F001385    = "NETGEAR Double 108 Mbps Wireless PC Card WG511U"
ATHER.DeviceDesc.5E001385    = "NETGEAR WPN311 RangeMax(TM) Wireless PCI Adapter"
ATHER.DeviceDesc.E000        = "LAN-Express AS IEEE 802.11g PCI-E Adapter"
ATHER.DeviceDesc.0406        = "LAN-Express AS IEEE 802.11g miniPCI Adapter" 
ATHER.DeviceDesc.0407        = "LAN-Express AS IEEE 802.11a/g miniPCI Adapter"
ATHER.DeviceDesc.3072        = "Atheros AR5008X Wireless Network Adapter"
ATHER.DeviceDesc.3091        = "Atheros AR928X Wireless Network Adapter"
ATHER.DeviceDesc.2091        = "Atheros AR922X Wireless Network Adapter"
ATHER.DeviceDesc.30A1        = "Atheros AR9285 Wireless Network Adapter"
ATHER.DeviceDesc.30AB        = "Atheros AR9002WB-1NG Wireless Network Adapter #1"
ATHER.DeviceDesc.30AD        = "Atheros AR9002WB-1NG Wireless Network Adapter #2"
ATHER.DeviceDesc.30AE        = "Atheros AR5008WB-EG Wireless Network Adapter #1"
ATHER.DeviceDesc.30AF        = "Atheros AR5008WB-EG Wireless Network Adapter #2"
ATHER.DeviceDesc.30A7        = "Atheros AR2427 Wireless Network Adapter"
ATHER.DeviceDesc.30A4        = "Atheros AR9287 Wireless Network Adapter"
ATHER.DeviceDesc.2099        = "Atheros AR9227 Wireless Network Adapter"
GIGA.DeviceDesc.E914	     = "Gigabyte GN-WI03N (mini) PCI WLAN Card"
GIGA.DeviceDesc.E915	     = "Gigabyte GN-WP02N PCI Express WLAN Card"
GIGA.DeviceDesc.E916	     = "Gigabyte GN-WI06N (mini) PCI Express WLAN Card"
GIGA.DeviceDesc.E815	     = "Gigabyte GN-WM02N Express WLAN Card"
GIGA.DeviceDesc.E801         = "Gigabyte GN-WLMA102 Cardbus WLAN Card"
GIGA.DeviceDesc.E811         = "Gigabyte GN-WMAG Cardbus WLAN Card"
GIGA.DeviceDesc.E814         = "Gigabyte GN-WM01GT Cardbus WLAN Card"
GIGA.DeviceDesc.0013         = "Gigabyte GN-WIAH (mini) PCI WLAN Card"
GIGA.DeviceDesc.E901         = "Gigabyte GN-WI01HT (mini) PCI WLAN Card"
GIGA.DeviceDesc.E911         = "Gigabyte GN-WIAG/GN-WPEAG (mini) PCI WLAN Card"
GIGA.DeviceDesc.E912         = "Gigabyte GN-WP01GT (mini) PCI WLAN Card"
GIGA.DeviceDesc.E913         = "Gigabyte GN-WI01GT (mini) PCI-E WLAN Card"
GIGA.DeviceDesc.E917         = "Gigabyte GN-WI07HT (mini) PCI-E WLAN Card"
GIGA.DeviceDesc.E918        = "Gigabyte GN-WS50G (mini) PCI-E WLAN Card"
GIGA.DeviceDesc.E9191458     = "Gigabyte GN-WS53HN Wireless LAN Mini PCI Express Adapter"
ATHER.DeviceDesc.DWA642      = "D-Link DWA-642 RangeBooster N Notebook Adapter"
ATHER.DeviceDesc.DWA645      = "D-Link DWA-645 RangeBooster N650 Notebook Adapter"
ATHER.DeviceDesc.DWA542      = "D-Link DWA-542 RangeBooster N Desktop Adapter"
ATHER.DeviceDesc.DWA547      = "D-Link DWA-547 RangeBooster N650 Desktop Adapter"
ATHER.DeviceDesc.DWA652      = "D-Link DWA-652 XtremeN Notebook Adapter"
ATHER.DeviceDesc.DWA552      = "D-Link DWA-552 XtremeN Desktop Adapter"
ATHER.DeviceDesc.DWA643      = "D-Link DWA-643 Xtreme N ExpressCard Notebook Adapter"
ATHER.DeviceDesc.DWA556      = "D-Link DWA-556 Xtreme N PCIe Desktop Adapter"
ATHER.DeviceDesc.DWA520      = "D-Link DWA-520 Wireless 108G Desktop Adapter"
ATHER.DeviceDesc.DWA620	     = "D-Link DWA-620 Wireless 108G Notebook Adapter"
ATHER.DeviceDesc.WDA1320     = "D-Link WDA-1320 Wireless G Desktop Adapter"
ATHER.DeviceDesc.WDA2320     = "D-Link WDA-2320 RangeBooster G Desktop Adapter"
ATHER.DeviceDesc.WNA2330     = "D-Link WNA-2330 RangeBooster G Notebook Adapter"
ATHER.DeviceDesc.WNA1330     = "D-Link WNA-1330 Wireless G Notebook Adapter"
ATIWC.DeviceDesc.ATICB	     = "Allied Telesyn AT-WCC201g Wireless Card Bus Adapter"
ATIWC.DeviceDesc.ATIPC	     = "Allied Telesyn AT-WCP201g Wireless PCI Adapter"
ATHER.DeviceDesc.0024	     = "Atheros AR5008X Wireless Network Adapter"
ATHER.DeviceDesc.7141144F    = "Atheros AR9281 Wireless Network Adapter"
ATHER.DeviceDesc.7136144F    = "Atheros AR9280 Wireless Network Adapter"
ATHER.DeviceDesc.7163144F    = "Atheros AR9283 Wireless Network Adapter"
ATHER.DeviceDesc.E006105B    = "Atheros AR5B91 Wireless Network Adapter"
ATHER.DeviceDesc.E01F105B    = "Atheros AR5B93 Wireless Network Adapter"
ATHER.DeviceDesc.663111AD    = "Atheros AR5B95 Wireless Network Adapter"
ATHER.DeviceDesc.660311AD    = "Atheros AR5B97 Wireless Network Adapter"
ATHER.DeviceDesc.1000168c    = "Atheros 802.11 a/b/g/n Dualband Wireless Network Module"
ATHER.DeviceDesc.CM9         = "WNC CM9 Wireless LAN mini-PCI Network Adapter"
ATHER.DeviceDesc.1ACE        = "TP-LINK Wireless N Adapter"
ATHER.DeviceDesc.00341B0A    = "Atheros AR9281 802.11b/g/n WLAN HMC Network"
ATHER.DeviceDesc.2A5F103C    = "Foxconn 802.11 a/b/g/n Wireless System Adaptor"
ATHER.DeviceDesc.500011AD    = "HP 802.11a/b/g Wireless Network Adapter"
ATHER.DeviceDesc.500111AD    = "HP 802.11b/g Wireless Network Adapter"
ATHER.DeviceDesc.D05B10FC    = "I-O DATA WHG-AGDN/CB Wireless LAN Adapter"
ATHER.DeviceDesc.7173144F    = "Askey WLAN and BT combo card"