; PccMfsScan_2k.inf for Windows2000
; (C) Panasonic System Networks Co.,Ltd. 2007

[Version]
Signature="$CHICAGO$"
DriverVer=08/23/2007,1.0.8.0
Class=Image
;LayoutFile=Layout.inf, Layout1.inf, Layout2.inf
ClassGUID={6bdd1fc6-810f-11d0-bec7-08002be2092f}
Provider=%Provider%
CatalogFile=PccMfsScan64.cat

[DestinationDirs]
DefaultDestDir=11
USB_SCAN.CopySys32Files=10,system32\drivers
TWAIN.CopyFiles=10,TWAIN_32\PccMfs

[Manufacturer]
%Mfg%=Models,NTamd64

[Models.NTamd64]
"Panasonic MFStation Scan" = USB_SCAN, USB\VID_04DA&PID_150C&MI_00
"Panasonic MFStation Scan" = USB_SCAN, USB\VID_04DA&PID_1506&MI_00
"Panasonic MFStation Scan" = USB_SCAN, USB\VID_04DA&PID_150D&MI_00
"Panasonic MFStation Scan" = USB_SCAN, USB\VID_04DA&PID_150E&MI_00
"Panasonic MFStation Scan" = USB_SCAN, USB\VID_04DA&PID_1502&MI_00
"Panasonic MFStation Scan" = USB_SCAN, USB\VID_04DA&PID_1507&MI_00
[USB_SCAN.NT]
Include=sti.inf
Needs=STI.USBSection
SubClass=StillImage
DeviceType=1
Capabilities=1
Events=USB_SCAN.Events
DeviceData=USB_SCAN.DeviceData
AddReg=USB_SCAN.AddReg.NT
;CopyFiles=USB_SCAN.CopySys32Files,TWAIN.CopyFiles
ICMProfiles="sRGB Color Space Profile.icm"

[USB_SCAN.NT.Services]
Include=sti.inf
Needs=STI.USBSection.Services

[USB_SCAN.AddReg.NT]

[USB_SCAN.CopySys32Files.NT]

[TWAIN.CopyFiles.NT]
PCMFSSD.ds,,,32
PCMFSSD.INI,,,32
;PCMFSSEL.DLL,,,32

[SourceDisksNames]
1 = %Floppy%,,,
2 = %Floppy%,%LANG_CABFILE% ,,

[SourceDisksFiles]
PCMFSSD.ds = 1
PCMFSSD.INI = 1
;PCMFSSEL.DLL = 1


; Default
[Strings]
Provider="Panasonic"
Mfg="Panasonic"
LANG_CABFILE = "SCANNER_CHS.cab"
Location="Panasonic Multi-Function Station Disk"
Floppy="Panasonic Multi-Function Station Disk"

; Chinese_Simplified
[Strings.0804]
Provider="Panasonic"
Mfg="Panasonic"
LANG_CABFILE = "SCANNER_CHS.cab"
Location="Panasonic Multi-Function Station Disk"
Floppy="Panasonic Multi-Function Station Disk"
