SNMP

Overview
  This page allows you to modify the SNMP parameters.
SNMP Mode of Operation
  The operation mode of SNMP is specified.
SNMP v1/v2c Mode Settings
  If using BRAdmin Professional before Ver. 2.80 or BRAdmin Light for Macintosh® before Ver. 1.10 It is necessary to check this setting when accessing the printer.
SNMPv3 Mode Settings
User Name
  Set the 'User name' to use SNMPv3 communication.
Key Type
  The key is used for authentication and encryption.
Password
  16 ASCII characters.
Binary Keys
  32-byte hexadecimal digit.
Context Name
  Set the 'Context Name' to use SNMPv3 communication.