# OMAP4
-omap 4
# Timeout and other config
-t 600 -p SEVM_MDDR_ELPIDA_4G -2 

# eMMC chips support write without prior erase but you can still do an explict erase
# Erase one group starting at offset 0
chip_erase EMMC 80000
# Erase one group starting at an offset of one group
chip_erase EMMC@80000 80000
# Erase the entire device
chip_erase EMMC 0
# Erase to the end of the decvice starting at an offset of one group
chip_erase EMMC@80000 0

# Download binary to start of device
chip_download EMMC .\test_data\pattern_1K.bin
# Download binary to device starting af offset 80000h
chip_download EMMC@80000 .\test_data\pattern_1K.bin

# Upload
chip_upload EMMC 400 c:.\temp\upload.bin
