;**************************************************************************************** 
;
; netr28u.inf
;
;   This installation script supports Windows 8
;   
;
;   Copyright (C) @ 2002-2011MERCURY TECHNOLOGIES CO., LTD. All Rights Reserved.
;   
;
;**************************************************************************************

[Version]
Signature       = "$Windows NT$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %Provider%
CatalogFile     = netr28u.cat ; For WHQL certification.
DriverVer       = 09/28/2012, 5.00.00.0000

[ControlFlags]
;***********Ralink 802.11n board  ***********
ExcludeFromSelect = *

[Manufacturer]
%Ralink%       = Ralink, NTX86.5.1, NTamd64.5.1, NTX86.6.0, NTamd64.6.0, NTX86.6.1, NTamd64.6.1

[Ralink.NTX86.5.1]
; DisplayName Section DeviceID
; ----------- ------- --------

[Ralink.NTamd64.5.1]
; DisplayName Section DeviceID
; ----------- ------- --------

[Ralink.NTX86.6.0]
; DisplayName Section DeviceID
; ----------- ------- --------

[Ralink.NTamd64.6.0]
; DisplayName Section DeviceID
; ----------- ------- --------

[Ralink.NTx86.6.1]
; DisplayName                   Section                     DeviceID
; -----------                   -------                     --------
%Generic.DeviceDesc%            = OS61_RTWLANSB.ndi,        USB\VID_148F&PID_5370
%Generic.DeviceDesc%            = OS61_RTWLANSB.ndi,        USB\VID_148F&PID_5372
%Generic.DeviceDesc%            = OS61_RTWLAN_5572_R.ndi,   USB\VID_148F&PID_5572
%Generic.DeviceDesc%            = OS61_RTWLANR_3573.ndi,    USB\VID_148F&PID_3573
%Generic.DeviceDesc%       	= OS61_RTWLANSB.ndi,        USB\VID_F201&PID_5370

[Ralink.NTamd64.6.1]
; DisplayName Section DeviceID
; ----------- ------- --------

;*******************************************************************************************
; Win7 specific entries
;*******************************************************************************************
[OS61_RTWLANSB.ndi.NT]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
AddReg                  = Common.reg, RTUSB_OS61.ndi.NT.reg, SingleBand.reg, AdhocN.reg, PsControl.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11


[OS61_RTWLANR_3573.ndi.NT]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
AddReg                  = Common.reg, RTUSB_OS61.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, RemoveFlag.reg, TxBf.reg, PsControl.reg, ChannelMode.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11


[OS61_RTWLAN_5572_R.ndi.NT]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
AddReg                  = Common.reg, RTUSB_OS61.ndi.NT.reg, DefaultBand.reg, AdhocN.reg, RemoveFlag.reg, PsControl.reg, ChannelMode.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11


;*******************************************************************************************
; Win7 services sections
;*******************************************************************************************
[OS61_RTWLANSB.ndi.NT.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService              = netr28u, 2, Generic.Service, common.EventLog

[OS61_RTWLANSB.ndi.NT.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[OS61_RTWLANR_3573.ndi.NT.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService              = netr28u, 2, Generic.Service, common.EventLog

[OS61_RTWLANR_3573.ndi.NT.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[OS61_RTWLAN_5572_R.ndi.NT.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService              = netr28u, 2, Generic.Service, common.EventLog

[OS61_RTWLAN_5572_R.ndi.NT.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

;*******************************************************************************************
; NT CoInstallers Sections
;*******************************************************************************************
[OS61_RTWLANSB.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[OS61_RTWLANR_3573.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[OS61_RTWLAN_5572_R.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

;*******************************************************************************************
; common regs for NT
;*******************************************************************************************

[Common.reg]
;
; CCX drastic roaming use
;
HKR, ,                            CCXPktLossLimitTime,    0, "30"

;
; CCX Dbm offset
;
HKR, ,                            CCXDbmOffset,    0, "4"

;
; CCX VO/VI Drop Period, 3 or 5 is recommanded
;
HKR, ,                            CACDropPeriod,    0, "0"

;
; CCX VO/VI Drop Criteria
;
HKR, ,                            CACDropCriteria,    0, "1700"

;
; WirelessMode
;
HKR, ,                            WirelessMode,    0, "9"

;
; Enable TX Burst
;
HKR, ,                            TXBurst,         0, "1"

;
; Use Short Slot Time
;
HKR, ,                            ShortSlot,       0, "1"

;
; Use Ofdm rate in adhoc mode
;
HKR, ,                            AdhocOfdm,       0, "1"

;
; Disable 5GHz adhoc mode
;
HKR, ,                            Adhoc5GDisable,  0, "0"

;
; AdhocN40MHzAllowed
;
HKR, ,                            AdhocN40MHzAllowed,0, "0"

;
; WSC Version2 
HKR, ,                            WSCVersion2,     0x00010001, 0x00000020

;
; WSC 2.0 Testbed for some test items. 
HKR, ,                            WSC20Testbed,     0x00010001, 0x0000000C

;
; PMF On/Off
;
HKR, ,                            MFPC,            0, "1"

;
; Test WHCK Usage
;
HKR, ,				OnTestingWHQL,		0,	"0"
HKR, ,				OnTestingCPUUtil,	0,	"0"

;
; Enable InBoxMode
;
HKR, ,				InBoxMode,		0, "0"

;
; Radio On/Off
;
HKR, ,                            Radio,           0, "0"
HKR, NDI\params\Radio,            ParamDesc,       0, %RadioOnOff%
HKR, NDI\params\Radio,            type,            0, "enum"
HKR, NDI\params\Radio,            default,         0, "0"
HKR, NDI\params\Radio\enum,       1,               0, %Disable%
HKR, NDI\params\Radio\enum,       0,               0, %Enable%

;
; Channel
;
HKR, ,                            Channel,         0, %CHANNEL%
HKR, Default,                     Channel,         0, %CHANNEL%

;
; RDG
;
HKR, ,                            RDG,             0, "1"

;
; WMMCapable
;
HKR, ,                            WMMCapable,      0, "1"

;
; CarrierDetect
;
HKR, ,                            CarrierDetect,   0, "0"

;
; SmartScan
;
HKR, ,                            SmartScan,       0, "0"
HKR, NDI\params\SmartScan,        ParamDesc,       0, %SmartScan%
HKR, NDI\params\SmartScan,        type,            0, "enum"
HKR, NDI\params\SmartScan,        default,         0, "0"
HKR, NDI\params\SmartScan\enum,   0,               0, %Disable%
HKR, NDI\params\SmartScan\enum,   1,               0, %Enable%

;
; Block ACK settings
;
HKR, ,                            BACapability,    0x10001, "0x0b034040"
HKR, Default,                     BACapability,    0x10001, "0x0b034040"

;
; Wifi Direct settings
;
HKR, ,                            WifiDirectControl,    0x10001, "0x84308078"
HKR, Default,                     WifiDirectControl,    0x10001, "0x84308078"

;
; P2P Reinforced ACK check
;
HKR, ,                            P2PAckCheck,    0, "1"
HKR, Default,                     P2PAckCheck,    0, "1"

;
; Enable P2P Video Boost within P2P Group
;
HKR, ,                            P2PVideoBoost,      0, "0"

;
; Transmit Rate setting
;
HKR, ,                            TransmitSetting, 0x10001, "0x2ba15"
HKR, Default,                     TransmitSetting, 0x10001, "0x2ba15"

;
; WPS Device Name
;
HKR, ,                            WPSDevName,      0, %WPS_DEVNAME_DEF_STR%
HKR, Default,                     WPSDevName,      0, %WPS_DEVNAME_DEF_STR%

;
; ProhibitTKIPonHT
;
HKR, ,                            ProhibitTKIPonHT,0, "1"

;
; Link Speed Status
;
HKR, ,                            LinkSpeedStatus, 0, "0"

;
; Fast Roaming Sensitivity
;
HKR, ,                                  FastRoamingSensitivity,    0, "0"
HKR, NDI\params\FastRoamingSensitivity,              ParamDesc,    0, %FAST_ROAMING_SENSITIVITY_STR%
HKR, NDI\params\FastRoamingSensitivity,              Type,         0, "enum"
HKR, NDI\params\FastRoamingSensitivity,              Default,      0, "0"
HKR, NDI\params\FastRoamingSensitivity,              Optional,     0, "0"
HKR, NDI\params\FastRoamingSensitivity\enum,         "0",          0, %DISABLE_STR%
HKR, NDI\params\FastRoamingSensitivity\enum,         "1",          0, %LOWEST_STR%
HKR, NDI\params\FastRoamingSensitivity\enum,         "2",          0, %MEDIUM_LOW_STR%
HKR, NDI\params\FastRoamingSensitivity\enum,         "3",          0, %MEDIUM_STR%
HKR, NDI\params\FastRoamingSensitivity\enum,         "4",          0, %MEDIUM_HIGH_STR%
HKR, NDI\params\FastRoamingSensitivity\enum,         "5",          0, %HIGHEST_STR% 

;
; Selective Suspend
;
HKR, ,                                 *SelectiveSuspend,      0, "1"
HKR, NDI\params\*SelectiveSuspend,         ParamDesc,          0, "Selective Suspend"
HKR, NDI\params\*SelectiveSuspend,         type,               0, "enum"
HKR, NDI\params\*SelectiveSuspend,         default,            0, "1"
HKR, NDI\params\*SelectiveSuspend\enum,    0,                  0, %Disable%
HKR, NDI\params\*SelectiveSuspend\enum,    1,                  0, %Enable%

HKR, ,                                 *SSIdleTimeout,      0, "5"
HKR, NDI\params\*SSIdleTimeout,         ParamDesc,          0, "Selective suspend idle timeout in senonds"
HKR, NDI\params\*SSIdleTimeout,         type,               0, "int"
HKR, NDI\params\*SSIdleTimeout,         default,            0, "5"
HKR, NDI\params\*SSIdleTimeout,         Min,                0, "1"
HKR, NDI\params\*SSIdleTimeout,         Max,                0, "60"

;
; Updated WiFi Driver and devce management setings don't become to the default value
;
[Fujitsu_Common.reg]
;
; CCX drastic roaming use
;
HKR, ,                            CCXPktLossLimitTime,    0, "30"

;
; CCX Dbm offset
;
HKR, ,                            CCXDbmOffset,    0, "4"

;
; CCX VO/VI Drop Period, 3 or 5 is recommanded
;
HKR, ,                            CACDropPeriod,    0, "0"

;
; CCX VO/VI Drop Criteria
;
HKR, ,                            CACDropCriteria,    0, "1700"

;
; WirelessMode
;
;HKR, ,                            WirelessMode,    0, "5"

;
; Enable TX Burst
;
HKR, ,                            TXBurst,         0, "1"

;
; Use Short Slot Time
;
HKR, ,                            ShortSlot,       0, "1"

;
; Use Ofdm rate in adhoc mode
;
HKR, ,                            AdhocOfdm,       0, "1"

;
; Disable 5GHz adhoc mode
;
HKR, ,                            Adhoc5GDisable,  0, "0"

;
; AdhocN40MHzAllowed
;
HKR, ,                            AdhocN40MHzAllowed,0, "0"

;
; WSC Version2 
HKR, ,                            WSCVersion2,     0x00010001, 0x00000020

;
; WSC 2.0 Testbed for some test items. 
HKR, ,                            WSC20Testbed,     0x00010001, 0x0000000C

;
; PMF On/Off
;
HKR, ,                            MFPC,            0, "1"

;
; Test WHCK Usage
;
HKR, ,				OnTestingWHQL,		0,	"0"
HKR, ,				OnTestingCPUUtil,	0,	"0"

;
; Enable InBoxMode
;
HKR, ,				InBoxMode,		0, "0"

;
; Radio On/Off
;
HKR, NDI\params\Radio,            ParamDesc,       0, %RadioOnOff%
HKR, NDI\params\Radio,            type,            0, "enum"
HKR, NDI\params\Radio,            default,         0, "0"
HKR, NDI\params\Radio\enum,       1,               0, %Disable%
HKR, NDI\params\Radio\enum,       0,               0, %Enable%

;
; Channel
;
HKR, ,                            Channel,         0, %CHANNEL%
HKR, Default,                     Channel,         0, %CHANNEL%

;
; RDG
;
HKR, ,                            RDG,             0, "1"

;
; WMMCapable
;
HKR, ,                            WMMCapable,      0, "1"

;
; CarrierDetect
;
HKR, ,                            CarrierDetect,   0, "0"

;
; SmartScan
;
HKR, NDI\params\SmartScan,        ParamDesc,       0, %SmartScan%
HKR, NDI\params\SmartScan,        type,            0, "enum"
HKR, NDI\params\SmartScan,        default,         0, "0"
HKR, NDI\params\SmartScan\enum,   0,               0, %Disable%
HKR, NDI\params\SmartScan\enum,   1,               0, %Enable%

;
; Block ACK settings
;
HKR, ,                            BACapability,    0x10001, "0x0b034040"
HKR, Default,                     BACapability,    0x10001, "0x0b034040"

;
; Wifi Direct settings
;
HKR, ,                            WifiDirectControl,    0x10001, "0x84308078"
HKR, Default,                     WifiDirectControl,    0x10001, "0x84308078"

;
; P2P Reinforced ACK check
;
HKR, ,                            P2PAckCheck,    0, "1"
HKR, Default,                     P2PAckCheck,    0, "1"

;
; Enable P2P Video Boost within P2P Group
;
HKR, ,                            P2PVideoBoost,      0, "0"

;
; Transmit Rate setting
;
HKR, ,                            TransmitSetting, 0x10001, "0x2ba15"
HKR, Default,                     TransmitSetting, 0x10001, "0x2ba15"

;
; WPS Device Name
;
HKR, ,                            WPSDevName,      0, %WPS_DEVNAME_DEF_STR%
HKR, Default,                     WPSDevName,      0, %WPS_DEVNAME_DEF_STR%

;
; ProhibitTKIPonHT
;
HKR, ,                            ProhibitTKIPonHT,0, "1"

;
; Link Speed Status
;
HKR, ,                            LinkSpeedStatus, 0, "0"

;
; Fast Roaming Sensitivity
;
HKR, NDI\params\FastRoamingSensitivity,              ParamDesc,    0, %FAST_ROAMING_SENSITIVITY_STR%
HKR, NDI\params\FastRoamingSensitivity,              Type,         0, "enum"
HKR, NDI\params\FastRoamingSensitivity,              Default,      0, "3"
HKR, NDI\params\FastRoamingSensitivity,              Optional,     0, "0"
HKR, NDI\params\FastRoamingSensitivity\enum,         "0",          0, %DISABLE_STR%
HKR, NDI\params\FastRoamingSensitivity\enum,         "1",          0, %LOWEST_STR%
HKR, NDI\params\FastRoamingSensitivity\enum,         "2",          0, %MEDIUM_LOW_STR%
HKR, NDI\params\FastRoamingSensitivity\enum,         "3",          0, %MEDIUM_STR%
HKR, NDI\params\FastRoamingSensitivity\enum,         "4",          0, %MEDIUM_HIGH_STR%
HKR, NDI\params\FastRoamingSensitivity\enum,         "5",          0, %HIGHEST_STR% 

; AdhocNMode
HKR, NDI\params\AdhocNMode,       ParamDesc,       0, %AdhocNMode%
HKR, NDI\params\AdhocNMode,       type,            0, "enum"
HKR, NDI\params\AdhocNMode,       default,         0, "0"
HKR, NDI\params\AdhocNMode\enum,  0,               0, %Disable%
HKR, NDI\params\AdhocNMode\enum,  1,               0, %Enable% 

; 2.4G/5G Switch
HKR, ,                              RaCoInstOpt,     0,"00101111"
HKR, NDI\params\WirelessMode,       ParamDesc,       0, %WirelessMode%
HKR, NDI\params\WirelessMode,       type,            0, "enum"
HKR, NDI\params\WirelessMode,       default,         0, "5"
HKR, NDI\params\WirelessMode\enum,  5,               0, %WirelessModeBoth%
HKR, NDI\params\WirelessMode\enum,  9,               0, %WirelessMode24G%
HKR, NDI\params\WirelessMode\enum,  8,               0, %WirelessMode5G%
;
; Selective Suspend
;

HKR, NDI\params\*SelectiveSuspend,         ParamDesc,          0, "Selective Suspend"
HKR, NDI\params\*SelectiveSuspend,         type,               0, "enum"
HKR, NDI\params\*SelectiveSuspend,         default,            0, "1"
HKR, NDI\params\*SelectiveSuspend\enum,    0,                  0, %Disable%
HKR, NDI\params\*SelectiveSuspend\enum,    1,                  0, %Enable%


HKR, NDI\params\*SSIdleTimeout,         ParamDesc,          0, "Selective suspend idle timeout in senonds"
HKR, NDI\params\*SSIdleTimeout,         type,               0, "int"
HKR, NDI\params\*SSIdleTimeout,         default,            0, "5"
HKR, NDI\params\*SSIdleTimeout,         Min,                0, "1"
HKR, NDI\params\*SSIdleTimeout,         Max,                0, "60"

[RemoveFlag.reg]
HKR, ,                            SafelyRemoveOff, 0, "1"
                                  
[IEEE80211H.reg]                  
HKR, ,                            IEEE80211H,      0, "0"
HKR, NDI\params\IEEE80211H,       ParamDesc,       0, %IEEE802_11h%
HKR, NDI\params\IEEE80211H,       type,            0, "enum"
HKR, NDI\params\IEEE80211H,       default,         0, "0"
HKR, NDI\params\IEEE80211H\enum,  0,               0, %Disable%
HKR, NDI\params\IEEE80211H\enum,  1,               0, %Enable%

[IEEE80211H_SET.reg]
HKR, ,                            IEEE80211H,      0, "1"
                                  
[CarrierDetect.reg]               
HKR, ,                            CarrierDetect,   0, "1"
                                  
[SmartScan.reg]                   
HKR, ,                            SmartScan,       0, "1"
                                  
[BackgroundScan.reg]
HKR, NDI\params\SmartScan,        ParamDesc,       0, %BackgroundScan%
HKR, NDI\params\SmartScan\enum,   0,               0, %ALLOW%
HKR, NDI\params\SmartScan\enum,   1,               0, %DISALLOW%

[AdhocN.reg]                      
;
; AdhocNMode
;
HKR, ,                            AdhocNMode,      0, "0"
HKR, NDI\params\AdhocNMode,       ParamDesc,       0, %AdhocNMode%
HKR, NDI\params\AdhocNMode,       type,            0, "enum"
HKR, NDI\params\AdhocNMode,       default,         0, "0"
HKR, NDI\params\AdhocNMode\enum,  0,               0, %Disable%
HKR, NDI\params\AdhocNMode\enum,  1,               0, %Enable%

[PsControl.reg]
;
; Power Saving Control
;
HKR, ,                            PSControl,       0x00010001, 0x00000001

; Disable Channel 14 for JP
[InitChn14Disabled.reg]
HKR, ,                            InitChn14Disabled,0,"1"

[SingleBand.reg]
;
; 2.4G Band
;
HKR, ,                                 CountryRegion,      0, "0"
HKR, NDI\params\CountryRegion,         ParamDesc,          0, %CountryRegion24G%
HKR, NDI\params\CountryRegion,         type,               0, "enum"
HKR, NDI\params\CountryRegion,         default,            0, "0"
HKR, NDI\params\CountryRegion\enum,    0,                  0, %CountryRegion24G_0%
HKR, NDI\params\CountryRegion\enum,    1,                  0, %CountryRegion24G_1%
HKR, NDI\params\CountryRegion\enum,    2,                  0, %CountryRegion24G_2%
HKR, NDI\params\CountryRegion\enum,    3,                  0, %CountryRegion24G_3%
HKR, NDI\params\CountryRegion\enum,    4,                  0, %CountryRegion24G_4%
HKR, NDI\params\CountryRegion\enum,    5,                  0, %CountryRegion24G_5%
HKR, NDI\params\CountryRegion\enum,    6,                  0, %CountryRegion24G_6%
HKR, NDI\params\CountryRegion\enum,    7,                  0, %CountryRegion24G_7%

[DefaultBand.reg]
;
; 2.4G Band
;
HKR, ,                                 CountryRegion,      0, "0"
HKR, NDI\params\CountryRegion,         ParamDesc,          0, %CountryRegion24G%
HKR, NDI\params\CountryRegion,         type,               0, "enum"
HKR, NDI\params\CountryRegion,         default,            0, "0"
HKR, NDI\params\CountryRegion\enum,    0,                  0, %CountryRegion24G_0%
HKR, NDI\params\CountryRegion\enum,    1,                  0, %CountryRegion24G_1%
HKR, NDI\params\CountryRegion\enum,    2,                  0, %CountryRegion24G_2%
HKR, NDI\params\CountryRegion\enum,    3,                  0, %CountryRegion24G_3%
HKR, NDI\params\CountryRegion\enum,    4,                  0, %CountryRegion24G_4%
HKR, NDI\params\CountryRegion\enum,    5,                  0, %CountryRegion24G_5%
HKR, NDI\params\CountryRegion\enum,    6,                  0, %CountryRegion24G_6%
HKR, NDI\params\CountryRegion\enum,    7,                  0, %CountryRegion24G_7%

;
; 5G Band
;
HKR, ,                                 CountryRegionABand, 0, "0"
HKR, NDI\params\CountryRegionABand,    ParamDesc,          0, %CountryRegion5G%
HKR, NDI\params\CountryRegionABand,    type,               0, "enum"
HKR, NDI\params\CountryRegionABand,    default,            0, "0"
HKR, NDI\params\CountryRegionABand\enum,0,                 0, %CountryRegion5G_0%
HKR, NDI\params\CountryRegionABand\enum,1,                 0, %CountryRegion5G_1%
HKR, NDI\params\CountryRegionABand\enum,2,                 0, %CountryRegion5G_2%
HKR, NDI\params\CountryRegionABand\enum,3,                 0, %CountryRegion5G_3%
HKR, NDI\params\CountryRegionABand\enum,4,                 0, %CountryRegion5G_4%
HKR, NDI\params\CountryRegionABand\enum,5,                 0, %CountryRegion5G_5%
HKR, NDI\params\CountryRegionABand\enum,6,                 0, %CountryRegion5G_6%
HKR, NDI\params\CountryRegionABand\enum,7,                 0, %CountryRegion5G_7%
HKR, NDI\params\CountryRegionABand\enum,8,                 0, %CountryRegion5G_8%
HKR, NDI\params\CountryRegionABand\enum,9,                 0, %CountryRegion5G_9%
HKR, NDI\params\CountryRegionABand\enum,10,                0, %CountryRegion5G_10%
HKR, NDI\params\CountryRegionABand\enum,11,                0, %CountryRegion5G_11%
HKR, NDI\params\CountryRegionABand\enum,12,                0, %CountryRegion5G_12%
HKR, NDI\params\CountryRegionABand\enum,13,                0, %CountryRegion5G_13%
HKR, NDI\params\CountryRegionABand\enum,14,                0, %CountryRegion5G_14%
HKR, NDI\params\CountryRegionABand\enum,15,                0, %CountryRegion5G_15%
HKR, NDI\params\CountryRegionABand\enum,16,                0, %CountryRegion5G_16%


[SingleBand_DisCh14.reg]
;
; 2.4G Band
;
HKR, ,                                 CountryRegion,      0, "0"
HKR, NDI\params\CountryRegion,         ParamDesc,          0, %CountryRegion24G%
HKR, NDI\params\CountryRegion,         type,               0, "enum"
HKR, NDI\params\CountryRegion,         default,            0, "0"
HKR, NDI\params\CountryRegion\enum,    0,                  0, %CountryRegion24G_0%
HKR, NDI\params\CountryRegion\enum,    1,                  0, %CountryRegion24G_1%
HKR, NDI\params\CountryRegion\enum,    2,                  0, %CountryRegion24G_2%
HKR, NDI\params\CountryRegion\enum,    3,                  0, %CountryRegion24G_3%
HKR, NDI\params\CountryRegion\enum,    6,                  0, %CountryRegion24G_6%
HKR, NDI\params\CountryRegion\enum,    7,                  0, %CountryRegion24G_7%


;
; Customer Request
;
[Customer1.reg]
;
; Allied Request
;
; WPS Device Name
HKR, ,                            WPSDevName,      0, %WPS_DEVNAME_CUSTOMER1%
HKR, Default,                     WPSDevName,      0, %WPS_DEVNAME_CUSTOMER1%

[Customer2.reg]
;
; D-Link Request
;
; WMMCapable
HKR, ,                            WMMCapable,      0, "1"
; Enable TX Burst
HKR, ,                            TXBurst,         0, "1"
; DLSCapable
HKR, ,                            DLSCapable,      0, "1"
; DirectMode
HKR, ,                            DirectMode,      0, "0"

[BTCoexist.reg]
HKR, ,                            BTSoftwareOn,      0, "0"
HKR, ,                            BTConfiguration, 0x00010001, 0x380004fd

[LinkSpeedStatusRxDynamicRate.reg]
;
; LinkSpeedStatus
;
HKR, ,                            LinkSpeedStatus, 0, "2"

[LinkSpeedStatus.reg]
;
; LinkSpeedStatus
;
HKR, ,                            LinkSpeedStatus, 0, "1"

[LinkQualitySetting.reg]
;
;LinkQualitySetting 
;
HKR, ,                            LinkQualitySetting, 0x00010001, "0x51"

; CoInstaller Option for Aurewave, MSI
;
; RaCoInstaller Options
;
[CoInstOpt_DisableN.reg]
HKR, ,                            RaCoInstOpt,     0,"00101111"
HKR, ,                            CountryWirelessMode,     0x00010001, 0x00001000 

; WirelessMode
HKR, ,                            WirelessMode,    0, "3"

[BaldEagle.reg]
;
; Bald Eagle Mechanism
;
HKR, ,                            BaldEagleSSID, 0, %BaldEagle_SSID%

[Led2.reg]
;
; Led Configuration
;
HKR, ,                            LedCfg,  0, "1"   ; 0=firmware(def), 1=asic

[Feature.reg]
HKR, ,                            FeatureSetting, 0x00010001, 0x1

[TxBf.reg]
;
; ETxBfEn
;
HKR, ,                            ETxBfEn,  0, "1"

;
; ETxBfTimeout
;
HKR, ,                            ETxBfTimeout, 0, "40000"

;ss
; ETxBfNonCompressedFeedback
;
HKR, ,                            ETxBfNonCompressedFeedback, 0, "0"

[TxRxConfigByRegistry.reg]
;
;TxRxConfigByRegistry
;
HKR, ,                            TxRxConfigByRegistry, 0, "1"

[MulticastRateAutoSelected.reg]
;
;MulticastRateAutoSelected
;
HKR, ,                            SoftAPForceMulticastRate, 	0,	"11000000"

[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "RaCoInst.dll,ClassCoInstaller"

[NotProhibitTKIPonHT.reg]
;
; Not ProhibitTKIPonHT
;
HKR, ,                            ProhibitTKIPonHT,0, "0"

[WirelessMode_BGN.reg]
; WirelessMode BGN Only
HKR, ,                            RaCoInstOpt,     0,"00101111"
HKR, ,                            CountryWirelessMode,     0x00010001, 0x00001110

HKR, ,                            WirelessMode,    0, "9"

[WirelessModeSwitch.reg]
; 2.4G/5G Switch
HKR, ,                              RaCoInstOpt,     0,"00101111"
HKR, ,                              WirelessMode,    0, "5"
HKR, NDI\params\WirelessMode,       ParamDesc,       0, %WirelessMode%
HKR, NDI\params\WirelessMode,       type,            0, "enum"
HKR, NDI\params\WirelessMode,       default,         0, "5"
HKR, NDI\params\WirelessMode\enum,  5,               0, %WirelessModeBoth%
HKR, NDI\params\WirelessMode\enum,  9,               0, %WirelessMode24G%
HKR, NDI\params\WirelessMode\enum,  8,               0, %WirelessMode5G%


[RoamingDef_medium.reg]
HKR, ,                                FastRoamingSensitivity,    0, "3"
HKR, NDI\params\FastRoamingSensitivity,              Default,    0, "3"


[TssiPatchForAntennaVariation.reg]
HKR, ,                            TssiPatchForAntennaVariation,  0, "1"

[StreamMode.reg]
HKR, ,                            StreamMode,         0, "1"

[AdTxPwrForFCCTest.reg]
HKR, ,                            AdTxPwrForFCCTest,  0, "1"

[CustomizedPowerMode.reg]
HKR, ,                            CustomizedPowerMode,  0, "1"

[ChannelMode.reg]
HKR, ,                                 ChannelMode, 0, "1"
HKR, NDI\params\ChannelMode,    ParamDesc,          0, %CHANNEL_MODE%
HKR, NDI\params\ChannelMode,    type,               0, "enum"
HKR, NDI\params\ChannelMode,    default,            0, "1"
HKR, NDI\params\ChannelMode\enum,0,                 0, %ChannelMode_0%
HKR, NDI\params\ChannelMode\enum,1,                 0, %ChannelMode_1%
HKR, NDI\params\ChannelMode\enum,2,                 0, %ChannelMode_2%

;
; Remove registry
;
[RegRemove.delReg]
; Remove CountryRegion
HKR, NDI\params\CountryRegion
HKR, NDI\params\CountryRegionABand

; Remove IEEE80211H
HKR, NDI\params\IEEE80211H

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************
[NT.CopyFiles]
netr28u.sys,,,2

[NT_CTV1W.CopyFiles]
CTV1W.sys,netr28u.sys,,2

[CoInstaller.CopyFiles]
RaCoInst.dll,,,2
RaCoInst.dat,,,2

[SourceDisksNames]
1 = %INSTALL_DISK_STR%,,,

[SourceDisksFiles]
netr28u.sys                = 1,,
RaCoInst.dll               = 1,,
RaCoInst.dat               = 1,,

[DestinationDirs]
NT.CopyFiles            = 12     ; system32\drivers subdirectory on NT
NT_CTV1W.CopyFiles      = 12
DefaultDestDir          = 11
CoInstaller.CopyFiles	= 11

;*******************************************************************************************
; NT specific
;*******************************************************************************************
[RTUSB_OS61.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "netr28u"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "wlan,ethernet,vwifi"

[RTUSB_CTV1W.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "CTV1W"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "wlan,ethernet,vwifi"

[Generic.Service]
DisplayName                 = %Generic.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\netr28u.sys
LoadOrderGroup              = NDIS

[CTV1W.Service]
DisplayName                 = %CTV1W.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\CTV1W.sys
LoadOrderGroup              = NDIS

[common.EventLog]
AddReg=common.AddEventLog.reg

[cisco_ctv1w.EventLog]
AddReg=CTV1W.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\netr28u.sys"
HKR, , TypesSupported,   0x00010001, 7

[CTV1W.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\CTV1W.sys"
HKR, , TypesSupported,   0x00010001, 7

;*******************************************************************************************
; Strings
;*******************************************************************************************
[strings]
Provider                    = "MERCURY"
Ralink                      = "MERCURY Technology, Corp."

Generic.DeviceDesc          = "MERCURY Wireless N Adapter"
INSTALL_DISK_STR            = "Wireless 11n USB Installation Disk"

Generic.Service.DispName    = "MERCURY Wireless N Adapter"
CTV1W.Service.DispName      = "MERCURY Wireless N Adapter"

;
; Parameters
;
RadioOnOff                  = "Radio On/Off"
Disable                     = "Disable"
Enable                      = "Enable"
CountryRegion24G            = "Country Region (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Country Region (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Multimedia/Gaming Environment"
AdhocNMode                  = "Adhoc support 802.11n"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MERCURY Client"
WPS_DEVNAME_CUSTOMER1       = "MERCURY Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"

FAST_ROAMING_SENSITIVITY_STR = "Roaming Sensitivity" 
DISABLE_STR                 = "6.Disable"
LOWEST_STR                  = "5.Lowest"
MEDIUM_LOW_STR              = "4.Low"
MEDIUM_STR                  = "3.Medium"
MEDIUM_HIGH_STR             = "2.High"
HIGHEST_STR                 = "1.Highest"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF			                = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

;*******************************************************************************************
; Strings --- Simplified Chinese
;*******************************************************************************************
[Strings.0804]
Provider                    = "MERCURY"
Ralink                      = "MERCURY Technology, Corp."
 

Generic.DeviceDesc          = "MERCURY Wireless N Adapter"
INSTALL_DISK_STR            = "Wireless 11n USB Installation Disk"

Generic.Service.DispName    = "MERCURY Wireless N Adapter"
CTV1W.Service.DispName      = "MERCURY Wireless N Adapter"

;
; Parameters
;
RadioOnOff                  = "无线装置 开/关"
Disable                     = "停用"
Enable                      = "启用"
CountryRegion24G            = "频道代码 (2.4GHz)"
CountryRegion24G_0          = "#0 (1-11)"
CountryRegion24G_1          = "#1 (1-13)"
CountryRegion24G_2          = "#2 (10-11)"
CountryRegion24G_3          = "#3 (10-13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1-14)"
CountryRegion24G_6          = "#6 (3-9)"
CountryRegion24G_7          = "#7 (5-13)"
CountryRegion5G             = "频道代码 (5GHz)"
CountryRegion5G_0           = "#0 (36-64,149-165)"
CountryRegion5G_1           = "#1 (36-140)"
CountryRegion5G_2           = "#2 (36-64)"
CountryRegion5G_3           = "#3 (52-64,149-161)"
CountryRegion5G_4           = "#4 (149-165)"
CountryRegion5G_5           = "#5 (149-161)"
CountryRegion5G_6           = "#6 (36-48)"
CountryRegion5G_7           = "#7 (36-165)"
CountryRegion5G_8           = "#8 (52-64)"
CountryRegion5G_9           = "#9 (36-116,132-165)"
CountryRegion5G_10          = "#10 (36-48,149-165)"
CountryRegion5G_11          = "#11 (36-120,149-161)"
CountryRegion5G_12          = "#12 (36-140)"
CountryRegion5G_13          = "#13 (52-161)"
CountryRegion5G_14          = "#14 (36-116,136-165)"
CountryRegion5G_15          = "#15 (149-173)"
CountryRegion5G_16          = "#16 (36-173)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "多媒体/游戏环境"
AdhocNMode                  = "随意网络支持802.11n"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MERCURY Client"
WPS_DEVNAME_CUSTOMER1       = "MERCURY Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"

FAST_ROAMING_SENSITIVITY_STR = "漫游灵敏度" 
DISABLE_STR                 = "6.停用"
LOWEST_STR                  = "5.最低"
MEDIUM_LOW_STR              = "4.低"
MEDIUM_STR                  = "3.中"
MEDIUM_HIGH_STR             = "2.高"
HIGHEST_STR                 = "1.最高"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF			                = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"
